/*
 * drivedb.h - smartmontools drive database file
 *
 * Home page of code is: https://www.smartmontools.org
 *
 * Copyright (C) 2003-11 Philip Williams, Bruce Allen
 * Copyright (C) 2008-25 Christian Franke
 *
 * SPDX-License-Identifier: GPL-2.0-or-later
 */

/*
 * Structure used to store drive database entries:
 *
 * struct drive_settings {
 *   const char * modelfamily;
 *   const char * modelregexp;
 *   const char * firmwareregexp;
 *   const char * warningmsg;
 *   const char * presets;
 * };
 *
 * The elements are used in the following ways:
 *
 *  modelfamily     Informal string about the model family/series of a
 *                  device. Set to "" if no info (apart from device id)
 *                  known.  The entry is ignored if this string starts with
 *                  a dollar sign.  Must not start with "USB:", see below.
 *  modelregexp     POSIX extended regular expression to match the model of
 *                  a device.  This should never be "".
 *  firmwareregexp  POSIX extended regular expression to match a devices's
 *                  firmware.  This is optional and should be "" if it is not
 *                  to be used.  If it is nonempty then it will be used to
 *                  narrow the set of devices matched by modelregexp.
 *  warningmsg      A message that may be displayed for matching drives.  For
 *                  example, to inform the user that they may need to apply a
 *                  firmware patch.
 *  presets         String with vendor-specific attribute ('-v') and firmware
 *                  bug fix ('-F') options.  Same syntax as in smartctl command
 *                  line.  The user's own settings override these.
 *
 * The regular expressions for drive model and firmware must match the full
 * string.  The effect of "^FULLSTRING$" is identical to "FULLSTRING".
 * The form ".*SUBSTRING.*" can be used if substring match is desired.
 *
 * The table will be searched from the start to end or until the first match,
 * so the order in the table is important for distinct entries that could match
 * the same drive.
 *
 *
 * Format for USB ID entries:
 *
 *  modelfamily     String with format "USB: DEVICE; BRIDGE" where
 *                  DEVICE is the name of the device and BRIDGE is
 *                  the name of the USB bridge.  Both may be empty
 *                  if no info known.
 *  modelregexp     POSIX extended regular expression to match the USB
 *                  vendor:product ID in hex notation ("0x1234:0xabcd").
 *                  This should never be "".
 *  firmwareregexp  POSIX extended regular expression to match the USB
 *                  bcdDevice info.  Only compared during search if other
 *                  entries with same USB vendor:product ID exist.
 *  warningmsg      Not used yet.
 *  presets         String with one device type ('-d') option.
 *
 */

/*
const drive_settings builtin_knowndrives[] = {
 */
  { "VERSION: 7.5/5894 2025-09-23 15:50:03 +0000 594733115da2",
    "-", "-",
    "Version information",
    ""
  },
  { "DEFAULT",
    "-", "-",
    "Default settings",
    "-v 1,raw48,Raw_Read_Error_Rate "
    "-v 2,raw48,Throughput_Performance "
    "-v 3,raw16(avg16),Spin_Up_Time "
    "-v 4,raw48,Start_Stop_Count "
    "-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 6,raw48,Read_Channel_Margin,HDD "
    "-v 7,raw48,Seek_Error_Rate,HDD "
    "-v 8,raw48,Seek_Time_Performance,HDD "
    "-v 9,raw24(raw8),Power_On_Hours "
    "-v 10,raw48,Spin_Retry_Count,HDD "
    "-v 11,raw48,Calibration_Retry_Count,HDD "
    "-v 12,raw48,Power_Cycle_Count "
    "-v 13,raw48,Read_Soft_Error_Rate "
    //  14-21 Unknown_Attribute
    "-v 22,raw48,Helium_Level,HDD " // WDC (HGST)
    "-v 23,raw48,Helium_Condition_Lower,HDD " // ] Toshiba
    "-v 24,raw48,Helium_Condition_Upper,HDD " // ]
    //  25-174 Unknown_Attribute
    "-v 175,raw48,Program_Fail_Count_Chip,SSD "
    "-v 176,raw48,Erase_Fail_Count_Chip,SSD "
    "-v 177,raw48,Wear_Leveling_Count,SSD "
    "-v 178,raw48,Used_Rsvd_Blk_Cnt_Chip,SSD "
    "-v 179,raw48,Used_Rsvd_Blk_Cnt_Tot,SSD "
    "-v 180,raw48,Unused_Rsvd_Blk_Cnt_Tot,SSD "
    "-v 181,raw48,Program_Fail_Cnt_Total "
    "-v 182,raw48,Erase_Fail_Count_Total,SSD "
    "-v 183,raw48,Runtime_Bad_Block "
    "-v 184,raw48,End-to-End_Error "
    //  185-186 Unknown_Attribute
    "-v 187,raw48,Reported_Uncorrect "
    "-v 188,raw48,Command_Timeout "
    "-v 189,raw48,High_Fly_Writes,HDD "
    "-v 190,tempminmax,Airflow_Temperature_Cel "
    "-v 191,raw48,G-Sense_Error_Rate,HDD "
    "-v 192,raw48,Power-Off_Retract_Count "
    "-v 193,raw48,Load_Cycle_Count,HDD "
    "-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw48,Hardware_ECC_Recovered "
    "-v 196,raw16(raw16),Reallocated_Event_Count "
    "-v 197,raw48,Current_Pending_Sector "
    "-v 198,raw48,Offline_Uncorrectable "
    "-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 200,raw48,Multi_Zone_Error_Rate,HDD " // Seagate Helium HDDs: "Pressure_Limit"
    "-v 201,raw48,Soft_Read_Error_Rate,HDD "
    "-v 202,raw48,Data_Address_Mark_Errs,HDD "
    "-v 203,raw48,Run_Out_Cancel "
    "-v 204,raw48,Soft_ECC_Correction "
    "-v 205,raw48,Thermal_Asperity_Rate "
    "-v 206,raw48,Flying_Height,HDD "
    "-v 207,raw48,Spin_High_Current,HDD "
    "-v 208,raw48,Spin_Buzz,HDD "
    "-v 209,raw48,Offline_Seek_Performnce,HDD "
    //  210-219 Unknown_Attribute
    "-v 220,raw48,Disk_Shift,HDD "
    "-v 221,raw48,G-Sense_Error_Rate,HDD "
    "-v 222,raw48,Loaded_Hours,HDD "
    "-v 223,raw48,Load_Retry_Count,HDD "
    "-v 224,raw48,Load_Friction,HDD "
    "-v 225,raw48,Load_Cycle_Count,HDD "
    "-v 226,raw48,Load-in_Time,HDD "
    "-v 227,raw48,Torq-amp_Count,HDD "
    "-v 228,raw48,Power-off_Retract_Count "
    //  229 Unknown_Attribute
    "-v 230,raw48,Head_Amplitude,HDD "
    "-v 231,raw48,Temperature_Celsius,HDD "
    "-v 232,raw48,Available_Reservd_Space "
    "-v 233,raw48,Media_Wearout_Indicator,SSD "
    //  234-239 Unknown_Attribute
    "-v 240,raw24(raw8),Head_Flying_Hours,HDD "
    "-v 241,raw48,Total_LBAs_Written "
    "-v 242,raw48,Total_LBAs_Read "
    //  243-249 Unknown_Attribute
    "-v 250,raw48,Read_Error_Retry_Rate "
    //  251-253 Unknown_Attribute
    "-v 254,raw48,Free_Fall_Sensor,HDD"
  },
  { "Swissbit C440 Industrial CompactFlash Card",
    // spec v1.23 found at https://www.farnell.com/datasheets/1821167.pdf
    // tested with SFCF4096H2BU4TO-I-MS-527-STD
    "SFCF(2048|4096|8192|16GB|32GB|64GB)H[0-9]BU[24]TO-(C|I)-(MS|QT|NU)-5[0-9]7-STD",
    "", "",
    "-v 196,raw24/raw24,Spare_Blocks "
    "-v 213,raw24/raw24,Spare_Blocks_Worst_Chip "
    "-v 229,raw48,Erase_Count "
    "-v 203,raw48,Total_ECC_Errors "
    "-v 232,raw48,Total_Number_of_Reads "
    "-v 214,raw48,Reserved_Attribute " // Spec says "to be determined"
    "-v 215,raw48,Current_TRIM_Percent "
  },
  { "Swissbit X-600m Series Industrial mSATA SSD",
    // spec v1.06 found at https://www.mouser.com/pdfdocs/Swissbit_X-600m_Datasheet.pdf
    // tested with SFSA016GU1AA2TO-I-DB-216-STD
    "SFSA(008|016|032|064|128)GU[0-9]AA[124]TO-(C|I)-(DB|QC|NC)-2[0-9]6-STD",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 160,raw48,Uncorrectable_Error_Cnt "
    "-v 161,raw48,Spare_Blocks_Remaining "
    "-v 163,raw48,Initial_Bad_Block_Count "
    "-v 164,raw48,Total_Erase_Count "
    "-v 165,raw48,Max_Erase_Count "
    "-v 166,raw48,Min_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 168,raw48,Max_Erase_Count_of_Spec "
    "-v 169,raw48,Power_On_Uncorr_Err_Cnt "
    "-v 192,raw48,Init_Spare_Blocks_Avail "
    "-v 193,raw48,Dynamic_Remaps "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 198,raw48,Offline_Uncorrectable "
    "-v 199,raw48,SATA_CRC_Error_Count "
    "-v 215,raw48,TRIM_Count "
    "-v 235,hex56,Flash_Writes_LBAs_Low "
    "-v 237,hex48,Flash_Writes_LBAs_High "
    "-v 241,hex56,Total_LBAs_Written_Low "
    "-v 242,hex56,Total_LBAs_Read_Low "
    "-v 243,hex48,Total_LBAs_Written_High "
    "-v 244,hex48,Total_LBAs_Read_High "
    "-v 248,raw48,Perc_Rated_Life_Remain "
    "-v 249,raw48,Spares_Remaining_Perc "
  },
  { "Swissbit X-7x Family SATA SSD", // tested with
      // SFSA060GM2AK1TO-C-6B-536-STD/SBR11007, SFSA020GU2AK1TO-I-6B-22P-STD/SBR15004,
      // SFSA160GM2AK1TA-I-8C-11P-STD/SBR15103, SFSA320GM2AK2TA-I-8C-21P-STD/SBR15103
    "SFSA....[MQSUV].AK.T[ABO].............",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 16,raw48,Avg_Erase_Count_pSLC "
    "-v 17,raw48,Rated_Erase_Count_pSLC "
    "-v 160,raw48,UECC_Sector_Count "
    "-v 161,raw48,Spare_Block_Count "
    "-v 163,raw48,Initial_Bad_Block_Count "
    "-v 164,raw48,Total_Erase_Count "
    "-v 165,raw48,Maximum_Erase_Count "
    "-v 166,raw48,Minimum_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 168,raw48,Rated_Erase_Count "
    "-v 169,raw48,Power_On_UECC_Err_Cnt "
    "-v 193,raw48,Dynamic_Remaps "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 215,raw48,Number_of_TRIM_Commands  "
    "-v 231,raw48,Life_Remaining_Percent "
    "-v 235,raw48,Flash_LBAs_Written "
    "-v 237,raw48,Flash_LBAs_Written_Exp "
  //"-v 241,raw48,Total_LBAs_Written "
  //"-v 242,raw48,Total_LBAs_Read "
    "-v 243,raw48,Host_LBA_Write_Exp "
    "-v 244,raw48,Host_LBA_Read_Exp "
    "-v 248,raw48,SSD_Remaining_Life_Perc "
  },
  { "Swissbit X-8x Family SATA SSD", // tested with
    // SFSA080GM1AO1TO-C-8C-11P-STD/AOR20008, SFSA020GM1AO1TO-I-6B-11P-STD/AOR20008
    "SFSA....M.AO.TO.............",
    "", "",
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 165,raw48,Maximum_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 168,raw48,Rated_Erase_Count "
    "-v 169,raw48,Power_On_Data_Repairs "
  //"-v 184,raw48,End-to-End_Error "
    "-v 185,raw48,E2E_ErrCnt_SATA-Flash "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
    "-v 196,raw48,Total_Spare_Block_Cnt "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 200,raw48,SATA_COM_Reset "
    "-v 213,raw48,Spare_Block_Cnt_Worst "
    "-v 215,raw48,Trim_Status "
    "-v 229,raw48,Total_Flash_Blk_Erases "
    "-v 232,raw48,Total_Read_Cnt "
    "-v 241,raw48,Total_Host_LBA_Written "
    "-v 242,raw48,Total_Host_LBA_Read "
    "-v 248,raw48,Remaining_Life "
  },
  { "Apacer SDM4 Series SSD Module",
    "(2|4|8|16|32|64)GB SATA Flash Drive", // tested with APSDM002G15AN-CT/SFDDA01C and SFI2101D
    "SF(DDA01C|I2101D)",
    "",
    "-v 160,raw48,Initial_Bad_Block_Count "
    "-v 161,raw48,Bad_Block_Count "
    "-v 162,raw48,Spare_Block_Count "
    "-v 163,raw48,Max_Erase_Count "
    "-v 164,raw48,Average_Erase_Count "
    "-v 165,raw48,Average_Erase_Count " // could be wrong
  },
  { "Apacer SDM5/5A/5A-M Series SSD Module",
    "(1|2|4|8|16|32|64)GB SATA Flash Drive", // tested with APSDM016GA2AN-PTM1/SFDK004A,
      // APSDM016GA3AN-ATM/SFDE001A, APSDM004G13AN-AT/SFDE001A
    "SF(DK004A|DE001A)",
    "",
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 163,raw48,Max_Erase_Count "
    "-v 164,raw48,Average_Erase_Count "
    "-v 166,raw48,Grown_Bad_Block_Count "
    "-v 167,raw48,SSD_Write_Protect_Mode "
    "-v 168,raw48,SATA_PHY_Err_Ct "
    "-v 175,raw48,Bad_Cluster_Table_Count "
    "-v 192,raw48,Unexpect_Power_Loss_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 241,raw48,Total_LBAs_Written "
  },
  { "Apacer AS340/350 SSDs",
    "Apacer AS3[45]0 ((12[08]|240|256|480|512|960)G|1T)B", // tested with
      // Apacer AS340 120GB/AP612PE0, Apacer AS350 1TB/AP613PE0
    "", "",
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 163,raw48,Max_Erase_Count "
    "-v 164,raw48,Average_Erase_Count "
    "-v 166,raw48,Later_Bad_Block_Count "
    "-v 167,raw48,SSD_Protect_Mode "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 175,raw48,Bad_Cluster_Table_Count "
    "-v 192,raw48,Unexpect_Power_Loss_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 231,raw48,Lifetime_Left "
  //"-v 241,raw48,Total_LBAs_Written "
  },
  { "Apacer SSDs",
    "([1248]|1[056]|20|3[02]|40|60|64|80|12[08]|160|240|256|320|480|512|640|960|1024|1280|1920|2048|3840|4096)(GB|TB) SATA Flash Drive|"
    "1TB SATA SSD|" // tested with 1TB SATA SSD/AP613PE0 (AP1TPPSS25-R)
    "S[GHTV]250-(M2[48][02]|25) ([1248]|1[056]|20|3[02]|40|60|64|80|12[08]|160|240|256|320|480|512|640|960|1024|1280|1920|2048|3840|4096)(GB|TB) SSD",
      // tested with 120GB SATA Flash Drive/SFMB6130, SH250-M242 128GB SSD/SFMB8120, ST250-M280 256GB SSD/SFMD6110
    "AP613PE0|SFM[BCDEGHJ][0-9A-Z][0-9A-Z][1-9A-Z][0-9A-Z]",
    "",
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 163,raw48,Maximum_Erase_Count "
    "-v 164,raw48,Average_Erase_Count "
    "-v 166,raw48,Total_Later_Bad_Blk_Ct "
    "-v 167,raw48,SSD_Protect_Mode "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 175,raw48,Bad_Cluster_Table_Ct "
    "-v 192,raw48,Unexpect_Power_Loss_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 231,raw48,Lifetime_Left "
  //"-v 241,raw48,Total_LBAs_Written "
  },
  { "Apple MacBook Air SSD", // probably Toshiba
    "APPLE SSD TS(064|128)E", // tested with APPLE SSD TS064E/TQAABBF0
    "", "",
    "-v 173,raw48,Wear_Leveling_Count " //  ]
    "-v 241,raw48,Host_Writes_GiB "     //  ]  guessed (ticket #655)
    "-v 242,raw48,Host_Reades_GiB "     //  ]
  },
  { "Apple SD/SM/TS...E/F/G SSDs", // SanDisk/Samsung/Toshiba?
    "APPLE SSD (S[DM]|TS)0?(128|256|512|768|1024)[EFG]", // tested with APPLE SSD SD256E/1021AP, SD0128F/A223321
      // APPLE SSD SM768E/CXM90A1Q, SM0512F/UXM2JA1Q, TS0256F/109L0704, SM0512G/BXW1SA0Q, SM1024G/BXW1SA0Q
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 169,raw48,Unknown_Apple_Attrib "
    "-v 173,raw48,Wear_Leveling_Count " // ]
    "-v 174,raw48,Host_Reads_MiB "      // ] guessed (ticket #342), S[DM]*F only
    "-v 175,raw48,Host_Writes_MiB "     // ]
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
  //"-v 240,raw48,Unknown_SSD_Attribute "
  },
  { "ATP SATA III Value Line SSDs",
    "ATP SATA III (M.2 (2242|2280)|mSATA|mSATA SSD|2.5 inch)",
      // tested M.2 2280 with firmware version SBFMBB.3 (Value Line),
      // ATP SATA III M.2 2280/SBFMBB.3
    "SBFMB1.1|SBFMBB.3|SBFMT1.3",
    "",
    "-v 1,raw48,Raw_Read_Error_Count "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 170,raw16,Bad_Bl_Ct_LATER_0_EARLY " // Raw value: Byte [5~4] Later bad block count
                                            //            Byte [3~2] 0
                                            //            Byte [1~0] Early bad block count (meaning see ticket #1642)
    "-v 173,raw16,Erase_Count_0_AVG_MAX "   // Raw value: Byte [5~4] 0
                                            //            Byte [3~2] Average erase count
                                            //            Byte [1~0] Max erase count
    "-v 192,raw48,Unexpected_Power_Loss "
  //"-v 194,tempminmax,Device_Temperature "
    "-v 218,raw48,CRC_Errors "
    "-v 231,raw48,Percent_Lifetime_Remain "
    "-v 241,raw48,Host_Writes_GiB "
  },
  { "ATP SATA III Superior Line SSDs",
    "ATP (SATA III|SATAIII|I-Temp. SATA III|I-Temp. SATAIII) (M.2 (2242|2280)|mSATA|2.5 inch) SSD",
      // tested M.2 2242 & 2280 with firmware version T0205B (Superior Line with PLP),
      // ATP SATA III M.2 2280 SSD/T0205B
    "T0205B|U0316B",
    "",
    "-v 1,raw48,Raw_Read_Error_Count "
    "-v 5,raw16(raw16),Realloc_Flash_Blocks_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 14,raw48,Device_Raw_Capacity "
    "-v 15,raw48,Device_User_Capacity "
    "-v 16,raw48,Initial_Spare_Blocks "
    "-v 17,raw48,Remaining_Spare_Blocks "
    "-v 100,raw48,Total_Erease_Count "
    "-v 160,raw48,Uncorrectable_Sectors "
    "-v 172,raw48,Block_Erase_Failures "
    "-v 173,raw48,Maximum_Erase_Count "
    "-v 174,raw48,Unexpected_Power_Loss "
    "-v 175,raw48,Average_Erase_Count "
    "-v 181,raw48,Block_Program_Failures "
    "-v 187,raw48,Reported_Uncorr_Errors "
  //"-v 194,tempminmax,Device_Temperature "
  //"-v 195,raw48,Hardware_ECC_Recovered "
    "-v 197,raw48,Current_Pending_ECC_Cnt " // Like Crucial MX500: May flip 0 <> 1 (ticket #1227)
    "-v 198,raw48,Offline_UErr_Media_Scan "
    "-v 199,raw48,SATA_FIS_CRC_Errors "
    "-v 202,raw48,Percent_Lifetime_Used "
    "-v 205,raw48,Thermal_Asperity_Rate "
    "-v 231,tempminmax,Controller_Temperature "
    "-v 234,raw48,Sectors_Read_from_NAND "
    "-v 235,raw48,Sectors_Written_to_SSD "
    "-v 241,raw48,Sectors_Written_to_NAND "
    "-v 242,raw48,Sectors_Read_from_SSD "
    "-v 248,raw48,Percent_Lifetime_Remain "
    "-v 249,raw48,Spare_Blocks_Remaining " // same as ID 17 (Remaining_Spare_Blocks)
  },
  { "ATP SATA III aMLC M.2 2242/80 Embedded SSDs",
    "ATP I-Temp M\\.2 22(42|80)", // tested with ATP I-Temp M.2 2242/R0822A,
      // ATP I-Temp M.2 2280/R0822A
    "","",
    "-v 1,raw48,Raw_Read_Error_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 14,raw48,Device_Raw_Capacity "
    "-v 15,raw48,Device_User_Capacity "
    "-v 16,raw48,Initial_Spare_Blocks "
    "-v 17,raw48,Remaining_Spare_Blocks "
    "-v 100,raw48,Total_Erease_Count "
    "-v 160,raw48,Uncorrectable_Sectors "
    "-v 172,raw48,Block_Erase_Failure "
    "-v 173,raw48,Max_Erase_Count "
    "-v 174,raw48,Unexpected_Power_Cycle "
    "-v 175,raw48,Average_Erase_Count "
    "-v 181,raw48,Program_Fail_Blocks "
    "-v 187,raw48,Reported_UE_Counts "
    "-v 194,raw48,Device_Temperature "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 198,raw48,Offline_Uncorrectable "
    "-v 199,raw48,SATA_CRC_Error_Count "
    "-v 202,raw48,Percent_Lifetime_Used "
    "-v 205,raw48,Thermal_Asperity_Rate "
    "-v 231,raw48,Controller_Temperature "
    "-v 234,raw48,Nand_Sectors_Read "
    "-v 235,raw48,Device_Sectors_Written "
    "-v 241,raw48,Nand_Sectors_Written "
    "-v 242,raw48,Device_Bytes_Read "
    "-v 248,raw48,PCT_Life_Remaining "
    "-v 249,raw48,Spare_Block_Remaining "
  },
  { "Crucial/Micron RealSSD C300/P300", // Marvell 88SS9174
    "C300-CTFDDA[AC](064|128|256)MAG|" // tested with C300-CTFDDAC128MAG/0002,
      // C300-CTFDDAC064MAG/0006
    "(C300-)?MTFDBAK(064|128|256)MAG(-1G1)?|" // tested with
      // C300-MTFDBAK128MAG/0006 (attr 9 only), MTFDBAK256MAG-1G1/0007
    "P300-MTFDDAC(050|100|200)SAL", // tested with P300-MTFDDAC100SAL/0003
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Grown_Failing_Block_Ct "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Wear_Leveling_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 181,raw16,Non4k_Aligned_Access "
    "-v 183,raw48,SATA_Iface_Downshift "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 188,raw48,Command_Timeout "
    "-v 189,raw48,Factory_Bad_Block_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 202,raw48,Percent_Lifetime_Used "
    "-v 206,raw48,Write_Error_Rate "
  },
  { "Crucial/Micron RealSSD m4/C400/P400", // Marvell 9176, fixed firmware
    "C400-MTFDDA[ACK](064|128|256|512)MAM|"
      // M4-CT032M4SSD3/04MH
    "M4-CT(032|064|128|256|512)M4SSD[123]|" // tested with M4-CT512M4SSD2/0309
    "MTFDDA[AK](064|128|256|512|050|100|200|400)MA[MNR]-1[JKS]1.*", // tested with
      // MTFDDAK256MAR-1K1AA/MA52, MTFDDAK256MAM-1K12/08TH,
      // MTFDDAA064MAR-1J1AB  49Y5835 49Y5838IBM/MA49 (P400e)
    "030[9-Z]|03[1-Z].|0[4-Z]..|[1-Z]....*", // >= "0309"
    "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Grown_Failing_Block_Ct "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Wear_Leveling_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 181,raw16,Non4k_Aligned_Access "
    "-v 183,raw48,SATA_Iface_Downshift "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 188,raw48,Command_Timeout "
    "-v 189,raw48,Factory_Bad_Block_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 202,raw48,Perc_Rated_Life_Used "
    "-v 206,raw48,Write_Error_Rate "
    "-v 225,raw48,Unknown_Marvell_Attr " // P400e
    "-v 231,raw48,Unknown_Marvell_Attr " // P400e
    "-v 242,raw48,Host_Reads" // P400e: 2MiB?
  },
  { "Crucial/Micron RealSSD m4/C400", // Marvell 9176, buggy or unknown firmware
    "C400-MTFDDA[ACK](064|128|256|512)MAM|" // tested with C400-MTFDDAC256MAM/0002
    "M4-CT(032|064|128|256|512)M4SSD[123]", // tested with M4-CT064M4SSD2/0002,
      // M4-CT064M4SSD2/0009, M4-CT256M4SSD3/000F
    "",
    "This drive may hang after 5184 hours of power-on time:\n"
    "https://www.tomshardware.com/news/Crucial-m4-Firmware-BSOD,14544.html\n"
    "See the following web page for firmware updates:\n"
    "https://www.crucial.com/usa/en/support-ssd",
    "-v 170,raw48,Grown_Failing_Block_Ct "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Wear_Leveling_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 181,raw16,Non4k_Aligned_Access "
    "-v 183,raw48,SATA_Iface_Downshift "
    "-v 189,raw48,Factory_Bad_Block_Ct "
    "-v 202,raw48,Perc_Rated_Life_Used "
    "-v 206,raw48,Write_Error_Rate"
  },
  { "Crucial/Micron Client SSDs", // MX100, MX200, BX300, MX300, BX500, MX500, M500, M600, 1100, 1300
      // See also tnfd22_client_ssd_smart_attributes.pdf Rev. E from 2018-09-28
      // (covers M500 FW>=MU03, M510, M550, MX100, M600, MX200, 1100, MX300, 1300)
    "Crucial_CT(128|256|512)MX100SSD1|"// Marvell 88SS9189, tested with Crucial_CT256MX100SSD1/MU01
    "Crucial_CT(200|250|256|500|512|1000|1024)MX200SSD[1346]|" // Marvell 88SS9189, tested with
      // Crucial_CT500MX200SSD1/MU01, Crucial_CT1024MX200SSD1/MU01, Crucial_CT250MX200SSD3/MU01,
      // Crucial_CT250MX200SSD1/MU03
    "Crucial_CT(275|525|750|1050|2050)MX300SSD[14]|" // Marvell 88SS1074, tested with
      // Crucial_CT275MX300SSD1/M0CR040, Crucial_CT525MX300SSD1/M0CR021, Crucial_CT750MX300SSD1/M0CR011,
      // Crucial_CT2050MX300SSD1/M0CR031
    "Crucial_CT(120|240|480|960)M500SSD[134]|" // Marvell 88SS9187, tested with
      // Crucial_CT120M500SSD1/MU02, Crucial_CT120M500SSD3/MU02, Crucial_CT240M500SSD1/MU03,
      // Crucial_CT480M500SSD1/MU03, Crucial_CT960M500SSD1/MU03, Crucial_CT240M500SSD4/MU05
    "Crucial_CT(128|256|512|1024)M550SSD[134]|" // tested with Crucial_CT512M550SSD3/MU01,
      // Crucial_CT1024M550SSD1/MU01, Crucial_CT128M550SSD4/MU02
    "CT(120|240|480)BX300SSD1|" // Silicon Motion SM2258, same attributes as Marvell-based Crucial SSDs,
      // tested with CT240BX300SSD1/M2CR010
    "CT(120|240|480|960|[124]000)BX500SSD1|" // Silicon Motion SM2258XT, tested with CT120BX500SSD1/M6CR013,
      // CT1000BX500SSD1/M6CR030, CT2000BX500SSD1/M6CR030, CT4000BX500SSD1/M6CR082
    "CT(250|500|[124]000)MX500SSD[14][A-Z]?|" // Silicon Motion SM2258, tested with CT250MX500SSD1/M3CR010,
      // CT500MX500SSD1/M3CR010, CT1000MX500SSD1/M3CR010, CT2000MX500SSD1/M3CR010, CT500MX500SSD1/M3CR020,
      // CT250MX500SSD4/M3CR022, CT500MX500SSD1/M3CR022, CT500MX500SSD1/M3CR023, CT1000MX500SSD1/M3CR032,
      // CT4000MX500SSD1/M3CR044, CT500MX500SSD1N/M3CR023
    "Micron_M500_MTFDDA[KTV](120|240|480|960)MAV|"// tested with Micron_M500_MTFDDAK960MAV/MU05
    "Micron_M500DC_(EE|MT)FDDA[AK](120|240|480|800)MBB|" // tested with Micron_M500DC_EEFDDAA120MBB/129,
      // Micron_M500DC_MTFDDAK800MBB/0129
    "(Micron[_ ])?M500IT[_ ]MTFDDA[KTY](032|050|060|064|120|128|240|256)[MS]BD|" // tested with M500IT_MTFDDAK240MBD/MG02
    "(Micron_)?M510[_-]MTFDDA[KTV](128|256)MAZ|" // tested with M510-MTFDDAK256MAZ/MU01
    "MICRON_M510DC_(EE|MT)FDDAK(120|240|480|800|960)MBP|" // tested with Micron_M510DC_MTFDDAK240MBP/0005
    "(Micron_)?M550[_-]MTFDDA[KTV](064|128|256|512|1T0)MAY|" // tested with M550-MTFDDAK256MAY/MU01
    "(Micron_M600_)?(EE|MT)FDDA[KTV](128|256|512|1T0)MBF[25Z]?(-.*)?|" // tested with Micron_M600_MTFDDAK1T0MBF/MU01,
      // MTFDDAK256MBF-1AN1ZABHA/M603
    "(Micron_1100_)?MTFDDA[KV](256|512|1T0|2T0)TBN(-.*)?|" // Marvell 88SS1074, tested with
      // Micron_1100_MTFDDAK256TBN/M0MU020, MTFDDAK256TBN/M0MA020 (OEM), MTFDDAV256TBN-1AR15ABHA/HPC0T14
    "Micron 1100 SATA (256G|512G|1T|2T)B|" // tested with Micron 1100 SATA 256GB/M0DL022
    "(Micron_1300_)?(EE|MT)FDDA[KV](256|512|1T0|2T0)TDL(-.*)?", // tested with Micron_1300_MTFDDAK256TDL/M5MU000,
      // Micron_1300_MTFDDAK1T0TDL/M5MU000, MTFDDAK2T0TDL/M5MU030, MTFDDAK256TDL-1AW1ZABFA/M5MA030
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
    "-v 5,raw48,Reallocate_NAND_Blk_Cnt "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Reserved_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Ave_Block-Erase_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 180,raw48,Unused_Reserve_NAND_Blk "
    "-v 183,raw48,SATA_Interfac_Downshift "
    "-v 184,raw48,Error_Correction_Count "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw48,Cumulativ_Corrected_ECC "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
    "-v 197,raw48,Current_Pending_ECC_Cnt " // MX500: May flip 0 <> 1 (ticket #1227)
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 202,raw48,Percent_Lifetime_Remain " // norm = max(100-raw,0); raw = percent_lifetime_used
    "-v 206,raw48,Write_Error_Rate "
    "-v 210,raw48,Success_RAIN_Recov_Cnt "
    "-v 223,raw48,Unkn_CrucialMicron_Attr " // M6CR030
    "-v 246,raw48,Total_LBAs_Written "
    "-v 247,raw48,Host_Program_Page_Count "
    "-v 248,raw48,FTL_Program_Page_Count "
    "-v 249,raw48,Unkn_CrucialMicron_Attr " // M6CR030
  //"-v 250,raw48,Read_Error_Retry_Rate "   // M6CR030
    "-v 251,raw48,Unkn_CrucialMicron_Attr " // M6CR030
    "-v 252,raw48,Unkn_CrucialMicron_Attr " // M6CR030
    "-v 253,raw48,Unkn_CrucialMicron_Attr " // M6CR030
    "-v 254,raw48,Unkn_CrucialMicron_Attr"  // M6CR030
  },
  { "Lexar 128GB SSD", // for other Lexar drives see ticket #1529
    "Lexar 128GB SSD", // Lexar 128GB SSD/H190117D
    "", "",
    "-v 5,raw48,New_Bad_Blk_Cnt "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 167,raw48,SSD_Protect_mode "
    "-v 168,raw48,SATA_PHY_Error_Cnt "
    "-v 169,raw48,Bad_Block_Cnt "
    "-v 171,raw48,Program_Fail_Cnt "
    "-v 172,raw48,Erase_Fail_Cnt "
    "-v 173,raw48,Erase_Cnt "
    "-v 175,raw48,Bad_Cluster_Cnt "
    "-v 177,raw48,Read_Retry_Cnt "
    "-v 180,raw48,Spare_Blk_Cnt_Left "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 206,raw48,Min_Erase_Cnt "
    "-v 207,raw48,Max_Erase_Cnt "
    "-v 208,raw48,Avg_Erase_Cnt "
    "-v 209,raw48,SLC_Min_Erase_Cnt "
    "-v 210,raw48,SLC_Max_Erase_Cnt "
    "-v 211,raw48,SLC_Avg_Erase_Cnt "
    "-v 231,raw48,SSD_Life_Left "
  //"-v 241,raw48,Total_LBAs_Written "
  //"-v 242,raw48,Total_LBAs_Read "
    "-v 245,raw48,Bit_Error_Cnt "
  },
  { "Micron 5100 / 52x0 / 5300 / 5400 SSDs",
    "(Micron_5100_)?(EE|MT)FDDA[KV](240|480|960|1T9|3T8|7T6)T(BY|CB|CC)(_SED)?|" // Matches both stock and Dell OEM
      // tested with Micron_5100_MTFDDAK3T8TCB/D0MU410, MTFDDAK3T8TCB/D0MU410,
      // Micron_5100_MTFDDAK3T8TBY_SED/D0MU445
    "(Micron_5200_)?MTFDDAK(240|480|960|1T9|3T8|7T6)TD(C|D|N)|" // tested with Micron_5200_MTFDDAK240TDN/D1MU005,
      // Micron_5200_MTFDDAK3T8TDD/D1MU505
    "Micron_5210_MTFDDAK(480|960|1T9|3T8|7T6)QDE|" // tested with Micron_5210_MTFDDAK7T6QDE/D2MU804
    "(Micron_5300(HC)?_)?MTFDDA[KV](240|480|960|1T9|3T8|7T6)TD[STU](_.*)?|" // tested with
      // Micron_5300_MTFDDAK1T9TDS/D3MU001, Micron_5300HC_MTFDDAK960TDS/D3MN010, MTFDDAK1T9TDT/D3MU001,
      // Micron_5300_MTFDDAV960TDS_CISCO/D3MU001
    "(Micron_5400_)?(EE|MT)FDDA[KV](240|480|960|1T9|3T8|7T6)TG[ABC](_SED)?|" // tested with
      // Micron_5400_MTFDDAK1T9TGB/D4MU001, Micron_5400_MTFDDAK960TGA_SED/D4CS001
    "VK001920G(WSXK|XAWN)", // HPE OEM, tested with VK001920GWSXK/HPG3 (5200?), VK001920GXAWN/HPG1 (5300?)
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "  // raw24(raw8)??
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Reserved_Block_Pct " // Percentage of remaining reserved blocks available
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Avg_Block-Erase_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
  //"-v 180,raw48,Unused_Rsvd_Blk_Cnt_Tot " // absolute count of remaining reserved blocks available
    "-v 183,raw48,SATA_Int_Downshift_Ct " // SATA speed downshift count
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect " // Number of UECC correction failures
  //"-v 188,raw48,Command_Timeout "
  //"-v 194,tempminmax,Temperature_Celsius " // 100 - degrees C, wraps: 101 reported as 255
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector " // Use the raw value
  //"-v 198,raw48,Offline_Uncorrectable "  // Use the raw value
  //"-v 199,raw48,UDMA_CRC_Error_Count "   // Use the raw value
    "-v 202,raw48,Percent_Lifetime_Remain " // Remaining endurance, trips at 10%
    "-v 206,raw48,Write_Error_Rate "
    "-v 210,raw48,RAIN_Success_Recovered "  // Total number of NAND pages recovered by RAIN
    "-v 211,raw48,Integ_Scan_Complete_Cnt "  // Number of periodic data integrity scans completed
    "-v 212,raw48,Integ_Scan_Folding_Cnt "   // Number of blocks reallocated by integrity scans
    "-v 213,raw48,Integ_Scan_Progress "      // Current is percentage, raw is absolute number of superblocks scanned by the current integrity scan
    "-v 246,raw48,Total_LBAs_Written "
    "-v 247,raw48,Host_Program_Page_Count "
    "-v 248,raw48,Bckgnd_Program_Page_Cnt"
  },
  { "Micron M500DC/M510DC Enterprise SSDs",
    "Micron_M500DC_(EE|MT)FDDA[AK](120|240|480|800)MBB|" // tested with
      // Micron_M500DC_EEFDDAA120MBB/129, Micron_M500DC_MTFDDAK800MBB/0129
    "MICRON_M510DC_(EE|MT)FDDAK(120|240|480|800|960)MBP", // tested with
      // Micron_M510DC_MTFDDAK240MBP/0005
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
    "-v 5,raw48,Reallocated_Block_Count "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Reserved_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Ave_Block-Erase_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 184,raw48,Error_Correction_Count "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 188,raw48,Command_Timeouts "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw48,Cumulativ_Corrected_ECC "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 202,raw48,Percent_Lifetime_Remain "
    "-v 206,raw48,Write_Error_Rate "
    "-v 247,raw48,Host_Program_Page_Count "
    "-v 248,raw48,Bckgnd_Program_Page_Cnt"
  },
  { "SandForce Driven SSDs", // Corsair Force LS with buggy firmware only
    "Corsair Force LS SSD", // tested with Corsair Force LS SSD/S9FM01.8
    "S9FM01\\.8",
    "A firmware update is available for this drive.\n"
    "It is HIGHLY RECOMMENDED for drives with specific serial numbers.\n"
    "See the following web page for details:\n"
    "https://www.smartmontools.org/ticket/628",
    "-v 1,raw24/raw32,Raw_Read_Error_Rate "
    "-v 5,raw48,Retired_Block_Count "
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 162,raw48,Unknown_SandForce_Attr "
    "-v 170,raw48,Reserve_Block_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Unknown_SandForce_Attr "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 181,raw48,Program_Fail_Count "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
    "-v 218,raw48,Unknown_SandForce_Attr "
    "-v 231,raw48,SSD_Life_Left "
    "-v 241,raw48,Lifetime_Writes_GiB "
    "-v 242,raw48,Lifetime_Reads_GiB"
  },
  { "SandForce Driven SSDs",
    "SanDisk SDSSDA(120|240|480)G|" // SanDisk SSD Plus, tested with SanDisk SDSSDA240G/U21010RL
    "SanDisk SD8S[BFN]AT128G1(00|12)2", // SanDisk Z400s, tested with
      // SanDisk SD8SFAT128G1122/Z2333000, SanDisk SD8SNAT128G1002/Z2317002
      // SanDisk SD8SBAT128G1002/Z2317002
    "", "",
    "-v 5,raw48,Retired_Block_Count "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 166,raw48,Min_PE_Cycles "
    "-v 167,raw48,Max_Bad_Blocks_Per_Die "
    "-v 168,raw48,Max_PE_Cycles "
    "-v 169,raw48,Total_Bad_Blocks "
    "-v 170,raw48,Grown_Bad_Blocks "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Average_PE_Cycles "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 230,raw48,Media_Wearout_Indicator "
  //"-v 232,raw48,Available_Reservd_Space "
    "-v 233,raw48,NAND_GiB_Written "
    "-v 241,raw48,Lifetime_Writes_GiB "
    "-v 242,raw48,Lifetime_Reads_GiB"
  },
  { "SandForce Driven SSDs",
    "SandForce 1st Ed\\.|" // Demo Drive, tested with firmware 320A13F0
    "ADATA SSD S(396|510|599) .?..GB|" // tested with ADATA SSD S510 60GB/320ABBF0,
      // ADATA SSD S599 256GB/3.1.0, 64GB/3.4.6
    "ADATA SP[389]00|" // tested with ADATA SP300/5.0.2d, SP800/5.0.6c,
      // ADATA SP900/5.0.6 (Premier Pro, SF-2281)
    "ADATA SSD S[PX]900 (64|128|256|512)GB-DL2|" // tested with ADATA SSD SP900 256GB-DL2/5.0.6,
      // ADATA SSD SX900 512GB-DL2/5.8.2
    "ADATA XM11 (128|256)GB|" // tested with ADATA XM11 128GB/5.0.1
    "ATP Velocity MIV (60|120|240|480)GB|" // tested with ATP Velocity MIV 480GB/110719
    "Comay BladeDrive E28 (800|1600|3200)GB|" // LSI SF-2581, tested with Comay BladeDrive E28 800GB/2.71
    "Corsair CSSD-F(40|60|80|115|120|160|240)GBP?2.*|" // Corsair Force, tested with
      // Corsair CSSD-F40GB2/1.1, Corsair CSSD-F115GB2-A/2.1a
    "Corsair Voyager GTX|" // Corsair Voyager GTX/S9FM02J6
    "Corsair Force ((3 |LS )?SSD|GS|GT)|" // SF-2281, tested with
      // Corsair Force SSD/5.05, 3 SSD/1.3.2, GT/1.3.3, GS/5.03,
      // Corsair Force LS SSD/S8FM06.5, S9FM01.8, S9FM02.0
    "FM-25S2S-(60|120|240)GBP2|" // G.SKILL Phoenix Pro, SF-1200, tested with
      // FM-25S2S-240GBP2/4.2
    "FTM(06|12|24|48)CT25H|" // Supertalent TeraDrive CT, tested with
      // FTM24CT25H/STTMP2P1
    "KINGSTON RBU-SC400S37(64|128|256)G|" // tested with KINGSTON RBU-SC400S37256G/KD1ABBF0
    "KINGSTON SE50S37?(100|240|480)G|" // tested with KINGSTON SE50S3100G/KE1ABBF0,
      // KINGSTON SE50S37100G/61AABBF0 (E50)
    "KINGSTON SH10[03]S3(90|120|240|480)G|" // HyperX (3K), SF-2281, tested with
      // SH100S3240G/320ABBF0, SH103S3120G/505ABBF0
    "KINGSTON SKC(300S37A|380S3)(60|120|180|240|480)G|" // KC300, SF-2281, tested with
      // SKC300S37A120G/KC4ABBF0, SKC380S3120G/507ABBF0
    "KINGSTON SVP200S3(7A)?(60|90|120|240|480)G|" // V+ 200, SF-2281, tested with
      // SVP200S37A480G/502ABBF0, SVP200S390G/332ABBF0
    "KINGSTON SMS200S3(30|60|120)G|" // mSATA, SF-2241, tested with SMS200S3120G/KC3ABBF0
    "KINGSTON SMS450S3(32|64|128)G|" // mSATA, SF-2281, tested with SMS450S3128G/503ABBF0
    "KINGSTON (SV300|SKC100|SE100)S3.*G|" // other SF-2281
    "KINGSTON SHFS37A(120|240|480)G|" // HyperX Fury, SF-2281, tested with KINGSTON SHFS37A240G/608ABBF0
    "KINGSTON SNS4151S316GD|" // KINGSTON SNS4151S316GD/S9FM01.6
    "MKNSSDCR(45|60|90|120|180|240|360|480)GB(-(7|DX7?|MX|G2))?|" // Mushkin Chronos (7mm/Deluxe/MX/G2),
      // SF-2281, tested with MKNSSDCR120GB, MKNSSDCR120GB-MX/560ABBF0, MKNSSDCR480GB-DX7/603ABBF0
    "MKNSSDEC(60|120|240|480|512)GB|" // Mushkin Enhanced ECO2, tested with MKNSSDEC120GB/604ABBF0
    "MKNSSDAT(30|40|60|120|180|240|480)GB(-(DX|V))?|" // Mushkin Atlas (Deluxe/Value), mSATA, SF-2281,
      // tested with MKNSSDAT120GB-V/540ABBF0
    "Mushkin MKNSSDCL(40|60|80|90|115|120|180|240|480)GB-DX2?|" // Mushkin Callisto deluxe,
      // SF-1200/1222, Mushkin MKNSSDCL60GB-DX/361A13F0
    "MXSSD3MDSF-(60|120)G|" // MX-DS FUSION, tested with MXSSD3MDSF-60G/2.32
    "OCZ[ -](AGILITY2([ -]EX)?|COLOSSUS2|ONYX2|VERTEX(2|-LE))( [123]\\..*)?|" // SF-1200,
      // tested with OCZ-VERTEX2/1.11, OCZ-VERTEX2 3.5/1.11
    "OCZ-NOCTI|" // mSATA, SF-2100, tested with OCZ-NOCTI/2.15
    "OCZ-REVODRIVE3?( X2)?|" // PCIe, SF-1200/2281, tested with
      // OCZ-REVODRIVE( X2)?/1.20, OCZ-REVODRIVE3 X2/2.11
    "OCZ-REVODRIVE350|"
    "OCZ[ -](VELO|VERTEX2[ -](EX|PRO))( [123]\\..*)?|" // SF-1500, tested with
      // OCZ VERTEX2-PRO/1.10 (Bogus thresholds for attribute 232 and 235)
    "D2[CR]STK251...-....(\\.C)?|" // OCZ Deneva 2 C/R, SF-22xx/25xx,
      // tested with D2CSTK251M11-0240/2.08, D2CSTK251A10-0240/2.15, D2RSTK251M11-0100.C/3.22
    "OCZ-(AGILITY3|SOLID3|VERTEX3(\\.20| LT| MI)?)|" // SF-2200, tested with OCZ-VERTEX3/2.02,
      // OCZ-AGILITY3/2.11, OCZ-SOLID3/2.15, OCZ-VERTEX3 MI/2.15, OCZ-VERTEX3 LT/2.22, OCZ-VERTEX3.20/2.60
    "OCZ Z-DRIVE R4 [CR]M8[48]|" // PCIe, SF-2282/2582, tested with OCZ Z-DRIVE R4 CM84/2.13
      // (Bogus attributes under Linux)
    "OCZ Z-DRIVE 4500|"
    "OCZ-VELO DRIVE|" // VeloDrive R, PCIe, tested with OCZ-VELO DRIVE/1.33
    "TALOS2|" // OCZ Talos 2 C/R, SAS (works with -d sat), 2*SF-2282, tested with TALOS2/3.20E
    "(APOC|DENC|DENEVA|FTNC|GFGC|MANG|MMOC|NIMC|TMSC).*|" // other OCZ SF-1200,
      // tested with DENCSTE251M11-0120/1.33, DENEVA PCI-E/1.33
    "(DENR|DRSAK|EC188|NIMR|PSIR|TRSAK).*|" // other OCZ SF-1500
    "OWC Aura Pro( 6G SSD)?|" // tested with OWC Aura Pro 6G SSD/507ABBF0, OWC Aura Pro/603ABBF0
    "OWC Mercury Electra (Pro )?[36]G SSD|" // tested with
      // OWC Mercury Electra 6G SSD/502ABBF0, OWC Mercury Electra Pro 3G SSD/541ABBF0
    "OWC Mercury E(xtreme|XTREME) Pro (6G |RE )?SSD|" // tested with
      // OWC Mercury Extreme Pro SSD/360A13F0, OWC Mercury EXTREME Pro 6G SSD/507ABBF0
    "Patriot Pyro|" // tested with Patriot Pyro/332ABBF0
    "SanDisk SDSSDX(60|120|240|480)GG25|" // SanDisk Extreme, SF-2281, tested with
      // SDSSDX240GG25/R201
    "SuperSSpeed S301 [0-9]*GB|" // SF-2281, tested with SuperSSpeed S301 128GB/503
    "SG9XCS2D(0?50|100|200|400)GESLT|" // Smart Storage Systems XceedIOPS2, tested with
      // SG9XCS2D200GESLT/SA03L370
    "SSD9SC(120|240|480)GED[EA]|" // PNY Prevail Elite, tested with SSD9SC120GEDA/334ABBF0
    "(TX32|TX31C1|VN0.?..GCNMK).*|" // Smart Storage Systems XceedSTOR
    "(TX22D1|TX21B1).*|" // Smart Storage Systems XceedIOPS2
    "TX52D1.*|" // Smart Storage Systems Xcel-200
    "TS(64|128|256|512)GSSD[37]20|" // Transcend SSD320/720, SF-2281, tested with
      // TS128GSSD320, TS256GSSD720/5.2.0
    "UGB(88P|99S)GC...H[BF].|" // Unigen, tested with
      // UGB88PGC100HF2/MP Rev2, UGB99SGC100HB3/RC Rev3
    "SG9XCS(1F|2D)(50|100|200|400)GE01|" // XceedIOPS, tested with SG9XCS2D50GE01/SA03F34V
    "VisionTek GoDrive (60|120|240|480)GB", // tested with VisionTek GoDrive 480GB/506ABBF0
    "", "",
    "-v 1,raw24/raw32,Raw_Read_Error_Rate "
    "-v 5,raw48,Retired_Block_Count "
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 13,raw24/raw32,Soft_Read_Error_Rate "
    "-v 100,raw48,Gigabytes_Erased "
    "-v 162,raw48,Unknown_SandForce_Attr " // Corsair Force LS SSD/S9FM01.8, *2.0
    "-v 170,raw48,Reserve_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Unknown_SandForce_Attr " // Corsair Force LS SSD/S9FM01.8, *2.0
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 177,raw48,Wear_Range_Delta "
    "-v 181,raw48,Program_Fail_Count "
    "-v 182,raw48,Erase_Fail_Count "
    "-v 184,raw48,IO_Error_Detect_Code_Ct "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 189,tempminmax,Airflow_Temperature_Cel "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw24/raw32,ECC_Uncorr_Error_Count "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
    "-v 198,raw24/raw32:210zr54,Uncorrectable_Sector_Ct " // KINGSTON SE100S3100G/510ABBF0
    "-v 199,raw48,SATA_CRC_Error_Count "
    "-v 201,raw24/raw32,Unc_Soft_Read_Err_Rate "
    "-v 204,raw24/raw32,Soft_ECC_Correct_Rate "
    "-v 218,raw48,Unknown_SandForce_Attr " // Corsair Force LS SSD/S9FM01.8, *2.0
    "-v 230,raw48,Life_Curve_Status "
    "-v 231,raw48,SSD_Life_Left "
  //"-v 232,raw48,Available_Reservd_Space "
    "-v 233,raw48,SandForce_Internal "
    "-v 234,raw48,SandForce_Internal "
    "-v 235,raw48,SuperCap_Health "
    "-v 241,raw48,Lifetime_Writes_GiB "
    "-v 242,raw48,Lifetime_Reads_GiB"
  },
  { "StorFly CFast SATA 6Gbps SSDs",
    // https://datasheet.octopart.com/VSFCS2CC060G-100-Virtium-datasheet-82287733.pdf
    // tested with StorFly VSFCS2CC060G-100/0409-000
    "StorFly VSFCS2C[CI](016|030|060|120|240)G-...",
    // C - commercial, I industrial
    "", "",
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 160,raw48,Uncorrectable_Error_Cnt "
    // 0729 - remaining in block life. In 0828  remaining is normalized to 100% then decreases
    "-v 161,raw48,Spares_Remaining "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 169,raw48,Lifetime_Remaining% "
    "-v 248,raw48,Lifetime_Remaining% " //  later then 0409 FW.
    "-v 249,raw48,Spares_Remaining_Perc " //  later then 0409 FW.
  },
  { "Phison Driven SSDs", // see MKP_521_Phison_SMART_attribute.pdf
    "BP4 mSATA SSD|" // MyDigital BP4, tested with BP4 mSATA SSD/S8FM06.9
    "Corsair Force LE(200)? SSD|" // tested with Corsair Force LE SSD/SAFC11.0,
      // Corsair Force LE200 SSD/SBFM10, .../SBFM60.9
    "DGSR2(128|256|512)GP13T|"  // tested with DGSR2512GP13T/SBFM61.5
    "GIGABYTE GP-GSTFS31((120|240|256|480)G|100T)NTD|" // tested with GIGABYTE GP-GSTFS31120GNTD/SBFM61.3
    "GOODRAM IRIDIUM PRO|" // tested with GOODRAM IRIDIUM PRO/SAFM01.5
    "IRP?-SSDPR-S25[AC]-(120|240|256|480|512|960|0[12]T)|" // Goodram IRIDM (PRO), tested with
      // IR-SSDPR-S25A-120/SBFM91.3, IR-SSDPR-S25A-240/SBFM91.2, IRP-SSDPR-S25C-512/SCFM13.3,
      // IRP-SSDPR-S25C-02T/SCFM13.2
    "KINGSTON O(C|M[48S])P0S3(64|128|256|512)B-[0A]0|" // tested with KINGSTON OCP0S364B-A0/SBFK62A3,
      // KINGSTON OM4P0S3256B-A0/SBFK62A3, KINGSTON OM8P0S364B-A0/SBFK62A3,
      // KINGSTON OMSP0S3128B-00/SBFK62A3
    "KINGSTON RBUSNS(4|8)180S3(32|64|128|256|512)GJ|" // RBU-SNSx180S3, tested with
      // KINGSTON RBUSNS4180S3256GJ/SBFK61D1, KINGSTON RBUSNS8180S3512GJ/SBFK61D1
    "KINGSTON SEDC400S37(400|480|800|960|1600|1800)G|" // DC400, tested with
      // KINGSTON SEDC400S37480G/SAFM02.[GH], KINGSTON SEDC400S37960G/SAFM32.I
    "KINGSTON SEDC(450R|500[MR]|600ME?)(480|960|1920|3840|7680)G|" // DC450R, DC500M/R, DC600M, tested with
      // KINGSTON SEDC450R480G/SCEKH3. KINGSTON SEDC500M1920G/SCEKJ2.3,
      // KINGSTON SEDC500R480G/SCEKJ2.3, KINGSTON SEDC450R7680G/SCEKH3.4,
      // KINGSTON SEDC600M7680G/SCEKH5.1, KINGSTON SEDC600ME960G/SCEKH5L5
    "KINGSTON SM2280S3G2(120|240|480)G|" // KINGSTON SM2280S3G2120G/SAFM01.R,
      // KINGSTON SM2280S3G2240G/SAFM01.W
    "KINGSTON SUV300S37A(120|240|480)G|" // UV300 SSD, tested with KINGSTON SUV300S37A120G/SAFM11.K
    "KINGSTON SKC310S3B?7A960G|" // SSDNow KC310, KINGSTON SKC310S37A960G/SAFM00.r
    "KINGSTON SKC400S37(128G|256G|512G|1T)|" // SSDNow KC400, KINGSTON SKC400S37128G
    "KINGSTON SV310S3(7A|D7|N7A|B7A)960G|" // SSDNow V310
    "KINGSTON SHSS3B?7A(120|240|480|960)G|" // HyperX Savage
    "KINGSTON SS200S330G|" // SSDNow S200, tested with KINGSTON SS200S330G/S8FM06.A
    "KINGSTON  ?SA400(M8|S37)(120|240|480|960)G|" // Kingston A400 SSD, Phison S11 or
      // Silicon Motion controller (see ticket #801), tested with
      // KINGSTON SA400S37240G/SBFK10D7, KINGSTON SA400S37120G/SBFK71E0, */SBFKB1D1
      // KINGSTON  SA400S37480G/SBFK10D7 (two spaces), KINGSTON SA400M8240G/SBFK61E1
    "KIOXIA-EXCERIA SATA SSD|" // KIOXIA-EXCERIA SATA SSD/SBFA18.1 (480GB)
    "Patriot (Blast|Blaze|Flare|Ignite)|" // tested with Patriot Blast/SAFM11.3,
      // Patriot Blaze/S9FM02, Patriot Flare/SBFM91.2, Patriot Ignite/SAFM01.7
    "Patriot Burst( (120|240|480|960)GB)?|" // tested with Patriot Burst/SBFM11.2,
      // Patriot Burst 480GB/SBFMLA.5
    "PNY CS(900|1311|2211) ((12|24|48|50|96)0G|[12]T)B SSD|" // tested with PNY CS900 120GB SSD/CS900612,
      // PNY CS900 240GB SSD/CS900613, PNY CS900 500GB SSD/CS900LA5, PNY CS900 500GB SSD/CS900Y13,
      // PNY CS900 1TB SSD/CS900615, PNY CS1311 120GB SSD/CS131122, PNY CS2211 240GB SSD/CS221016
    "PNY ELITE PSSD|" // tested with PNY ELITE PSSD/CS105P13 (240G)
    "S11-(128|256|512)G-PHISON-SSD-B27|" // tested with: S11-512G-PHISON-SSD-B27/SBFMJ1.3
    "SSD Smartbuy (60|64|120|128|240|256|480|512|960|1024|2000)GB|" // PS3111-S11, tested with
      // SSD Smartbuy 240GB/SBFM91.1, SSD Smartbuy 64GB/SBFM21.1
    "SSD PHISON (128|256)GB PS3110-S10C|" // tested with SSD PHISON 128GB PS3110-S10C/SAFM12.2,
      // SSD PHISON 256GB PS3110-S10C/SAFM12.2
    "SSDPR-CX400-(128|256|512|1024)|" // Goodram CX400, tested with SSDPR-CX400-512/SBFM61.3
    "TEAM L3 EVO SSD (120|240|480|960)GB|" // TEAM L3 EVO SSD 120GB/SBFM11.0
    "SSM28(128|256|512)GPTCB3B-S11[24]61[123]|" // tested with SSM28256GPTCB3B-S112612/SBFM61.2
    "SVM2S46(128|256|512)GNPI51UF", // tested with SVM2S46128GNPI51UF/SBFMH1.2
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
    "-v 2,raw48,Not_In_Use "
    "-v 3,raw48,Not_In_Use "
    "-v 5,raw48,Retired_Block_Count "
    "-v 7,raw48,Not_In_Use "
    "-v 8,raw48,Not_In_Use "
  //"-v 9,raw24(raw8),Power_On_Hours "
    "-v 10,raw48,Not_In_Use "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 167,raw48,Write_Protect_Mode " // DC500
    "-v 168,raw48,SATA_Phy_Error_Count "
    "-v 169,raw48,Bad_Block_Rate " // DC500
    "-v 170,raw24/raw24:z54z10,Bad_Blk_Ct_Lat/Erl " // Later bad block/Early bad block (see #1642)
    "-v 172,raw48,Erase_Fail_Count " // DC500
    "-v 173,raw16(avg16),MaxAvgErase_Ct "
    "-v 175,raw48,Not_In_Use "
    "-v 181,raw48,Program_Fail_Count " // DC500
    "-v 182,raw48,Erase_Fail_Count " // DC500
    "-v 183,raw48,Unknown_Phison_Attr "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 193,raw48,Power_Fail_Uncompl_Cnt "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw48,Power_Fail_Health "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
    "-v 197,raw48,Not_In_Use "
    "-v 199,raw48,SATA_CRC_Error_Count "
    "-v 207,raw48,Thermal_Throttling_Cnt "
    "-v 218,raw48,CRC_Error_Count "
    "-v 231,raw48,SSD_Life_Left "
    "-v 232,raw48,Read_Fail_Count "
    "-v 233,raw48,Flash_Writes_GiB "
    "-v 240,raw48,Not_In_Use "
    "-v 241,raw48,Lifetime_Writes_GiB " // KIOXIA-EXCERIA SATA SSD/SBFA18.1: 32MiB ?
    "-v 242,raw48,Lifetime_Reads_GiB "
    "-v 244,raw48,Average_Erase_Count "
    "-v 245,raw48,Max_Erase_Count "
    "-v 246,raw48,Total_Erase_Count "
  },
  // this is a copy of the Phison bases record for the OEM drives with a very
  // weak information in the model. Detection is based on Firmware.
  { "Phison Driven OEM SSDs", // see MKP_521_Phison_SMART_attribute.pdf
    "Gigastone SSD|" // tested with GSTB512G (Gigastone SSD/SHFM20.2)
    "GOODRAM|" // tested with GOODRAM CX200 (GOODRAM/SAFM12.2)
    "Hoodisk SSD|" // tested with Hoodisk SSD/SBFM01.3, Hoodisk SSD/SBFMJ1.3
    "INTENSO|" // tested with Intenso SSD SATA III Top (INTENSO/S9FM02.6, .../SAFM01.6)
    "INTENSO SATA III SSD|" // tested with INTENSO SATA III SSD/SBFM11.2, .../SBFM81.3
    "Kingmax SATA SSD (120|240|480|960)GB|" // tested with Kingmax SATA SSD 240GB/SBFMY1.3
    "SATA SSD|" // tested with Supermicro SSD-DM032-PHI (SATA SSD/S9FM02.1),
      // PC Engines msata16d (SATA SSD/S9FM02.3), FoxLine flssd240x4s(SATA SSD/SBFM10.5)
    "SPCC Solid State Disk|" // Silicon Power, tested with SPCC Solid State Disk/SBFD00.3,
      // SPCC Solid State Disk/SBFM61.2, SPCC Solid State Disk/SBFMT1.3
    "SSDPR-CX400-(128|256|512|1024|2028)-G2", // Goodram CX400 G2, tested with
      // SSDPR-CX400-512-G2/SBFMLA.5 (SSDPR-CX400-128-G2/SN07373 differs, see ticket #1689)
    "S[89ABH]F[DM][0-9JLTY][0-9A]\\.[0-9]",
    "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
    "-v 2,raw48,Not_In_Use "
    "-v 3,raw48,Not_In_Use "
    "-v 5,raw48,Retired_Block_Count "
    "-v 7,raw48,Not_In_Use "
    "-v 8,raw48,Not_In_Use "
  //"-v 9,raw24(raw8),Power_On_Hours "
    "-v 10,raw48,Not_In_Use "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 168,raw48,SATA_Phy_Error_Count "
    "-v 170,raw24/raw24:z54z10,Bad_Blk_Ct_Lat/Erl " // Later bad block/Early bad block (see #1642)
    "-v 173,raw16(avg16),MaxAvgErase_Ct "
    "-v 175,raw48,Not_In_Use "
    "-v 183,raw48,Unknown_Attribute "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 192,raw48,Unsafe_Shutdown_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 196,raw48,Not_In_Use "
    "-v 197,raw48,Not_In_Use "
    "-v 199,raw48,CRC_Error_Count "
    "-v 218,raw48,CRC_Error_Count "
    "-v 231,raw48,SSD_Life_Left "
    "-v 233,raw48,Flash_Writes_GiB "
    "-v 240,raw48,Not_In_Use "
    "-v 241,raw48,Lifetime_Writes_GiB "
    "-v 242,raw48,Lifetime_Reads_GiB "
    "-v 244,raw48,Average_Erase_Count "
    "-v 245,raw48,Max_Erase_Count "
    "-v 246,raw48,Total_Erase_Count "
  },
  { "Indilinx Barefoot based SSDs",
    "Corsair CSSD-V(32|60|64|128|256)GB2|" // Corsair Nova, tested with Corsair CSSD-V32GB2/2.2
    "Corsair CMFSSD-(32|64|128|256)D1|" // Corsair Extreme, tested with Corsair CMFSSD-128D1/1.0
    "CRUCIAL_CT(64|128|256)M225|" // tested with CRUCIAL_CT64M225/1571
    "G.SKILL FALCON (64|128|256)GB SSD|" // tested with G.SKILL FALCON 128GB SSD/2030
    "OCZ[ -](AGILITY|ONYX|VERTEX( 1199|-TURBO| v1\\.10)?)|" // tested with
      // OCZ-ONYX/1.6, OCZ-VERTEX 1199/00.P97, OCZ-VERTEX/1.30, OCZ VERTEX-TURBO/1.5, OCZ-VERTEX v1.10/1370
    "Patriot[ -]Torqx.*|"
    "RENICE Z2|" // tested with RENICE Z2/2030
    "STT_FT[MD](28|32|56|64)GX25H|" // Super Talent Ultradrive GX, tested with STT_FTM64GX25H/1916
    "TS(18|25)M(64|128)MLC(16|32|64|128|256|512)GSSD|" // ASAX Leopard Hunt II, tested with TS25M64MLC64GSSD/0.1
    "FM-25S2I-(64|128)GBFII|" // G.Skill FALCON II, tested with FM-25S2I-64GBFII
    "TS(60|120)GSSD25D-M", // Transcend Ultra SSD (SATA II), see also Ticket #80
    "", "",
    "-v 1,raw64 " // Raw_Read_Error_Rate
    "-v 9,raw64 " // Power_On_Hours
    "-v 12,raw64 " // Power_Cycle_Count
    "-v 184,raw64,Initial_Bad_Block_Count "
    "-v 195,raw64,Program_Failure_Blk_Ct "
    "-v 196,raw64,Erase_Failure_Blk_Ct "
    "-v 197,raw64,Read_Failure_Blk_Ct "
    "-v 198,raw64,Read_Sectors_Tot_Ct "
    "-v 199,raw64,Write_Sectors_Tot_Ct "
    "-v 200,raw64,Read_Commands_Tot_Ct "
    "-v 201,raw64,Write_Commands_Tot_Ct "
    "-v 202,raw64,Error_Bits_Flash_Tot_Ct "
    "-v 203,raw64,Corr_Read_Errors_Tot_Ct "
    "-v 204,raw64,Bad_Block_Full_Flag "
    "-v 205,raw64,Max_PE_Count_Spec "
    "-v 206,raw64,Min_Erase_Count "
    "-v 207,raw64,Max_Erase_Count "
    "-v 208,raw64,Average_Erase_Count "
    "-v 209,raw64,Remaining_Lifetime_Perc "
    "-v 210,raw64,Indilinx_Internal "
    "-v 211,raw64,SATA_Error_Ct_CRC "
    "-v 212,raw64,SATA_Error_Ct_Handshake "
    "-v 213,raw64,Indilinx_Internal"
  },
  { "Indilinx Barefoot_2/Everest/Martini based SSDs",
    "OCZ VERTEX[ -]PLUS|" // tested with OCZ VERTEX-PLUS/3.55, OCZ VERTEX PLUS/3.55
    "OCZ-VERTEX PLUS R2|" // Barefoot 2, tested with OCZ-VERTEX PLUS R2/1.2
    "OCZ-OCTANE|" // Everest 1, tested with OCZ-OCTANE/1.13
    "OCZ-PETROL|" // Everest 1, tested with OCZ-PETROL/3.12
    "OCZ-AGILITY4|" // Everest 2, tested with OCZ-AGILITY4/1.5.2
    "OCZ-VERTEX4", // Everest 2, tested with OCZ-VERTEX4/1.5
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 232,raw48,Lifetime_Writes " // LBA?
  //"-v 233,raw48,Media_Wearout_Indicator"
  },
  { "Indilinx Barefoot 3 based SSDs",
    "OCZ-VECTOR(1[58]0)?|" // tested with OCZ-VECTOR/1.03, OCZ-VECTOR150/1.2, OCZ-VECTOR180
    "OCZ-VERTEX4[56]0A?|" // Barefoot 3 M10, tested with OCZ-VERTEX450/1.0, OCZ-VERTEX460/1.0, VERTEX460A
    "OCZ-SABER1000|"
    "OCZ-ARC100|"
    "Radeon R7", // Barefoot 3 M00, tested with Radeon R7/1.00
    "", "",
    "-v 5,raw48,Runtime_Bad_Block "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 171,raw48,Avail_OP_Block_Count "
    "-v 174,raw48,Pwr_Cycle_Ct_Unplanned "
    "-v 187,raw48,Total_Unc_NAND_Reads "
    "-v 195,raw48,Total_Prog_Failures "
    "-v 196,raw48,Total_Erase_Failures "
    "-v 197,raw48,Total_Unc_Read_Failures "
    "-v 198,raw48,Host_Reads_GiB "
    "-v 199,raw48,Host_Writes_GiB "
    "-v 205,raw48,Max_Rated_PE_Count "
    "-v 206,raw48,Min_Erase_Count "
    "-v 207,raw48,Max_Erase_Count "
    "-v 208,raw48,Average_Erase_Count "
    "-v 210,raw48,SATA_CRC_Error_Count "
    "-v 212,raw48,Pages_Requiring_Rd_Rtry "
    "-v 213,raw48,Snmple_Retry_Attempts "
    "-v 214,raw48,Adaptive_Retry_Attempts "
    "-v 222,raw48,RAID_Recovery_Count "
    "-v 224,raw48,In_Warranty "
    "-v 225,raw48,DAS_Polarity "
    "-v 226,raw48,Partial_Pfail "
    "-v 230,raw48,Write_Throttling "
    "-v 233,raw48,Remaining_Lifetime_Perc "
    "-v 241,raw48,Host_Writes_GiB " // M00/M10
    "-v 242,raw48,Host_Reads_GiB "  // M00/M10
    "-v 249,raw48,Total_NAND_Prog_Ct_GiB "
    "-v 251,raw48,Total_NAND_Read_Ct_GiB"
  },
  { "OCZ Intrepid 3000 SSDs", // tested with OCZ INTREPID 3600/1.4.3.6, 3800/1.4.3.0, 3700/1.5.0.4
    "OCZ INTREPID 3[678]00",
    "", "",
    "-v 5,raw48,Runtime_Bad_Block "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 100,raw48,Total_Blocks_Erased "
    "-v 171,raw48,Avail_OP_Block_Count "
    "-v 174,raw48,Pwr_Cycle_Ct_Unplanned "
    "-v 184,raw48,Factory_Bad_Block_Count "
    "-v 187,raw48,Total_Unc_NAND_Reads "
    "-v 190,tempminmax,Temperature_Celsius "
    "-v 195,raw48,Total_Prog_Failures "
    "-v 196,raw48,Total_Erase_Failures "
    "-v 197,raw48,Total_Unc_Read_Failures "
    "-v 198,raw48,Host_Reads_GiB "
    "-v 199,raw48,Host_Writes_GiB "
    "-v 202,raw48,Total_Read_Bits_Corr_Ct "
    "-v 205,raw48,Max_Rated_PE_Count "
    "-v 206,raw48,Min_Erase_Count "
    "-v 207,raw48,Max_Erase_Count "
    "-v 208,raw48,Average_Erase_Count "
    "-v 210,raw48,SATA_CRC_Error_Count "
    "-v 211,raw48,SATA_UNC_Count "
    "-v 212,raw48,NAND_Reads_with_Retry "
    "-v 213,raw48,Simple_Rd_Rtry_Attempts "
    "-v 214,raw48,Adaptv_Rd_Rtry_Attempts "
    "-v 221,raw48,Int_Data_Path_Prot_Unc "
    "-v 222,raw48,RAID_Recovery_Count "
    "-v 230,raw48,SuperCap_Charge_Status " // 0=not charged, 1=fully charged, 2=unknown
    "-v 233,raw48,Remaining_Lifetime_Perc "
    "-v 249,raw48,Total_NAND_Prog_Ct_GiB "
    "-v 251,raw48,Total_NAND_Read_Ct_GiB"
  },
  { "OCZ/Toshiba Trion SSDs",
    "OCZ-TRION1[05]0|" // tested with OCZ-TRION100/SAFM11.2A, TRION150/SAFZ72.2
    "TOSHIBA-TR150|" // tested with TOSHIBA-TR150/SAFZ12.3
    "TOSHIBA Q300( Pro\\.)?", // tested with TOSHIBA Q300 Pro./JYRA0101
    "", "",
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 167,raw48,SSD_Protect_Mode "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 169,raw48,Bad_Block_Count "
    "-v 173,raw48,Erase_Count "
    "-v 192,raw48,Unexpect_Power_Loss_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 241,raw48,Host_Writes"
  },
  { "InnoDisk InnoLite SATADOM D150QV SSDs", // tested with InnoLite SATADOM D150QV-L/120319
                                             // InnoLite SATADOM D150QV/120319
    "InnoLite SATADOM D150QV.*",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 2,raw48,Throughput_Performance "
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 7,raw48,Seek_Error_Rate " // from InnoDisk iSMART Linux tool, useless for SSD
  //"-v 8,raw48,Seek_Time_Performance "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 10,raw48,Spin_Retry_Count "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 170,raw16,Bad_Block_Count_New/Tot "
    "-v 173,raw16,Erase_Count_Max/Avg "
    "-v 175,raw48,Bad_Cluster_Table_Count "
    "-v 192,raw48,Unexpect_Power_Loss_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 197,raw48,Current_Pending_Sector "
    "-v 229,hex48,Flash_ID "
    "-v 235,raw16,Lat_Bad_Blk_Era/Wri/Rea "
    "-v 236,raw48,Unstable_Power_Count "
    "-v 240,raw48,Write_Head"
  },
  { "Innodisk 1ME3/3ME/3SE SSDs", // tested with 2.5" SATA SSD 3ME/S140714,
      // Mini PCIeDOM 1ME3/S15604, InnoDisk Corp. - mSATA 3SE/S130710
    "((1\\.8|2\\.5)\"? SATA SSD|InnoDisk Corp\\. - mSATA|Mini PCIeDOM|SATA Slim) (1ME3|3[MS]E)",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 2,raw48,Throughput_Performance "
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 7,raw48,Seek_Error_Rate "       // ?
    "-v 8,raw48,Seek_Time_Performance " // ?
  //"-v 9,raw24(raw8),Power_On_Hours "
    "-v 10,raw48,Spin_Retry_Count "     // ?
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 169,hex48,Unknown_Innodisk_Attr "
    "-v 170,raw16,Bad_Block_Count "
    "-v 173,raw16,Erase_Count "
    "-v 175,raw48,Bad_Cluster_Table_Count "
    "-v 176,raw48,Uncorr_RECORD_Count "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius " // ] only in spec
  //"-v 197,raw48,Current_Pending_Sector "
    "-v 225,raw48,Unknown_Innodisk_Attr "
    "-v 229,hex48,Flash_ID "
    "-v 235,raw48,Later_Bad_Block "
    "-v 236,raw48,Unstable_Power_Count "
    "-v 240,raw48,Write_Head"
  },
  { "Innodisk 3IE2/3ME2/3MG2/3SE2/3TG6 SSDs", // tested with 2.5" SATA SSD 3MG2-P/M140402,
      // 1.8 SATA SSD 3IE2-P/M150821, 2.5" SATA SSD 3IE2-P/M150821,
      // SATA Slim 3MG2-P/M141114, M.2 (S80) 3MG2-P/M141114, M.2 (S42) 3SE2-P/M150821,
      // M.2 (S42) 3ME2/M151013, SATA Slim 3TG6-P/A19926J
    "((1\\.8|2\\.5)\"? SATA SSD|SATA Slim|M\\.2 \\(S(42|80)\\)) 3(IE2|ME2|MG2|SE2|TG6)(-P)?",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 2,raw48,Throughput_Performance "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 160,raw48,Uncorrectable_Error_Cnt "
    "-v 161,raw48,Number_of_Pure_Spare "
    "-v 163,raw48,Total_Bad_Block_Count "
    "-v 164,raw48,Total_Erase_Count "
    "-v 165,raw48,Max_Erase_Count "
    "-v 166,raw48,Min_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 168,raw48,Max_Erase_Count_of_Spec "
    "-v 169,raw48,Remaining_Lifetime_Perc "
    "-v 170,raw48,Spare_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
  //"-v 175,raw48,Program_Fail_Count_Chip "
  //"-v 176,raw48,Erase_Fail_Count_Chip "
  //"-v 177,raw48,Wear_Leveling_Count "
    "-v 178,raw48,Runtime_Invalid_Blk_Cnt "
  //"-v 181,raw48,Program_Fail_Cnt_Total "
  //"-v 182,raw48,Erase_Fail_Count_Total "
  //"-v 187,raw48,Reported_Uncorrect " // ] only in spec
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "  // ]
    "-v 229,raw48,Flash_ID "  // ]
  //"-v 232,raw48,Available_Reservd_Space "
    "-v 233,raw48,Flash_Writes_32MiB " // ]
    "-v 234,raw48,Flash_Reads_32MiB "  // ]
    "-v 235,raw48,Later_Bad_Block_Info "  // ]
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 245,raw48,Flash_Writes_32MiB "
    "-v 248,raw48,Remaining_Life "
    "-v 249,raw48,Spare_Blocks_Remaining"
  },
  { "Innodisk 1IE3/3IE3/3ME3/3IE4/3ME4 SSDs", // tested with 2.5" SATA SSD 3ME3/S15A19,
      // InnoDisk Corp. - mSATA 3ME3/S15A19, mSATA mini 3ME3/S15A19, M.2 (S42) 3ME3,
      // SATA Slim 3ME3/S15A19, SATADOM-MH 3ME3/S15A19, SATADOM-ML 3ME3/S15A19,
      // SATADOM-MV 3ME3/S15A19, SATADOM-SL 3ME3/S15A19, SATADOM-SV 3ME3/S15A19,
      // SATADOM-SL 3IE3/S151019N, 2.5" SATA SSD 3IE3/S15C14i, CFast 3IE3/S15C14i,
      // InnoDisk Corp. - mSATA 3IE3/S15C14i, Mini PCIeDOM 1IE3/S15C14i, CFast 3ME3/S15A19
      // mSATA mini 3IE3/S15C14i, M.2 (S42) 3IE3/S15C14i, SATA Slim 3IE3/S15C14i,
      // SATADOM-SH 3IE3 V2/S15C14i, SATADOM-SL 3IE3 V2/S15A19i, SATADOM-SV 3IE3 V2/S15C14i
      // mSATA 3ME4/L16711, M.2 (S42) 3ME4/L16711, SATADOM-MH 3ME4/L16B01,
      // SATADOM-SH 3ME4/L16B01, SATADOM-SH Type C 3ME4/L16B01, SATADOM-SH Type D 3ME4/L16B01,
      // mSATA 3IE4/L16B01Hi
    "(2.5\" SATA SSD|CFast|Mini PCIeDOM|(InnoDisk Corp\\. - )?mSATA( mini)?) (1IE3|3[IM]E[34])( V2)?|"
    "(M\\.2 \\(S42\\)|SATA Slim|SATADOM-[MS][HLV]( Type [CD])?) (1IE3|3[IM]E[34])( V2)?",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 2,raw48,Throughput_Performance "
  //"-v 3,raw16(avg16),Spin_Up_Time "
    "-v 5,raw48,Later_Bad_Block "
    "-v 7,raw48,Seek_Error_Rate "       // ?
    "-v 8,raw48,Seek_Time_Performance " // ?
  //"-v 9,raw24(raw8),Power_On_Hours "
    "-v 10,raw48,Spin_Retry_Count "     // ?
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 163,raw48,Total_Bad_Block_Count "
    "-v 165,raw48,Max_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 169,raw48,Remaining_Lifetime_Perc "
    "-v 170,raw48,Spare_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 175,raw48,Bad_Cluster_Table_Count "
    "-v 176,raw48,RANGE_RECORD_Count "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 197,raw48,Current_Pending_Sector "
    "-v 225,raw48,Data_Log_Write_Count "
    "-v 229,hex48,Flash_ID "
    "-v 232,raw48,Spares_Remaining_Perc "
    "-v 235,raw16,Later_Bad_Blk_Inf_R/W/E " // Read/Write/Erase
    "-v 240,raw48,Write_Head "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB"
  },
  { "InnoDisk iCF 9000 / 1SE2 Cards", // tested with InnoDisk Corp. - iCF9000 1GB/140808,
      // InnoDisk Corp. - iCF9000 64GB/140808, InnoDisk Corp. - EDC 1SE2 H 64GB/131216
    "InnoDisk Corp\\. - (iCF9000|EDC 1SE2 H) (1|2|4|8|16|32|64)GB",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 160,raw48,Uncorrectable_Error_Cnt "
    "-v 161,raw48,Valid_Spare_Block_Cnt "
    "-v 162,raw48,Child_Pair_Count "
    "-v 163,raw48,Initial_Bad_Block_Count "
    "-v 164,raw48,Total_Erase_Count "
    "-v 165,raw48,Max_Erase_Count "
    "-v 166,raw48,Min_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
  //"-v 229,raw48,Flash_ID " // only in spec
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB"
  },
  { "Intel X25-E SSDs", // tested with
      // INTELSSDSA2SH064G1IB 43W7659 44E9163IBM/447C8860
    "(INTEL)?SSDSA2SH(032|064)G1.* (.*IBM|INTEL)", // G1 = first generation
    "", "",
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Intel_Internal "
    "-v 227,raw48,Intel_Internal "
    "-v 228,raw48,Intel_Internal "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator"
  },
  { "Intel X18-M/X25-M G1 SSDs",
    "INTEL SSDSA[12]MH(080|160)G1.*",  // G1 = first generation, 50nm
    "", "",
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Intel_Internal "
    "-v 227,raw48,Intel_Internal "
    "-v 228,raw48,Intel_Internal "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator"
  },
  { "Intel X18-M/X25-M/X25-V G2 SSDs", // fixed firmware
      // tested with INTEL SSDSA2M(080|160)G2GC/2CV102J8 (X25-M)
    "INTEL SSDSA[12]M(040|080|120|160)G2.*",  // G2 = second generation, 34nm
    "2CV102(J[89A-Z]|[K-Z].)", // >= "2CV102J8"
    "",
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
  //"-v 184,raw48,End-to-End_Error " // G2 only
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator"
  },
  { "Intel X18-M/X25-M/X25-V G2 SSDs", // buggy or unknown firmware
      // tested with INTEL SSDSA2M040G2GC/2CV102HD (X25-V)
    "INTEL SSDSA[12]M(040|080|120|160)G2.*",
    "",
    "This drive may require a firmware update to\n"
    "fix possible drive hangs when reading SMART self-test log.",
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes"
  },
  { "Intel 311/313 Series SSDs", // tested with INTEL SSDSA2VP020G2/2CV102M5,
      // INTEL SSDSA2VP020G3/9CV10379, INTEL SSDMAEXC024G3H/9CV10379
    "INTEL SSD(SA2VP|MAEXC)(020|024)G[23]H?",
      // SA2VP = 2.5", MAEXC = mSATA, G2 = 311, G3 = 313
    "", "",
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Reserve_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB"
  },
  { "Intel 320 Series SSDs", // tested with INTEL SSDSA2CT040G3/4PC10362,
      // INTEL SSDSA2CW160G3/4PC10362, SSDSA2BT040G3/4PC10362, SSDSA2BW120G3A/4PC10362,
      // INTEL SSDSA2BW300G3D/4PC10362, SSDSA2BW160G3L/4PC1LE04, SSDSA1NW160G3/4PC10362,
      // INTEL SSDSA2BW160G3H/4PC10365
    "INTEL SSDSA[12][BCN][WT](040|080|120|160|300|600)G3[ADHL]?",
      // 2B = 2.5" 7mm, 2C = 2.5" 9.5mm, 1N = 1.8" microSATA, *H = HP OEM
    "", "",
    "-F nologdir "
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Reserve_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 183,raw48,SATA_Downshift_Count " // FW >= 4Px10362
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 199,raw48,CRC_Error_Count "      // FW >= 4Px10362
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB"
  },
  { "Intel 710 Series SSDs", // tested with INTEL SSDSA2BZ[12]00G3/6PB10362
    "INTEL SSDSA2BZ(100|200|300)G3",
    "", "",
    "-F nologdir "
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Reserve_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct " // Missing in 710 specification from September 2011
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 190,tempminmax,Airflow_Temperature_Cel "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB"
  },
  { "Intel 510 Series SSDs",
    "INTEL SSDSC2MH(120|250)A2",
    "", "",
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator"
  },
  { "Intel 520 Series SSDs", // tested with INTEL SSDSC2CW120A3/400i, SSDSC2BW480A3F/400i,
      // INTEL SSDSC2BW180A3L/LB3i
    "INTEL SSDSC2[BC]W(060|120|180|240|480)A3[FL]?",
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
  //"-v 184,raw48,End-to-End_Error "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
  //"-v 192,raw48,Power-Off_Retract_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 249,raw48,NAND_Writes_1GiB"
  },
  { "Intel 525 Series SSDs", // mSATA, tested with SSDMCEAC120B3/LLLi
    "INTEL SSDMCEAC(030|060|090|120|180|240)B3",
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
  //"-v 190,tempminmax,Airflow_Temperature_Cel "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 249,raw48,NAND_Writes_1GiB"
  },
  { "Intel 53x and Pro 1500/2500 Series SSDs", // SandForce SF-2281, tested with
      // INTEL SSDSC2BW180A4/DC12, INTEL SSDSC2BW240A4/DC12, INTEL SSDMCEAW120A4/DC33,
      // INTEL SSDMCEAW240A4/DC33, INTEL SSDSC2BF180A4H/LH6i, INTEL SSDSC2BF480A5/TG26,
      // INTEL SSDSC2BF240A5L/LT2i, INTEL SSDSC2BW240H6/RG21
    "INTEL SSD(MCEA|SC2B|SCKJ)[WF](056|080|120|180|240|360|480)(A4H?|A5L?|H6)",
      // SC2B = 2.5", MCEA = mSATA, SCKJ = M.2; A4 = 530/Pro 1500, A5 = Pro 2500, H6 = 535
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
  //"-v 190,tempminmax,Airflow_Temperature_Cel "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 249,raw48,NAND_Writes_1GiB"
  },
  { "Intel 330/335 Series SSDs", // tested with INTEL SSDSC2CT180A3/300i, SSDSC2CT240A3/300i,
      // INTEL SSDSC2CT240A4/335t
    "INTEL SSDSC2CT(060|120|180|240)A[34]", // A4 = 335 Series
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
  //"-v 12,raw48,Power_Cycle_Count "
  //"-v 181,raw48,Program_Fail_Cnt_Total " // ] Missing in 330 specification from April 2012
  //"-v 182,raw48,Erase_Fail_Count_Total " // ]
  //"-v 192,raw48,Power-Off_Retract_Count "
    "-v 225,raw48,Host_Writes_32MiB "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 249,raw48,NAND_Writes_1GiB"
  },
  { "Intel 540 Series SSDs", // INTEL SSDSC2KW120H6/LSF036C, INTEL SSDSC2KW480H6/LSF036C
    "INTEL SSDSC[K2]KW(120H|180H|240H|360H|480H|010X)6",
    "", "",
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 183,raw48,SATA_Downshift_Count "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes "
    "-v 249,raw48,NAND_Writes_1GiB"
  },
  { "Intel 545s Series SSDs", // tested with INTEL SSDSCKKW512G8, INTEL SSDSC2KW512G8/LHF002C
      // SSDSCKKW128G8X1, SSDSCKKW256G8X1, SSDSCKKW512G8X1, SSDSCKKW010T8X1
      // INTEL SSDSCKKF512G8 SATA 512GB/LHFD05N
    "INTEL SSDSC[2K]K[WF](128G|256G|512G|010T)8.*",
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
  //"-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
  //"-v 173 is missing in official Intel doc"
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 190,tempminmax,Temperature_Case "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 199,raw48,CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
  //"-v 236 is missing in official Intel doc"
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 249,raw48,NAND_Writes_1GiB "
  //"-v 252 is missing in official intel doc"
  },
  { "Intel 730 and DC S35x0/3610/3700 Series SSDs", // tested with INTEL SSDSC2BP480G4, SSDSC2BB120G4/D2010355,
      // INTEL SSDSC2BB800G4T, SSDSC2BA200G3/5DV10250, SSDSC2BB080G6/G2010130,  SSDSC2BX200G4/G2010110,
      // INTEL SSDSC2BB016T6/G2010140, SSDSC2BX016T4/G2010140, SSDSC2BB150G7/N2010101,
      // INTEL SSDSC2BB480H4/D2010380, INTEL SSDSC2BB240G4C/D201FJ14, INTEL SSDSC2BA800G3E/5DV10250,
      // INTEL SSDSC1BG400G4/G2010150
    "INTEL SSDSC(1N|[12]B)[ABGPX]((080|100|120|150|160|200|240|300|400|480|600|800)[GH][3467][CERT]?|(012|016)T[46])|"
      // A = S3700, B*4 = S3500, B*6 = S3510, P = 730, X = S3610
      // Dell ships drives with model of the form SSDSC2BB120G4R
    "VK000(120|240|480)GWSXF", // tested with VK000480GWSXF/HPG2 (HPE INTEL SSDSC2BB480G4)
    "", "",
  //"-v 3,raw16(avg16),Spin_Up_Time "
  //"-v 4,raw48,Start_Stop_Count "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
    "-v 11,raw48,Unknown_Intel_Attribute " // VK000480GWSXF
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Unknown_Intel_Attribute " // VK000480GWSXF
    "-v 174,raw48,Unsafe_Shutdown_Count "
    "-v 175,raw16(raw16),Power_Loss_Cap_Test "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 190,tempminmax,Temperature_Case "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 194,tempminmax,Temperature_Internal "
  //"-v 197,raw48,Current_Pending_Sector "
    "-v 199,raw48,CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 234,raw24/raw32:04321,Thermal_Throttle "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 243,raw48,NAND_Writes_32MiB " // S3510/3610
    "-F xerrorlba" // tested with SSDSC2BB600G4/D2010355
  },
  { "Intel SSD Pro 5400s Series", // Tested with SSDSC2KF480H6/LSF036P,
      // INTEL SSDSC2KF256H6 SATA 256GB/LBFD16N
    "INTEL SSDSC[2K]KF((120|180|240|256|360|480|512)H|010X)6( .*)?",
    "", "",
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 183,raw48,SATA_Downshift_Count "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes "
    "-v 249,raw48,NAND_Writes_1GiB "
  },
  { "Intel DC S3110 Series SSDs", // Tested with INTEL SSDSCKKI256G8
    "INTEL SSDSCKKI(128|256|512)G8",
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
  //"-v 173 is missing in official Intel doc"
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
  //"-v 190,tempminmax,Airflow_Temperature_Cel "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
  //"-v 236 is missing in official Intel doc"
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 249,raw48,NAND_Writes_1GiB "
  //"-v 252 is missing in official Intel doc"
  },
  { "Intel 3710 Series SSDs", // INTEL SSDSC2BA200G4R/G201DL2B (dell)
    "INTEL SSDSC2BA(200G|400G|800G|012T)4.?",
    "", "",
    "-v 9,msec24hour32,Power_On_Hours_and_Msec "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 183,raw48,SATA_Downshift_Count "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes "
    "-v 234,raw24/raw32:04321,Thermal_Throttle "
    "-v 243,raw48,NAND_Writes_32MiB "
  },
  { "Intel S3520 Series SSDs", // INTEL SSDSC2BB960G7/N2010112, INTEL SSDSC2BB016T7/N2010112
    "INTEL SSDSC(2|K)(J|B)B(240G|480G|960G|150G|760G|800G|012T|016T)7.?",
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unsafe_Shutdown_Count "
    "-v 175,raw16(raw16),Power_Loss_Cap_Test "
    "-v 183,raw48,SATA_Downshift_Count "
    "-v 184,raw48,End-to-End_Error_Count "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
    "-v 190,tempminmax,Case_Temperature "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 194,tempminmax,Drive_Temperature "
    "-v 197,raw48,Pending_Sector_Count "
    "-v 199,raw48,CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 234,raw24/raw32:04321,Thermal_Throttle_Status "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 243,raw48,NAND_Writes_32MiB"
  },
  { "Dell Certified Intel S3520 Series SSDs",
    "SSDSC(2|K)(J|B)B(240G|480G|960G|120G|760G|800G|012T|016T)7R.?",
    "", "",
    "-v 170,raw48,Available_Reservd_Space "
    "-v 174,raw48,Unsafe_Shutdown_Count "
    "-v 195,raw48,Uncorrectable_Error_Cnt "
    "-v 199,raw48,CRC_Error_Count "
    "-v 201,raw16(raw16),Power_Loss_Cap_Test "
    "-v 202,raw48,End_of_Life "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
    "-v 233,raw48,Total_LBAs_Written "
    "-v 234,raw24/raw32:04321,Thermal_Throttle_Status "
    "-v 245,raw48,Percent_Life_Remaining"
  },
  { "Intel/Solidigm S46x0/S45x0 Series SSDs", // INTEL SSDSC2KB480G7/SCV10100,
      // INTEL SSDSC2KB960G7/SCV10100, INTEL SSDSC2KB038T7/SCV10100,
      // INTEL SSDSC2KB038T7/SCV10121, INTEL SSDSC2KG240G7/SCV10100,
      // INTEL SSDSC2KB480GZ/7CV10100, INTEL SSDSC2KB076T8/XCV10132,
      // SOLIDIGM SSDSC2KB960GZ/7CV10130
    "(INTEL|SOLIDIGM) SSDSC(2K|KK)(B|G)(240G|480G|960G|019T|038T|076T)[78Z].?",
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unsafe_Shutdown_Count "
    "-v 175,raw16(raw16),Power_Loss_Cap_Test "
    "-v 183,raw48,SATA_Downshift_Count "
    "-v 184,raw48,End-to-End_Error_Count "
    "-v 187,raw48,Uncorrectable_Error_Cnt "
    "-v 190,tempminmax,Drive_Temperature "
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 197,raw48,Pending_Sector_Count "
    "-v 199,raw48,CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator "
    "-v 234,raw24/raw32:04321,Thermal_Throttle_Status "
    "-v 235,raw16(raw16),Power_Loss_Cap_Test "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 243,raw48,NAND_Writes_32MiB"
  },
  { "Dell Certified Intel S4x00/D3-S4x10 Series SSDs", // INTEL SSDSC2KB480G7R/SCV1DL58,
      // INTEL SSDSC2KB960G7R/SCV1DL58, INTEL SSDSC2KB038T7R/SCV1DL58,
      // INTEL SSDSC2KB038T7R/SCV1DL58, INTEL SSDSC2KG240G7R/SCV1DL58
    "SSDSC(2K|KK)(B|G)(240G|480G|960G|019T|038T)(7R|8R).?",
    "", "",
    "-v 170,raw48,Available_Reservd_Space "
    "-v 174,raw48,Unsafe_Shutdown_Count "
    "-v 195,raw48,Uncorrectable_Error_Cnt "
    "-v 199,raw48,CRC_Error_Count "
    "-v 201,raw16(raw16),Power_Loss_Cap_Test "
    "-v 202,raw48,End_of_Life "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic " // Timed Workload Media Wear Indicator (percent*1024)
    "-v 227,raw48,Workld_Host_Reads_Perc "  // Timed Workload Host Reads Percentage
    "-v 228,raw48,Workload_Minutes " // 226,227,228 can be reset by 'smartctl -t vendor,0x40'
    "-v 233,raw48,Total_LBAs_Written "
    "-v 234,raw24/raw32:04321,Thermal_Throttle_Status "
    "-v 245,raw48,Percent_Life_Remaining"
  },
  { "Kingston branded X25-V SSDs", // fixed firmware
    "KINGSTON SSDNow 40GB",
    "2CV102(J[89A-Z]|[K-Z].)", // >= "2CV102J8"
    "",
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes"
  },
  { "Kingston branded X25-V SSDs", // buggy or unknown firmware
    "KINGSTON SSDNow 40GB",
    "",
    "This drive may require a firmware update to\n"
    "fix possible drive hangs when reading SMART self-test log.\n"
    "To update Kingston branded drives, a modified Intel update\n"
    "tool must be used. Search for \"kingston 40gb firmware\".",
    "-v 192,raw48,Unsafe_Shutdown_Count "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 226,raw48,Workld_Media_Wear_Indic "
    "-v 227,raw48,Workld_Host_Reads_Perc "
    "-v 228,raw48,Workload_Minutes"
  },
  { "Kingston SSDNow UV400/500",
    "KINGSTON SUV400S37A?(120|240|480|960)G|" // tested with KINGSTON SUV400S37120G/0C3J96R9,
      // KINGSTON SUV400S37240G/0C3J96R9, KINGSTON SUV400S37240G/0C3K87RA,
      // KINGSTON SUV400S37120G/0C3K87RA
    "KINGSTON SUV500(M[8S])?(120|240|480|960)G", // tested with KINGSTON SUV500120G/003056R6,
      // KINGSTON SUV500240G/003056R6, KINGSTON SUV500480G/003056RI,
      // KINGSTON SUV500MS120G/003056RA, KINGSTON SUV500MS120G/003056RI,
      // KINGSTON SUV500M8120G/003056RI
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 100,raw48,Unknown_Kingston_Attr "
    "-v 101,raw48,Unknown_Kingston_Attr "
    "-v 170,raw48,Reserved_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
  //"-v 175,raw48,Program_Fail_Count_Chip "
  //"-v 176,raw48,Erase_Fail_Count_Chip "
  //"-v 177,raw48,Wear_Leveling_Count "
  //"-v 178,raw48,Used_Rsvd_Blk_Cnt_Chip "
  //"-v 180,raw48,Unused_Rsvd_Blk_Cnt_Tot "
  //"-v 183,raw48,Runtime_Bad_Block "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 201,raw48,Unc_Read_Error_Rate "
  //"-v 204,raw48,Soft_ECC_Correction "
    "-v 231,raw48,SSD_Life_Left "
    "-v 241,raw48,Host_Writes_GiB "
    "-v 242,raw48,Host_Reads_GiB "
    "-v 250,raw48,Read_Retry_Count"
  },
  { "JMicron based SSDs", // JMicron JMF60x
    "Kingston SSDNow V Series [0-9]*GB|" // tested with Kingston SSDNow V Series 64GB/B090522a
    "TS(2|4|8|16|32|64|128|192)GSSD(18|25)[MS]?-[MS]", // Transcend IDE and SATA, tested with
      // TS32GSSD25-M/V090331, TS32GSSD18M-M/v090331
    "[BVv].*", // other Transcend SSD versions will be caught by subsequent entry
    "",
  //"-v 9,raw24(raw8),Power_On_Hours " // raw value always 0?
  //"-v 12,raw48,Power_Cycle_Count "
  //"-v 194,tempminmax,Temperature_Celsius " // raw value always 0?
    "-v 229,hex64:w012345r,Halt_System/Flash_ID " // Halt, Flash[7]
    "-v 232,hex64:w012345r,Firmware_Version_Info " // "YYMMDD", #Channels, #Banks
    "-v 233,hex48:w01234,ECC_Fail_Record " // Fail number, Row[3], Channel, Bank
    "-v 234,raw24/raw24:w01234,Avg/Max_Erase_Count "
    "-v 235,raw24/raw24:w01z23,Good/Sys_Block_Count"
  },
  { "JMicron/Maxiotek based SSDs", // JMicron JMF61x, JMF66x, JMF670
    "ADATA S596 Turbo|"  // tested with ADATA S596 Turbo 256GB SATA SSD (JMicron JMF616)
    "ADATA SP310|"  // Premier Pro SP310 mSATA, JMF667, tested with ADATA SP310/3.04
    "ADATA SP600(NS34)?|" // tested with ADATA SP600/2.4 (JMicron JMF661)
    "ADATA SX930|"  // tested with ADATA SX930/6.8SE
    "APPLE SSD TS(064|128|256|512)C|"  // Toshiba?, tested with APPLE SSD TS064C/CJAA0201
    "IM2S3138E-(128|256)GM-B|" // ADATA OEM, tested with IM2S3138E-128GM-B/DA002
    "KingSpec KDM-SA\\.51-008GMJ|" // tested with KingSpec KDM-SA.51-008GMJ/1.092.37 (JMF605?)
    "KINGSTON SNV425S2(64|128)GB|"  // SSDNow V Series (2. Generation, JMF618),
                                    // tested with KINGSTON SNV425S264GB/C091126a
    "KINGSTON SSDNOW 30GB|" // tested with KINGSTON SSDNOW 30GB/AJXA0202
    "KINGSTON SS100S2(8|16)G|"  // SSDNow S100 Series, tested with KINGSTON SS100S28G/D100309a
    "KINGSTON SNVP325S2(64|128|256|512)GB|" // SSDNow V+ Series, tested with KINGSTON SNVP325S2128GB/AGYA0201
    "KINGSTON SVP?100S2B?(64|96|128|256|512)G|"  // SSDNow V100/V+100 Series,
      // tested with KINGSTON SVP100S296G/CJR10202, KINGSTON SV100S2256G/D110225a
    "KINGSTON SV200S3(64|128|256)G|" // SSDNow V200 Series, tested with KINGSTON SV200S3128G/E120506a
    "[MN]T-(64|128|256|512|[124]TB?)( 22..)?|" // KingSpec MT/NT, MAS0902A-B2C or CS1802A-B2C, tested with
      // MT-512/SN12574, NT-512/T191212, NT-1TB 2242/SN12574
    "TOSHIBA THNS128GG4BBAA|"  // Toshiba / Super Talent UltraDrive DX,
                               // tested with Toshiba 128GB 2.5" SSD (built in MacBooks)
    "TOSHIBA THNSNC128GMLJ|" // tested with THNSNC128GMLJ/CJTA0202 (built in Toshiba Protege/Dynabook)
    "TS(8|16|32|64|128|192|256|512)GSSD25S?-(MD?|S)|" // Transcend IDE and SATA, JMF612, tested with
      // TS256GSSD25S-M/101028, TS32GSSD25-M/20101227
    "TS(32|64|128|256)G(SSD|MSA)[37]40K?", // Transcend SSD340/340K/740 SATA/mSATA, JMF667/670, tested with
      // TS256GSSD340/SVN263, TS256GSSD340/SVN423b, TS256GMSA340/SVN263,
      // TS128GSSD340K/SVN216,TS64GSSD740/SVN167d
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 2,raw48,Throughput_Performance "
    "-v 3,raw48,Unknown_JMF_Attribute "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 7,raw48,Unknown_JMF_Attribute "
    "-v 8,raw48,Unknown_JMF_Attribute "
  //"-v 9,raw24(raw8),Power_On_Hours "
    "-v 10,raw48,Unknown_JMF_Attribute "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 167,raw48,Unknown_JMF_Attribute "
    "-v 168,raw48,SATA_Phy_Error_Count "
    "-v 169,raw48,Unknown_JMF_Attribute "
    "-v 170,raw16,Bad_Block_Count "
    "-v 173,raw16,Erase_Count " // JMF661: different?
    "-v 175,raw48,Bad_Cluster_Table_Count "
    "-v 180,raw48,Unknown_JMF_Attribute "
    "-v 187,raw48,Unknown_JMF_Attribute "
    "-v 192,raw48,Unexpect_Power_Loss_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 197,raw48,Current_Pending_Sector "
    "-v 231,raw48,Unknown_JMF_Attribute "
    "-v 233,raw48,Unknown_JMF_Attribute " // FW SVN423b
    "-v 234,raw48,Unknown_JMF_Attribute " // FW SVN423b
    "-v 240,raw48,Unknown_JMF_Attribute "
  //"-v 241,raw48,Total_LBAs_Written "    // FW SVN423b
  //"-v 242,raw48,Total_LBAs_Read "       // FW SVN423b
  },
  { "Plextor M3/M5/M6/M7/S2G Series SSDs", // Marvell 88SS9174 (M3, M5S), 88SS9187 (M5P, M5Pro), 88SS9188 (M6M/S),
      // tested with PLEXTOR PX-128M3/1.01, PX-128M3P/1.04, PX-256M3/1.05, PX-128M5S/1.02, PX-256M5S/1.03,
      // PX-128M5M/1.05, PX-128M5S/1.05, PX-128M5Pro/1.05, PX-512M5Pro/1.06, PX-256M5P/1.01, PX-128M6S/1.03
      // (1.04/5 Firmware self-test log lifetime unit is bogus, possibly 1/256 hours)
      // PLEXTOR PX-256M6S+/1.00, PLEXTOR  PX-128M3/1.00, PLEXTOR PX-128M3/1.07, PLEXTOR PX-128M6V/1.04,
      // PLEXTOR PX-128M6G-2242/1.01, PLEXTOR PX-512M7VC/1.05, PLEXTOR PX-512M8VC +/1.00,
      // PLEXTOR PX-512S2G/1.02 (Silicon Motion SM2258 ?)
    "PLEXTOR  ?PX-(64|128|256|512|768)(M(3P?|5[MPS]|5Pro|6[GMSV]|[78]VC)|S2G)(\\+|-.*| )?",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Unknown_Plextor_Attrib "  // M6S/1.03
    "-v 171,raw48,Unknown_Plextor_Attrib "  // M6S/1.03
    "-v 172,raw48,Unknown_Plextor_Attrib "  // M6S/1.03
    "-v 173,raw48,Unknown_Plextor_Attrib "  // M6S/1.03
    "-v 174,raw48,Unknown_Plextor_Attrib "  // M6S/1.03
  //"-v 175,raw48,Program_Fail_Count_Chip " // M6S/1.03
  //"-v 176,raw48,Erase_Fail_Count_Chip "   // M6S/1.03
  //"-v 177,raw48,Wear_Leveling_Count "
  //"-v 178,raw48,Used_Rsvd_Blk_Cnt_Chip "
  //"-v 179,raw48,Used_Rsvd_Blk_Cnt_Tot "   // M6S/1.03
  //"-v 180,raw48,Unused_Rsvd_Blk_Cnt_Tot " // M6S/1.03
  //"-v 181,raw48,Program_Fail_Cnt_Total "
  //"-v 182,raw48,Erase_Fail_Count_Total "
  //"-v 183,raw48,Runtime_Bad_Block "       // M6S/1.03
  //"-v 184,raw48,End-to-End_Error "        // M6S/1.03
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 188,raw48,Command_Timeout "         // M6S/1.03
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 195,raw48,Hardware_ECC_Recovered "  // MS6/1.03
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
  //"-v 232,raw48,Available_Reservd_Space "
  //"-v 233,raw48,Media_Wearout_Indicator " // MS6/1.03
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB"
  },
  { "Samsung based SSDs",
    "SAMSUNG SSD PM800 .*GB|"  // SAMSUNG PM800 SSDs, tested with SAMSUNG SSD PM800 TH 64GB/VBM25D1Q
    "SAMSUNG SSD PM810 .*GB|"  // SAMSUNG PM810 (470 series) SSDs, tested with
      // SAMSUNG SSD PM810 2.5" 128GB/AXM06D1Q
    "SAMSUNG SSD SM841N? (2\\.5\"? 7mm |mSATA )?(128|256|512)GB( SED)?|" // tested with
      // SAMSUNG SSD SM841 2.5" 7mm 256GB/DXM02D0Q, SAMSUNG SSD SM841 mSATA 512GB/DXM44D0Q,
      // SAMSUNG SSD SM841N 2.5 7mm 128GB/DXM03D0Q, SAMSUNG SSD SM841N mSATA 256GB SED/DXM45D6Q
    "SAMSUNG SSD PM851 (mSATA |M\\.2 )?(2280 )?(128|256|512)GB|" // tested with SAMSUNG SSD PM851 mSATA 128GB,
      // SAMSUNG SSD PM851 M.2 2280 256GB/EXT25D0Q
    "SAMSUNG 470 Series SSD|"  // tested with SAMSUNG 470 Series SSD 64GB/AXM09B1Q
    "Samsung SSD 750 EVO (120|250|500)GB|" // tested with Samsung SSD 750 EVO 250GB/MAT01B6Q
    "SAMSUNG SSD 830 Series|"  // tested with SAMSUNG SSD 830 Series 64GB/CXM03B1Q
    "SAMSUNG SSD PM830 .*|" // SAMSUNG SSD PM830 2.5" 7mm 128GB/CXM03D1Q
    "MZ7PC(512|256|128|064)HA(GH|FU|DR)-000.*|" // probably PM830, tested with SAMSUNG MZ7PC128HAFU-000L1/CXM04L1Q
    "Samsung SSD 840 (PRO )?Series|" // tested with Samsung SSD 840 PRO Series 128GB/DXM04B0Q,
      // Samsung SSD 840 Series/DXT06B0Q
    "Samsung SSD 8[4-7]0 EVO (mSATA |M\\.2 )?((120|250|500|750)G|[124]T)B|" // tested with
      // Samsung SSD 840 EVO (120|250|500|750)GB/EXT0AB0Q,
      // Samsung SSD 840 EVO (120|250)GB/EXT0BB6Q, 1TB/EXT0BB0Q, 120GB mSATA/EXT41B6Q,
      // Samsung SSD 850 EVO 250GB/EMT01B6Q, Samsung SSD 850 EVO M.2 250GB/EMT21B6Q,
      // Samsung SSD 850 EVO mSATA 120GB/EMT41B6Q, Samsung SSD 850 EVO 2TB/EMT02B6Q,
      // Samsung SSD 860 EVO 250GB/RVT01B6Q, Samsung SSD 860 EVO mSATA 250GB/RVT41B6Q,
      // Samsung SSD 860 EVO 500GB/RVT01B6Q, Samsung SSD 860 EVO mSATA 500GB/RVT41B6Q,
      // Samsung SSD 860 EVO mSATA 1TB/RVT41B6Q, Samsung SSD 860 EVO 2TB/RVT01B6Q,
      // Samsung SSD 860 EVO 4TB/RVT04B6Q, Samsung SSD 870 EVO 1TB/SVT01B6Q,
      // Samsung SSD 870 EVO 4TB/SVT02B6Q
    "Samsung SSD 8[56]0 PRO ((128|256|512)G|[124]T)B|" // tested with Samsung SSD 850 PRO 128GB/EXM01B6Q,
      // Samsung SSD 850 PRO 1TB/EXM01B6Q, Samsung SSD 850 PRO 2TB/EXM02B6Q,
      // Samsung SSD 860 PRO 256GB/RVM01B6Q, Samsung SSD 860 PRO 512GB/RVM01B6Q,
      // Samsung SSD 860 PRO 1TB/RVM01B6Q
    "Samsung SSD 8[67]0 QVO [1248]TB|" // tested with Samsung SSD 860 QVO 1TB/RVQ02B6Q,
      // Samsung SSD 860 QVO 2TB/RVQ01B6Q, Samsung SSD 870 QVO 4TB/SVQ01B6Q
    "Samsung SSD 883 DCT ((240|480|960)G|(1\\.92|3\\.84)T)B|" // tested with
      // Samsung SSD 883 DCT 480GB/HXT7404Q, Samsung SSD 883 DCT 3.84TB/HXT7404Q
    "Samsung SSD 845DC EVO .*|" // Samsung SSD 845DC EVO 960GB/EXT03X3Q
    "SAMSUNG MZ7PA256HMDR-.*|" // PM810 (470 Series), tested with SAMSUNG MZ7PA256HMDR-010H1/AXM07H1Q
    "SAMSUNG MZ[7M]PC(032|064|128|256|512)HBCD-.*|" // PM830, tested with SAMSUNG MZMPC032HBCD-000L1/CXM12L1Q
    "SAMSUNG MZ7[TP]D(128|256|512)H(AFV|CGM)-.*|" // 840 / 840 Pro (T/P), tested with.
      // SAMSUNG MZ7TD256HAFV-000L7/DXT06L6Q, SAMSUNG MZ7PD256HCGM-000H7/DXM06H6Q
    "SAMSUNG MZ[7M]TD(128|256|512)HA[GF][LMV]-.*|" // PM841, tested with SAMSUNG MZMTD512HAGL-00000/DXT4200Q,
      // SAMSUNG MZ7TD512HAGM-000L1/DXT06L0Q, SAMSUNG MZMTD128HAFV-000L1/DXT43L0Q
    "SAMSUNG MZ7WD((120|240)H[AC]FV|480H[AC]GM|960H[AC]GP)-.*|" // SM843T(N?) Series, tested with
      // SAMSUNG MZ7WD120HAFV-00003/DXM85W3Q, SAMSUNG MZ7WD120HCFV-00003/DXM9203Q,
      // SAMSUNG MZ7WD960HCGP-000PU/DXM9BW4Q (SM843TN?)
    "SAMSUNG MZ[7N]TE(128|256|512)HM(HP|JH)-.*|" // PM851, tested with SAMSUNG MZ7TE256HMHP-000L7/EXT09L6Q,
      // SAMSUNG MZNTE256HMHP-000H1/EXT22H0Q, SAMSUNG MZNTE512HMJH-000L2/EXT26L0Q
    "SAMSUNG MZMPF(032|064)HCFV-.*|" // CM851 mSATA, tested with SAMSUNG MZMPF032HCFV-000H1/FXM42H2Q
    "SAMSUNG MZ7GE(240HMGR|(480|960)HMHP)-00003|" // SM853T Series, tested with
      // SAMSUNG MZ7GE240HMGR-00003/EXT0303Q
    "SAMSUNG MZ7LM(120|240|480|960|1T9|3T8)HC(JM|HP|GR|FD)-.*|" // PM863 Series, tested with
      // SAMSUNG MZ7LM960HCHP-0E003/GXT3003Q
    "(SAMSUNG )?MZ7LM(240|480|960|1T9|3T8)HM(JP|HQ|LP)(-.*|0D3)|" // PM863a Series, tested with
      // SAMSUNG MZ7LM3T8HMLP-00005/GXT5104Q, MZ7LM240HMHQ0D3/GC5B (Dell)
    "(SAMSUNG )?MZ7KM(120|240|480|960|1T9)H[AM](FD|GR|H[PQ]|J[MP])(-.*|0D3)|" // SM863(a), tested with
      // SAMSUNG MZ7KM480HAHP-0E005/GXM1003Q, SAMSUNG MZ7KM480HMHQ-00005/GXM5104Q,
      // SAMSUNG MZ7KM960HMJP-00005/GXM5304Q, MZ7KM960HMJP0D3/GD53 (Dell)
    "SAMSUNG MZ[7N]LH(128|256|512|1T0)H[AB](JD|HQ|L[BU])-.*|" // PM881, tested with
      // SAMSUNG MZ7LH512HALU-00000/RVT0200Q
    "SAMSUNG MZ7LH(240|480|960|1T9|3T8|7T6)H[AM](HQ|JR|LT|LA)-.*|" //PM883, tested with SAMSUNG MZ7LH960HAJR-00005
    "SAMSUNG MZ7L3(240|480|960|1T9|3T8|7T6)H(B[LN][AT]|CHQ|CJR)-.*|" // PM893/897, tested with
      // SAMSUNG MZ7L3240HCHQ-00A07/JXTC104Q, SAMSUNG MZ7L3480HCHQ-00A07/JXTC104Q,
      // SAMSUNG MZ7L3480HBLT-00A07/JXTE004Q, SAMSUNG MZ7L33T8HBLT-00A07/JXTC104Q
    "MK000(240|480|960)G(WCEV|ZXR[AB])|" // MK000960GZXRB/HPG0 (HPE MZ7L3960HBLT-00AH3),
      // MK000480GZXRA/HPG0 (HPE P18432-B21), MK000480GWCEV/HPG3 (HPE)
    "SAMSUNG MZ7KH(240|480|960|1T9|3T8)HA(HQ|JR|LS)-.*|" //SM883
    "SAMSUNG MZ[7N](LF|TY)(128|192|256)H[CD](GS|HP)-.*|" // CM871/871a, tested with SAMSUNG MZNLF128HCHP-000H1/FXT21H1Q,
      // SAMSUNG MZNTY256HDHP-000/MAT21K0Q, SAMSUNG MZ7LF192HCGS-000L1/FXT03L1Q
    "SAMSUNG MZ[7NY]LN(128|256|512|1T0)H[ACM](GR|HP|HQ|J[HPQ]|LR)-.*|" // PM871/871a/b, tested with
      // SAMSUNG MZ7LN128HCHP-00000/EMT0100Q, SAMSUNG MZ7LN256HAHQ-000H1/MVT03H6Q,
      // SAMSUNG MZNLN256HMHQ-000H1/MAV21H3Q, SAMSUNG MZYLN256HCHP-000L2/EMT63L0Q
    "SAMSUNG SSD PM871 .*|" // SAMSUNG SSD PM871 2.5 7mm 256GB/EMT02D0Q
      // SAMSUNG MZ7LN256HMJP-00000/MAV0100Q, SAMSUNG MZ7LN512HMJP-00000/MAV0100Q
    "SAMSUNG MZHPV(128|256|512)HDG(L|M)-.*|" // SM951, tested with SAMSUNG MZHPV512HDGL-00000/BXW2500Q,
      // SAMSUNG MZHPV128HDGM-00000 (BXW2500Q)
    "Samsung Portable SSD T5", // tested with Samsung Portable SSD T5 (0x04e8:0x61f5)
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 170,raw48,Unused_Rsvd_Blk_Ct_Chip " // CM871
    "-v 171,raw48,Program_Fail_Count_Chip " // CM871
    "-v 172,raw48,Erase_Fail_Count_Chip " // CM871
    "-v 173,raw48,Wear_Leveling_Count " // CM871
    "-v 174,raw48,Unexpect_Power_Loss_Ct " // CM871
  //"-v 175,raw48,Program_Fail_Count_Chip "
  //"-v 176,raw48,Erase_Fail_Count_Chip "
  //"-v 177,raw48,Wear_Leveling_Count "
  //"-v 178,raw48,Used_Rsvd_Blk_Cnt_Chip "
  //"-v 179,raw48,Used_Rsvd_Blk_Cnt_Tot "
  //"-v 180,raw48,Unused_Rsvd_Blk_Cnt_Tot "
  //"-v 181,raw48,Program_Fail_Cnt_Total "
  //"-v 182,raw48,Erase_Fail_Count_Total "
  //"-v 183,raw48,Runtime_Bad_Block "
  //"-v 184,raw48,End-to-End_Error " // SM843T Series
    "-v 187,raw48,Uncorrectable_Error_Cnt "
  //"-v 190,tempminmax,Airflow_Temperature_Cel "  // seems to be some sort of temperature value for 470 Series?
    "-v 191,raw48,Unknown_Samsung_Attr " // PM810
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw48,ECC_Error_Rate "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector " // PM893
  //"-v 198,raw48,Offline_Uncorrectable "
    "-v 199,raw48,CRC_Error_Count "
    "-v 201,raw48,Supercap_Status "
    "-v 202,raw48,Exception_Mode_Status " // PM893
  //"-v 233,raw48,Media_Wearout_Indicator " // PM851, 840
    "-v 234,raw48,Unknown_Samsung_Attr " // PM851, 840
    "-v 235,raw48,POR_Recovery_Count " // PM851, 830/840/850, PM893
    "-v 236,raw48,Unknown_Samsung_Attr " // PM851, 840
    "-v 237,raw48,Unknown_Samsung_Attr " // PM851, 840
    "-v 238,raw48,Unknown_Samsung_Attr " // PM851, 840
  //"-v 241,raw48,Total_LBAs_Written "
  //"-v 242,raw48,Total_LBAs_Read " // PM851, SM841N
    "-v 243,raw48,SATA_Downshift_Ct " // PM863, PM893
    "-v 244,raw48,Thermal_Throttle_St " // PM863, PM893
    "-v 245,raw48,Timed_Workld_Media_Wear " // PM863, PM893
    "-v 246,raw48,Timed_Workld_RdWr_Ratio " // PM863, PM893
    "-v 247,raw48,Timed_Workld_Timer " // PM863, PM893
    "-v 249,raw48,NAND_Writes_1GiB " // CM871a, PM871
    "-v 250,raw48,SATA_Iface_Downshift " // from the spec
    "-v 251,raw48,NAND_Writes " // PM863, PM893
    "-v 252,raw48,Added_Bad_Flash_Blk_Ct" // 870 EVO FW SVT02B6Q
  },
  { "Marvell based SanDisk SSDs",
    "SanDisk SD5SG2[0-9]*G1052E|" // X100 (88SS9174), tested with SanDisk SD5SG2256G1052E/10.04.01
    "SanDisk SD6S[BFP][12]M[0-9]*G(1022I?|1102)?|" // X110/X210 (88SS9175/187?), tested with SanDisk SD6SB1M064G1022I/X231600,
      // SanDisk SD6SB1M256G1022I/X231600, SanDisk SD6SF1M128G1022/X231200, SanDisk SD6SB2M512G1022I/X210400
      // SanDisk SD6SP1M128G1102/X231302
    "SanDisk SD7S[BN][67]S-?(128|256|512|960)G(1122|-1006)?|" // X300 (88SS9189?), tested with
      // SanDisk SD7SB6S128G1122/X3310000, SanDisk SD7SN6S-512G-1006/X3511006, SanDisk SD7SB7S960G/X36310DC
    "SanDisk SD8[ST][BN]8U-?((128|256|512)G|1T00)(1122|-10[01]6)|" // X400 (88SS1074), tested with SanDisk SD8SB8U128G1122/X4120000
      // SanDisk SD8TB8U-512G-1016/X4163116
    "SanDisk SD9S[BN]8W-?((128|256|512)G|[12]T00)(1122|-1006|1020)|" // X600, tested with SanDisk SD9SB8W128G1122/X6107000, SD9SB8W-512G-1006/X6103006
      // SanDisk SD9SB8W1T001122/X6107000, SD9SB8W256G1122/X6107000, SanDisk SD9SN8W128G1020/X6101020
    "SanDisk SDSSDA-((120|240|480)G|[12]T00)|" // Plus, tested with SanDisk SDSSDA-2T00/411040RL
    "SanDisk SDSSDHP[0-9]*G|" // Ultra Plus (88SS9175), tested with SanDisk SDSSDHP128G/X23[01]6RL
    "SanDisk (SDSSDHII|Ultra II )[0-9]*GB?|" // Ultra II (88SS9190/88SS9189), tested with
      // SanDisk SDSSDHII120G/X31200RL, SanDisk Ultra II 960GB/X41100RL
    "SanDisk SDSSDH2(128|256)G|" // SanDisk SDSSDH2128G/X211200
    "SanDisk SDSSDH3 ?((250|500|512|1000|1024|2000)G|[124]T00)|" // Ultra 3D, tested with SanDisk SDSSDH3250G/X61170RL,
      // SanDisk SDSSDH3 250G/401120RL, SanDisk SDSSDH3500G/X61110RL, SanDisk SDSSDH3 512G/40101000,
      // SanDisk SDSSDH31024G/X6107000, SanDisk SDSSDH3 1T00/415020RL, SanDisk SDSSDH3 2T00/411040RL,
      // SanDisk SDSSDH3 4T00/411040RL
    "SanDisk SDSSDXPS?[0-9]*G|" // Extreme II/Pro (88SS9187), tested with SanDisk SDSSDXP480G/R1311,
      // SanDisk SDSSDXPS480G/X21200RL
    "SanDisk SSD G5 BICS4|" // WD Blue SSD WDS100T2B0A (#1378), tested with SanDisk SSD G5 BICS4/415000WD
    "SanDisk SSD PLUS (120|240|480|[12]000) ?GB|" // Plus (88SS1074), tested with SanDisk SSD PLUS 120 GB/UE3000RL,
      // SanDisk SSD PLUS 120 GB/UE4500RL, SanDisk SSD PLUS 1000GB/UH4400RL
      // SanDisk SSD PLUS 2000GB/UP4504RL
    "SSD SATAIII 16GB", // SSD SATAIII 16GB/i221100 (see #923)
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 165,raw48,Total_Write/Erase_Count "
    "-v 166,raw48,Min_W/E_Cycle "
    "-v 167,raw48,Min_Bad_Block/Die "
    "-v 168,raw48,Maximum_Erase_Cycle "
    "-v 169,raw48,Total_Bad_Block "
    "-v 170,raw48,Unknown_Marvell_Attr " // SDSSDH3 4T00
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Avg_Write/Erase_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 188,raw48,Command_Timeout "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 199,raw48,SATA_CRC_Error "
    "-v 201,raw48,Lifetime_Remaining% "
    "-v 212,raw48,SATA_PHY_Error "
    "-v 230,raw16,Perc_Write/Erase_Count "
    "-v 232,raw48,Perc_Avail_Resrvd_Space "
    "-v 233,raw48,Total_NAND_Writes_GiB "
    "-v 234,raw48,Perc_Write/Erase_Ct_BC "
    "-v 241,raw48,Total_Writes_GiB "
    "-v 242,raw48,Total_Reads_GiB "
    "-v 243,raw48,Unknown_Marvell_Attr "
    "-v 244,raw48,Thermal_Throttle "
    "-v 249,raw48,TLC_NAND_GB_Writes"
  },
  { "SanDisk based SSDs", // see also #463 for the vendor attribute description
    "SanDisk iSSD P4 [0-9]*GB|" // tested with SanDisk iSSD P4 16GB/SSD 9.14
    "SanDisk pSSD|" // tested with SandDisk pSSD/3 (62.7 GB, SanDisk Extreme USB3.0 SDCZ80-064G-J57, 0x0781:0x5580)
    "SanDisk SDSSDP[0-9]*G|" // tested with SanDisk SDSSDP064G/1.0.0, SDSSDP128G/2.0.0
    "SanDisk SDSSDRC032G|" // tested with SanDisk SanDisk SDSSDRC032G/3.1.0
    "SanDisk SSD i100 [0-9]*GB|" // tested with SanDisk SSD i100 8GB/11.56.04, 24GB/11.56.04
    "SanDisk SSD U100 ([0-9]*GB|SMG2)|" // tested with SanDisk SSD U100 8GB/10.56.00, 256GB/10.01.02, SMG2/10.56.04
    "SanDisk SSD U110 (8|16|24|32|64|128)GB|" // tested with SanDisk SSD U110 32GB/U221000
    "SanDisk SDSA6[DGM]M-[0-9]*G-.*|" // tested with SanDisk SDSA6GM-016G-1006/U221006, SanDisk SDSA6MM-016G-1006/U221006,
      // SanDisk SDSA6GM-016G-1006/U221006
    "SanDisk SD7[SU]B[23]Q(064|128|256|512)G.*", // tested with SD7SB3Q064G1122/SD7UB3Q256G1122/SD7SB3Q128G/SD7UB2Q512G1122
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 165,raw48,Total_Write/Erase_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Avg_Write/Erase_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
  //"-v 187,raw48,Reported_Uncorrect "
    "-v 212,raw48,SATA_PHY_Error "
    "-v 230,raw48,Perc_Write/Erase_Count "
    "-v 232,raw48,Perc_Avail_Resrvd_Space "
    "-v 234,raw48,Perc_Write/Erase_Ct_BC "
  //"-v 241,raw48,Total_LBAs_Written "
  //"-v 242,raw48,Total_LBAs_Read "
    "-v 244,raw48,Thermal_Throttle "
  },
  // SDLF1DAR-480G-1HAW/ZR07RE41
  // SDLF1DAR-480G-1JA1/RP41ZH06
  { "Sandisk SATA Cloudspeed Max and GEN2 ESS SSDs",
    "SD[A-Z0-9]{2}[1-3][A-Z]{3}-?[0-9]{3}[GT]-?1[A-Z0-9]{3}",
    "","",
    "-v 13,raw48,Lifetime_UECC_Ct "
    "-v 32,raw48,Lifetime_Write_AmpFctr "
    "-v 33,raw48,Write_AmpFctr "
    "-v 170,raw48,Reserve_Erase_BlkCt "
    "-v 171,raw48,Program_Fail_Ct "
    "-v 172,raw48,Erase_Fail_Ct "
    "-v 173,raw48,Percent_Life_Used "
    "-v 174,raw48,Unexpect_Power_Loss "
    "-v 175,raw48,Lifetime_Die_Failure_Ct "
    "-v 177,raw48,Lifetime_Remaining% "
    "-v 178,raw48,SSD_LifeLeft(0.01%) "
    "-v 180,raw48,Undetected_Data_Err_Ct "
    "-v 183,raw48,LT_Link_Rate_DwnGrd_Ct "
    "-v 191,raw48,Clean_Shutdown_Ct "
    "-v 192,raw48,Unclean_Shutdown_Ct "
    "-v 196,raw48,Lifetime_Retried_Blk_Ct "
    "-v 204,raw48,Average_Block-Erase_Ct "
    "-v 205,raw48,Read_Retry_Enable_Ct "
    "-v 206,raw48,Successful_RaidRecov_Ct "
    "-v 207,raw48,Trimmed_Sector_Ct "
    "-v 211,raw48,Read_Disturb_ReallocEvt "
    "-v 233,raw48,Lifetime_Nand_Writes "
    "-v 235,raw48,Capacitor_Health "
    "-v 244,raw48,Therm_Throt_Activation "
    "-v 245,raw48,Drive_Life_Remaining% "
    "-v 253,raw48,SPI_Test_Remaining "
  },
  { "Sandisk SATA CS1K GEN1 ESS SSDs",
    "SD[A-Z0-9]{2}[NO][A-Z0-9]{3}-?[0-9]{3}[GT]-?1[A-Z0-9]{3}",
    "","",
    "-v 1,raw48,UECC_Ct "
    "-v 2,raw48,Internal_File_Check "
    "-v 5,raw16(raw16),Retried_Blk_Ct "
    "-v 32,raw48,Write_Ampflication "
    "-v 170,raw48,Reserve_Blk_Remaining "
    "-v 171,raw48,Program_Fail_Ct "
    "-v 172,raw48,Erase_Fail_Ct "
    "-v 173,raw48,Drive_Life_Used% "
    "-v 174,raw48,Unexpect_PwrLoss_Ct "
    "-v 175,raw48,PwrLoss_ProtectionFail "
    "-v 177,raw48,DriveLife_Remaining% "
    "-v 178,raw48,SSD_Life_Left "
    "-v 180,raw48,End_to_End_Err_Detect "
    "-v 190,raw48,Drive_Temp_Warning "
    "-v 195,raw48,Uncorrectable_Err_Ct "
    "-v 202,raw48,Exception_Mode_Status "
    "-v 233,raw48,Number_Of_Write_Ct "
    "-v 245,raw48,DriveLife_Used% "
  },
  { "Silicon Motion based SSDs",
    "ADATA_IMSS332-((008|016|032|064|128|256|512)G|001T)[AEMT]P?|" // tested with ADATA_IMSS332-128GTP/Q0810B
    "ADATA (SP550|SU(630|650(NS38)?|655|[89]00))|" // tested with ADATA SP550/O0803B5a, ADATA SU630/S1127B0,
      // ADATA SU650/S0212B0, ADATA SU650/V8X01c45, ADATA SU650/V8X21c64, ADATA SU650NS38/P191202a,
      // ADATA SU655/V8X01c55, ADATA SU800/Q0913A, ADATA SU800/R0427A, ADATA SU800/R0918B, ADATA SU900/Q0125A,
      // ADATA SU900/Q0710B
    "AMD R5SL512G|"// tested with AMD R5SL512G/V0929A0
    "CORSAIR FORCE LX SSD|" // tested with CORSAIR FORCE LX SSD/N0307A
    "CHN (25SATA01M|mSATAM3) (060|128|256|512)|" // Zheino A1/M3 tested with CHN 25SATA01M 060/20150529,
      // CHN mSATAM3 128/Q1124A0,
    "CIS 2S M305 (16|32|64|128|256)GB|" // Ceroz M305, tested with CIS 2S M305 64GB/P0316B
    "CT(120|250|500|1000)BX100SSD1|" // Crucial BX100, tested with CT250BX100SSD1/MU02,
      // CT500BX100SSD1/MU02, CT1000BX100SSD1/MU02
    "CT(240|480|960)BX200SSD1|" // Crucial BX200 Solid State Drive, tested with CT480BX200SSD1/MU02.6
    "DREVO X1 SSD|" // tested with DREVO X1 SSD/Q0111A
    "Drevo X1 pro (64|128|256)G|" // tested with Drevo X1 pro 64G/Q0303B
    "DEXP SSD C100 (128|256|512)Gb|" // tested with DEXP SSD C100 256Gb/V0218A0
    "HP SSD S700 ((128|256|512)G|1T)B|" // tested with HP SSD S700 1TB/V0823A0
    "JAJS[56]00M((12[08]|240|256|480|512|960)C|1TB)(-1)?|" // J&A LEVEN JS500/600 (Intenso TOP), tested with
      // JAJS500M120C-1/P0614D, JAJS600M1TB/T0529A0, JAJS600M256C/U0803A0
    "KingDian S100 (32|64)GB|" // SM2244LT, tested with KingDian S100 32GB/0311A
    "KingDian S(200|280|400) ((60|120|240|480)GB|1TB)|" // SM2256EN, tested with KingDian S200 60GB/R0724A0
      // KingDian S280 120GB/Q0526A, KingDian S280 1TB/S0509A0, KingDian S400 120GB/Q0607A
    "KingSpec KSD-[PS]A25\\.[1-9]-(016|032|064|128)(MS|SJ)|" // tested with KingSpec KSD-PA25.6-064MS/20140803
    "KINGSTON SKC600(MS)?(256|512|1024|2048)G|" // KC600 MS=mSATA, tested with KINGSTON SKC600256G/S4500105,
      // KINGSTON SKC600MS256G/S4500107
    "LITEON L[CM]H-(128|256|512)V2[MS](-.*)?|" // tested with LITEON LCH-256V2S-HP/2C02,
      // LITEON LCH-256V2S/3C87901, LITEON LMH-256V2M-11 MSATA 256GB/FM8110C
    "MKNSSDRE((25[06]|500|512)G|[12]T)B(-LT)?|" // Mushkin, tested with MKNSSDRE256GB/N1007C,
      // MKNSSDRE250GB-LT/O1026A
    "MKNSSD(S2|TR)(12[08]|2[45]0|480|500)GB(-(3DL|LT))?|" // Mushkin, tested with MKNSSDS2500GB/T0818A0,
      // MKNSSDTR500GB/O1126A, MKNSSDTR128GB-3DL/Q0616B0
    "NFN025SA31T-.*|" // Neo Forza (?), from HP Laptop, tested with NFN025SA31T-6000000/S0628A0
    "NFORCE (256|512)25 - SSZS13|" // Nextron NForce, tested with NFORCE 25625 - SSZS13/V0915A0
    "ONDA S-12 64GB|" // tested with ONDA S-12 64GB/U0401A0
    "OWC Envoy Pro|" // tested with OWC Envoy Pro/R0522A0 (0x1e91:0xa2a5)
    "Patriot P2[01]0 ((128|256|512)GB|[12]TB)|" // tested with Patriot P200 256GB/S1022A0,
      // Patriot P210 256GB/HPS2227P
    "R3SL(120|240|480|960)G|" // AMD Radeon SSDs, tested with R3SL240G/P0422C
    "Ramsta SSD S800 (120|240|480)GB|" // SM2258G, tested with Ramsta SSD S800 480GB/RS81V0
    "SED2QII-LP SATA SSD ((64|128|256|512)GB|[12]TB)|" // ACPI SED2QII-LP, tested with
      // SED2QII-LP SATA SSD 64GB/S0410A
    "T60|" // KingSpec T60, tested with T60/20151120
    "TCSUNBOW [MX]3 (60|120|240|480)GB|" // TC-Sunbow M3/X3, tested with TCSUNBOW M3 240GB/R0327B0,
      // TCSUNBOW X3 120GB/R1211A0, TCSUNBOW X3 480GB/S0509A0
    "TEAM( T253(TD|X6)?|L5Lite3D)((120|240|256|480|512)G|[12]TB?)|" // TEAMGROUP, tested with
      // TEAML5Lite3D240G/R0302A0 (L5Lite 3D), TEAM T253TD480G/Q0410A, TEAM T253X6256G/U1014A0 (CX2)
      // TEAM T2532TB/SN14546
    "TS((16|32|64|128|256|512)G|1T)(SSD|MS[AM])(230S?|3[67]0[SI]?|420[IK]?)|" // Transcend SSD230/360/370/420
      // SATA/mSATA, TS6500, tested with TS128GMSA230S/02J0S86A, TS32GMSA370/20140402,
      // mSATA MSM360 mini SSD, tested with TS32GMSM360/Q0407A
      // TS128GMSA370I/P1225CH1
      // TS16GMSA370/20140516, TS64GSSD370/20140516, TS256GSSD370/N0815B, TS256GSSD370S/N1114H,
      // TS512GSSD370S/N1114H, TS32GSSD420I/N1114H, TS32GSSD420K/P1225CE
    "TS(16|32|64|128|512|256)GMTS4[03]0S?|" // TS256GMTS400, TS256GMTS430S/S0423A
    "TS(120|240)GMTS420S?|" // Transcend MTS420, tested with TS120GMTS420S/R0510A0
    "TS(128G|256G|512G|1T|2T|4T)SSD230S|" // TS128GSSD230S/P1025F8, TS2TSSD230S/22Z4W14J
    "TS(120|240|480|960)GSSD220S|" // TS480GSSD220S/P0520AA
    "TS((64|128|256|512)G|[12]T)SSD452K|"// Transcend 452K, tested with TS128GSSD452K/02J0S86A
    "TS(16G|32G|64G|128G|256G|512G|1T)MTS800S?|" // MTS800, tested with TS1TMTS800/O1225H1
    "TS(16|32|64)GMSA630|" // MSA630 mSATA SSD, tested with TS32GMSA630/N0113E1
    "TS(32|64|128)GPSD330|" // Transcend PSD SSD, tested with TS64GPSD330/20140121
    "TS(16|32|64|96|128|256)GSSD(630|360S)|" // Transcend 630/360S, tested with TS16GSSD630/N0113E1,
      // TS256GSSD360S/R0123A0
    "TS(128G|256G|512G|1T)ESD400K|" // Transcend ESD400 Portable, tested with
      // TS256GESD400K/R0605AS (0x2174:0x2000)
    "TS(128G|256G|512G|1T)MTS830S|" // Transcend 830S, tested with TS256GMTS830S/02J0T3HB
    "TSG(16|32|64|128|256|512)MTS400ISI|" // Transcend MTS400I, tested with TSG64MTS400ISI/S0903D
    "UMAX 2242 (128|256|512)GB", // tested with UMAX 2242 256GB/U0330A0
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 2,raw48,Throughput_Performance "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 148,raw48,Total_SLC_Erase_Ct "
    "-v 149,raw48,Max_SLC_Erase_Ct "
    "-v 150,raw48,Min_SLC_Erase_Ct "
    "-v 151,raw48,Average_SLC_Erase_Ct "
    "-v 159,raw48,DRAM_1_Bit_Error_Count " // KINGSTON SKC600256G/S4500105
    "-v 160,raw48,Uncorrectable_Error_Cnt "
    "-v 161,raw48,Valid_Spare_Block_Cnt "
    "-v 162,raw48,Cache_Block_Count " // Transcend MSM360
    "-v 163,raw48,Initial_Bad_Block_Count "
    "-v 164,raw48,Total_Erase_Count "
    "-v 165,raw48,Max_Erase_Count "
    "-v 166,raw48,Min_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 168,raw48,Max_Erase_Count_of_Spec "
    "-v 169,raw48,Remaining_Lifetime_Perc "
  //"-v 175,raw48,Program_Fail_Count_Chip "
  //"-v 176,raw48,Erase_Fail_Count_Chip "
  //"-v 177,raw48,Wear_Leveling_Count "
    "-v 178,raw48,Runtime_Invalid_Blk_Cnt "
  //"-v 181,raw48,Program_Fail_Cnt_Total "
  //"-v 182,raw48,Erase_Fail_Count_Total "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 225,raw48,Host_Writes_32MiB " // FW 20140402
    "-v 231,raw48,SSD_Life_Left " // KINGSTON SKC600256G/S4500105
  //"-v 232,raw48,Available_Reservd_Space "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 245,raw48,TLC_Writes_32MiB " // FW N0815B, N1114H // TS128GMSA370I: Flash Write Sector Count
    "-v 246,raw48,SLC_Writes_32MiB "
    "-v 247,raw48,Raid_Recoverty_Ct "
    "-v 248,raw48,Unkn_SiliconMotion_Attr " // ADATA SU900/Q0125A
    "-v 249,raw48,Unkn_SiliconMotion_Attr " // ADATA SU650/V8X01c45
  //"-v 250,raw48,Read_Error_Retry_Rate " // ADATA SU800/Q0913A
    "-v 251,raw48,Unkn_SiliconMotion_Attr" // ADATA SU800/Q0913A
  },
  // Supermicro SSD-DM032-SMCMVN1, tested with SuperMicro SSD/SOB20R, see (#1380)
  { "Supermicro SATA DOM (SuperDOM)",
    "SuperMicro SSD",
    "", "",
    "-v 1,raw48,Raw_Read_Error_Rate "
    "-v 15,raw48,User_Cpcty_Sector_Cnt "
    "-v 160,raw48,Not_In_Use "
    "-v 161,raw48,Not_In_Use "
    "-v 163,raw48,Not_In_Use "
    "-v 164,raw48,Not_In_Use "
    "-v 165,raw48,Not_In_Use "
    "-v 166,raw48,Minimum_PE_Cycles_TLC "
    "-v 167,raw48,Not_In_Use "
    "-v 168,raw48,Maximum_PE_Cycles_TLC "
    "-v 231,raw48,SSD_Life_Left "
    "-v 233,raw48,NAND_Writes_1GiB "
    "-v 241,raw48,Lifetime_Writes_GiB "
    "-v 242,raw48,Lifetime_Reads_GiB "
  },
  { "Silicon Motion based OEM SSDs", // Like 'Silicon Motion based SSDs' but with FW detection
    "240GB|" // from Lenovo T430 Thinkpad, tested with 240GB/P0510E
    "Dogfish SSD (128|256|512)GB|" // tested with Dogfish SSD 128GB/S1211A0
    "GIM(16|32|64|128|256|512)|"// GUDGA GIM, tested with GIM128/U0401A0
    "INTENSO( SSD)?|" // tested with INTENSO/S1211A0 (Portable SSD 256GB premium edition),
      // INTENSO/V0609A0, INTENSO SSD/V0823A0, INTENSO/V0718B0, INTENSO SSD/W0413A0, INTENSO SSD/W0714A0,
    "Intenso  ?SSD( S(ata|ATA) ?III)?|" // tested with Intenso SSD/Q1107A0, Intenso  SSD Sata III/P0510E,
      // Intenso SSD Sata III/R0817B0, Intenso SSD Sata III/S0222A0, Intenso SSD Sata III/V0303B0,
      // Intenso SSD SATAIII/W0825A0,
    "KingFast|" // tested with KingFast/P0725A (F6M), KingFast/S0424A0 (120GB), KingFast/S1128B0 (512GB)
    "KSM512|" // KingSpec, tested with KSM512/S0509A0
    "LDLC|" // tested with LDLC/KFS03005
    "Netac MobileDataStar|" // tested with Netac MobileDataStar/HPS2227I (0x0dd8:0x0562)
    "ORICO|" // ORICO S500PRO, tested with ORICO/W0201A0 (2TB)
    "ORTIAL SSD|" // tested with ORTIAL SSD/U0202A0 (128GB)
    "RX7 (240|256|512)G|" // tested with RX7 240G/T0910A0
    "SATA3 ((12[08]|240|256|480)G|[12]T)B SSD|" // TCSUNBOW X3, tested with SATA3 240GB SSD/S0618A0,
      // SATA3 1TB SSD/S1230A0,
      // KingDian S370, tested with SATA3 128GB SSD/T0311A0, SATA3 256GB SSD/S1127B0
      // KingDian S280, tested with SATA3 240GB SSD/T0519A0
    "SPCC M\\.2 SSD|" // Silicon Power A/M55, tested with SPCC M.2 SSD/Q0627A0, SPCC M.2 SSD/U0506A0,
      // SPCC M.2 SSD/U1209A0
    "SSD 120GB|" // Intenso M.2 SSD High, tested with SSD 120GB/R0529A
    "T-FORCE (128|256|512)GB|" // tested with T-FORCE 512GB/T0910A0
    "Verbatim Vi550 S3|" // tested with Verbatim Vi550 S3/U1124A0 (128GB),
       // may also exist with different controllers (tickets #1626, #1629, #1774, #1930, GH issues/185),
    "Vi550 S3", // another variant (ticket #1899), tested with Vi550 S3/HP3418C5
    "HP(3418C5|S2227I)|KFS03005|P0510E|P0725A|Q(0627|1107)A0|R(0529A|0817B0)|"
    "S(0222|0424|0509|0618|1211|1230)A0|S112[78]B0|T0(311|519|910)A0|"
    "U(0202|0401|0506|1124|1209)A0|V0((609|823)A|(303|718)B)0|V1027A0|"
    "W(0201|0413|0714|0825)A0",
    "",
    "-v 148,raw48,Total_SLC_Erase_Ct "
    "-v 149,raw48,Max_SLC_Erase_Ct "
    "-v 150,raw48,Min_SLC_Erase_Ct "
    "-v 151,raw48,Average_SLC_Erase_Ct "
    "-v 159,raw48,Unkn_SiliconMotion_Attr "
    "-v 160,raw48,Uncorrectable_Error_Cnt "
    "-v 161,raw48,Valid_Spare_Block_Cnt "
    "-v 163,raw48,Initial_Bad_Block_Count "
    "-v 164,raw48,Total_Erase_Count "
    "-v 165,raw48,Max_Erase_Count "
    "-v 166,raw48,Min_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 168,raw48,Max_Erase_Count_of_Spec "
    "-v 169,raw48,Remaining_Lifetime_Perc "
    "-v 178,raw48,Runtime_Invalid_Blk_Cnt "
    "-v 225,raw48,Host_Writes_32MiB "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 245,raw48,TLC_Writes_32MiB "
    "-v 246,raw48,SLC_Writes_32MiB "
    "-v 247,raw48,Raid_Recoverty_Ct "
    "-v 248,raw48,Unkn_SiliconMotion_Attr "
    "-v 251,raw48,Unkn_SiliconMotion_Attr"
  },
  { "SMART Modular Technologies mSATA XL+ SLC SSDs", // tested with SH9MST6D16GJSI01
    "SH9MST6D[0-9]*GJSI?[0-9]*",
    "", "", // attributes info from https://www.mouser.com/ds/2/723/smartmodular_09302015_SH9MST6DxxxGJSxxx_rA[1]-770719.pdf
    "-v 1,raw48,Uncorrectable_ECC_Cnt "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
    "-v 9,raw48,Power_On_Hours " // override default raw24(raw8) format
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 14,raw48,Device_Capacity_LBAs "
    "-v 15,raw48,User_Capacity_LBAs " // spec DecID is wrong, HexID is right
    "-v 16,raw48,Init_Spare_Blocks_Avail " // spec DecID is wrong, HexID is right
    "-v 17,raw48,Spare_Blocks_Remaining " // spec DecID is wrong, HexID is right
    "-v 100,raw48,Total_Erase_Count "
    "-v 168,raw48,SATA_PHY_Err_Ct "
    "-v 170,raw48,Initial_Bad_Block_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Max_Erase_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 175,raw48,Average_Erase_Count "
  //"-v 181,raw48,Program_Fail_Cnt_Total "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 197,raw48,Not_In_Use "
    "-v 198,raw48,Not_In_Use "
    "-v 199,raw48,SATA_CRC_Error_Count "
    "-v 202,raw48,Perc_Rated_Life_Used "
    "-v 231,raw48,Perc_Rated_Life_Remain "
    "-v 232,raw48,Read_Fail_Count "
    "-v 234,raw48,Flash_Reads_LBAs "
    "-v 235,raw48,Flash_Writes_LBAs "
  //"-v 241,raw48,Total_LBAs_Written "
  //"-v 242,raw48,Total_LBAs_Read "
    //  247-248 Missing in specification from April 2015
  },
  { "Smart Storage Systems Xcel-10 SSDs",
    "SMART A25FD-(32|64|128)GI32N", // tested with SMART A25FD-128GI32N/B9F23D4K
    "", "",
    "-v 1,raw48,Not_Supported "
    "-v 2,raw48,Not_Supported "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 191,raw48,Not_Supported "
  //"-v 192,raw48,Power-Off_Retract_Count "
    "-v 197,raw48,ECC_Error_Count "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 251,raw48,Min_Spares_Remain_Perc " // percentage of the total number of spare blocks available
    "-v 252,raw48,Added_Bad_Flash_Blk_Ct " // number of bad flash blocks
    "-v 254,raw48,Total_Erase_Blocks_Ct" // number of times the drive has erased any erase block
  },
  { "Smart Storage Systems XceedSecure2 SSDs",
    "(SMART|Adtron) ([AIS]25FBS|S35FCS).*",
    "", "",
    "-v 9,sec2hour,Power_On_Hours "
    "-v 194,hex64,Proprietary_194"
  },
  { "Smart Storage Systems XceedUltraX/Adtron A25FBX SSDs",
    "(SMART|Adtron) (A|I)25FBX.*",
    "", "",
    "-v 9,hex64,Proprietary_9 "
    "-v 194,hex48,Proprietary_194"
  },
  { "Smart Storage Systems Adtron A25FB 2xN SSDs",
    "(SMART|Adtron) A25FB.*2.N",
    "", "",
    "-v 110,hex64,Proprietary_HWC "
    "-v 111,hex64,Proprietary_MP "
    "-v 112,hex64,Proprietary_RtR "
    "-v 113,hex64,Proprietary_RR "
    "-v 120,hex64,Proprietary_HFAll "
    "-v 121,hex64,Proprietary_HF1st "
    "-v 122,hex64,Proprietary_HF2nd "
    "-v 123,hex64,Proprietary_HF3rd "
    "-v 125,hex64,Proprietary_SFAll "
    "-v 126,hex64,Proprietary_SF1st "
    "-v 127,hex64,Proprietary_SF2nd "
    "-v 128,hex64,Proprietary_SF3rd "
    "-v 194,raw24/raw32:zvzzzw,Fractional_Temperature"
  },
  { "Smart Storage Systems Adtron A25FB 3xN SSDs",
    "(SMART|Adtron) A25FB-.*3.N",
    "", "",
    "-v 9,sec2hour,Power_On_Hours "
    "-v 113,hex48,Proprietary_RR "
    "-v 130,raw48:54321,Minimum_Spares_All_Zs"
  //"-v 194,tempminmax,Temperature_Celsius"
  },
  { "SSSTC ERX GD/CD Series SSDs", // Marvel DEAN 2.1
    "(SSSTC|SATA) ER[2-9]-[CG]D(240|480|960|1920|3840|7680|15360)A?|" // tested with
      // SSSTC ER3-GD240/F2MRD0F, SSSTC ER2-GD480/E4N23021, SSSTC ER3-CD960A/F3MRD0Y,
      // SSSTC ER2-CD1920A/E5MN401, SSSTC ER4-CD7680A/G62RD14
    "AF[2-9]MA31DT[ED]LT(240|480|960|1920|3840|7680|15360)A?", // tested with
      // AF2MA31DTDLT240A/F2M96T0, AF3MA31DTELT240A/F2M9601
    "","",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 100,raw48,Max_Min_EC_Count "
    "-v 170,raw48,Available_Reservd_Space "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Average_PE_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 175,raw48,PLP_Failure "
  //"-v 176,raw48,Erase_Fail_Count_Chip "
  //"-v 177,raw48,Wear_Leveling_Count "
  //"-v 178,raw48,Used_Rsvd_Blk_Cnt_Chip "
  //"-v 179,raw48,Used_Rsvd_Blk_Cnt_Tot "
    "-v 180,raw48,Over-Provisioning_Rate "
    "-v 181,raw48,Sys_Percent_Life_Remain "
    "-v 182,raw48,Heavy_GC_Log "
    "-v 183,raw48,SATA_Iface_Downshift "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 188,raw48,Command_Timeout "
    "-v 189,raw48,Maximum_Erase_Count "
  //"-v 190,tempminmax,Airflow_Temperature_Cel "
    "-v 191,raw48,Mininum_Erase_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 202,raw48,Percent_Lifetime_Remain "
    "-v 210,raw48,Raid_Success_Recover_Ct "
    "-v 229,raw48,PLP_Failure "
    "-v 231,raw48,Percent_Lifetime_Remain "
  //"-v 232,raw48,Available_Reservd_Space "
    "-v 233,raw48,Percent_Lifetime_Remain "
    "-v 234,raw48,Thermal_Throttle_Status "
  //"-v 241,raw48,Total_LBAs_Written "
  //"-v 242,raw48,Total_LBAs_Read "
    "-v 243,raw48,Total_NAND_Written " // GiB?
    "-v 244,raw48,SoC_Data_Path_Prot_Det "
    "-v 245,raw48,Thermal_Sensor_Health "
    "-v 246,raw48,Heavy_Read_Retry_count "
    "-v 247,raw48,NOR_Health "
    "-v 248,raw48,Cross_Temp_Duration "
    "-v 249,raw48,SSD_Health"
  },
  { "STEC Mach2 CompactFlash Cards", // tested with STEC M2P CF 1.0.0/K1385MS
    "STEC M2P CF 1.0.0",
    "", "",
    "-v 100,raw48,Erase_Program_Cycles "
    "-v 103,raw48,Remaining_Energy_Storg "
    "-v 170,raw48,Reserved_Block_Count "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Wear_Leveling_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 211,raw48,Unknown_Attribute " // ] Missing in specification
    "-v 212,raw48,Unknown_Attribute"  // ] from September 2012
  },
  { "Transcend CompactFlash Cards", // tested with TRANSCEND/20080820,
      // TS4GCF133/20100709, TS16GCF133/20100709, TS16GCF150/20110407
    "TRANSCEND|TS(4|8|16)GCF(133|150)",
    "", "",
    "-v 7,raw48,Unknown_Attribute "
    "-v 8,raw48,Unknown_Attribute"
  },
  { "XITC SSDs", // tested with XITC SS6000SES327-7680G/F6600002, XITC SS6000SES3N6-240GB/F6600002,
      // XITC SS6000SES327-3840G/F6600002, XITC SS6000SES327-1920G/F6600002
    "XITC SS6000SES3(27|N6)-(24|48|96|192|384|768)0GB?",
    "","",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 160,raw48,Uncorrectable_Error_Cnt "
    "-v 161,raw48,Number_of_Pure_Spare "
    "-v 163,raw48,Initial_Bad_Block_Count "
    "-v 164,raw48,Total_Erase_Count "
    "-v 165,raw48,Max_Erase_Count "
    "-v 166,raw48,Min_Erase_Count "
    "-v 167,raw48,Average_Erase_Count "
    "-v 170,raw48,Grown_Failing_Block_Ct "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 175,raw16,Capacitor_Life "
  //"-v 177,raw48,Wear_Leveling_Count "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw8,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 197,raw48,Current_Pending_Sector "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 202,raw48,Available_Reservd_Space "
    "-v 232,raw48,Percent_Life_Used "
    "-v 233,raw48,Flash_Writes_32MiB "
    "-v 234,raw48,Flash_Reads_32MiB "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB "
    "-v 250,raw16,SATA_Downshift_Cnt "
  },
  { "Xmore Industrial SATA SSDs", // tested with M2CA032GXAIMS-003Z/XP01.1GB
    "(CFAST|M2[AC]A|MSATA|SSD)[0-9]{3}[GT]XA[CEI][MT][MST]-[0-9]{3}[TZ]",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 168,raw48,SATA_Phy_Error_Count "
    "-v 169,raw48,Bad_Block_Rate "
    "-v 170,raw24/raw24:z54z10,Bad_Blk_Ct_Lat/Erl " // Later bad block/Early bad block
    "-v 173,raw16(avg16),MaxAvgErase_Ct "
    "-v 192,raw48,Unexpect_Power_Loss_Ct "
  //"-v 194,tempminmax,Temperature_Celsius " // optional
    "-v 218,raw48,SATA_CRC_Error_Count "
    "-v 231,raw48,Percent_Lifetime_Remain "
    "-v 241,raw48,Host_Writes_GiB"
  },
  { "Marvell SSD SD88SA024BA0 (SUN branded)",
    "MARVELL SD88SA024BA0 SUN24G 0902M0054V",
    "", "", ""
  },
  { "HP 1TB SATA disk GB1000EAFJL",
    "GB1000EAFJL",
    "", "", ""
  },
  { "HP 500GB SATA disk MM0500EANCR",
    "MM0500EANCR",
    "", "", ""
  },
  { "HP 250GB SATA disk VB0250EAVER",
    "VB0250EAVER",
    "", "", ""
  },
  { "IBM Deskstar 60GXP",  // ER60A46A firmware
    "(IBM-|Hitachi )?IC35L0[12346]0AVER07.*",
    "ER60A46A",
    "", ""
  },
  { "IBM Deskstar 60GXP",  // All other firmware
    "(IBM-|Hitachi )?IC35L0[12346]0AVER07.*",
    "",
    "IBM Deskstar 60GXP drives may need upgraded SMART firmware.\n"
    "Please see https://haque.net/dtla_update/",
    ""
  },
  { "IBM Deskstar 40GV & 75GXP (A5AA/A6AA firmware)",
    "(IBM-)?DTLA-30[57]0[123467][05].*",
    "T[WX][123468AG][OF]A[56]AA",
    "", ""
  },
  { "IBM Deskstar 40GV & 75GXP (all other firmware)",
    "(IBM-)?DTLA-30[57]0[123467][05].*",
    "",
    "IBM Deskstar 40GV and 75GXP drives may need upgraded SMART firmware.\n"
    "Please see https://haque.net/dtla_update/",
    ""
  },
  { "", // ExcelStor J240, J340, J360, J680, J880 and J8160
    "ExcelStor Technology J(24|34|36|68|88|816)0",
    "", "", ""
  },
  { "", // Fujitsu M1623TAU
    "FUJITSU M1623TAU",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MHG",
    "FUJITSU MHG2...ATU?.*",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MHH",
    "FUJITSU MHH2...ATU?.*",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MHJ",
    "FUJITSU MHJ2...ATU?.*",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MHK",
    "FUJITSU MHK2...ATU?.*",
    "",
    "",
    "-v 9,seconds"
  },
  { "",  // Fujitsu MHL2300AT
    "FUJITSU MHL2300AT",
    "",
    "This drive's firmware has a harmless Drive Identity Structure\n"
    "checksum error bug.",
    "-v 9,seconds"
  },
  { "",  // MHM2200AT, MHM2150AT, MHM2100AT, MHM2060AT
    "FUJITSU MHM2(20|15|10|06)0AT",
    "",
    "This drive's firmware has a harmless Drive Identity Structure\n"
    "checksum error bug.",
    "-v 9,seconds"
  },
  { "Fujitsu MHN",
    "FUJITSU MHN2...AT",
    "",
    "",
    "-v 9,seconds"
  },
  { "", // Fujitsu MHR2020AT
    "FUJITSU MHR2020AT",
    "",
    "",
    "-v 9,seconds"
  },
  { "", // Fujitsu MHR2040AT
    "FUJITSU MHR2040AT",
    "",    // Tested on 40BA
    "",
    "-v 9,seconds -v 192,emergencyretractcyclect "
    "-v 198,offlinescanuncsectorct -v 200,writeerrorcount"
  },
  { "Fujitsu MHS AT",
    "FUJITSU MHS20[6432]0AT(  .)?",
    "",
    "",
    "-v 9,seconds -v 192,emergencyretractcyclect "
    "-v 198,offlinescanuncsectorct -v 200,writeerrorcount "
    "-v 201,detectedtacount"
  },
  { "Fujitsu MHT", // tested with FUJITSU MHT2030AC/909B
    "FUJITSU MHT2...(AC|AH|AS|AT|BH)U?.*",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MHU",
    "FUJITSU MHU2...ATU?.*",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MHV",
    "FUJITSU MHV2...(AH|AS|AT|BH|BS|BT).*",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MPA..MPG",
    "FUJITSU MP[A-G]3...A[HTEV]U?.*",
    "",
    "",
    "-v 9,seconds"
  },
  { "Fujitsu MHY BH",
    "FUJITSU MHY2(04|06|08|10|12|16|20|25)0BH.*",
    "", "",
    "-v 240,raw48,Transfer_Error_Rate"
  },
  { "Fujitsu MHW AC", // tested with FUJITSU MHW2060AC/00900004
    "FUJITSU MHW20(40|60)AC",
    "", "", ""
  },
  { "Fujitsu MHW BH",
    "FUJITSU MHW2(04|06|08|10|12|16)0BH.*",
    "", "", ""
  },
  { "Fujitsu MHW BJ",
    "FUJITSU MHW2(08|12|16)0BJ.*",
    "", "", ""
  },
  { "Fujitsu MHZ BH",
    "FUJITSU MHZ2(04|08|12|16|20|25|32)0BH.*",
    "", "", ""
  },
  { "Fujitsu MHZ BJ",
    "FUJITSU MHZ2(08|12|16|20|25|32)0BJ.*",
    "",
    "",
    "-v 9,minutes"
  },
  { "Fujitsu MHZ BS",
    "FUJITSU MHZ2(12|25)0BS.*",
    "", "", ""
  },
  { "Fujitsu MHZ BK",
    "FUJITSU MHZ2(08|12|16|25)0BK.*",
    "", "", ""
  },
  { "Fujitsu MJA BH",
    "FUJITSU MJA2(08|12|16|25|32|40|50)0BH.*",
    "", "", ""
  },
  { "", // Samsung SV4012H (known firmware)
    "SAMSUNG SV4012H",
    "RM100-08",
    "",
    "-v 9,halfminutes -F samsung"
  },
  { "", // Samsung SV4012H (all other firmware)
    "SAMSUNG SV4012H",
    "",
    "May need -F samsung disabled; see manual for details.",
    "-v 9,halfminutes -F samsung"
  },
  { "", // Samsung SV0412H (known firmware)
    "SAMSUNG SV0412H",
    "SK100-01",
    "",
    "-v 9,halfminutes -v 194,10xCelsius -F samsung"
  },
  { "", // Samsung SV0412H (all other firmware)
    "SAMSUNG SV0412H",
    "",
    "May need -F samsung disabled; see manual for details.",
    "-v 9,halfminutes -v 194,10xCelsius -F samsung"
  },
  { "", // Samsung SV1204H (known firmware)
    "SAMSUNG SV1204H",
    "RK100-1[3-5]",
    "",
    "-v 9,halfminutes -v 194,10xCelsius -F samsung"
  },
  { "", // Samsung SV1204H (all other firmware)
    "SAMSUNG SV1204H",
    "",
    "May need -F samsung disabled; see manual for details.",
    "-v 9,halfminutes -v 194,10xCelsius -F samsung"
  },
  { "", // SAMSUNG SV0322A tested with FW JK200-35
    "SAMSUNG SV0322A",
    "", "", ""
  },
  { "SAMSUNG SpinPoint V80", // tested with SV1604N/TR100-23
    "SAMSUNG SV(0211|0401|0612|0802|1203|1604)N",
    "",
    "",
    "-v 9,halfminutes -F samsung2"
  },
  { "", // SAMSUNG SP40A2H with RR100-07 firmware
    "SAMSUNG SP40A2H",
    "RR100-07",
    "",
    "-v 9,halfminutes -F samsung"
  },
  { "", // SAMSUNG SP80A4H with RT100-06 firmware
    "SAMSUNG SP80A4H",
    "RT100-06",
    "",
    "-v 9,halfminutes -F samsung"
  },
  { "", // SAMSUNG SP8004H with QW100-61 firmware
    "SAMSUNG SP8004H",
    "QW100-61",
    "",
    "-v 9,halfminutes -F samsung"
  },
  { "SAMSUNG SpinPoint F1 DT", // tested with HD103UJ/1AA01113
    "SAMSUNG HD(083G|16[12]G|25[12]H|32[12]H|50[12]I|642J|75[23]L|10[23]U)J",
    "", "", ""
  },
  { "SAMSUNG SpinPoint F1 EG", // tested with HD103UI/1AA01113
    "SAMSUNG HD(252H|322H|502I|642J|753L|103U)I",
    "", "", ""
  },
  { "SAMSUNG SpinPoint F1 RE", // tested with HE103UJ/1AA01113
    "SAMSUNG HE(252H|322H|502I|642J|753L|103U)J",
    "", "", ""
  },
  { "SAMSUNG SpinPoint F2 EG", // tested with HD154UI/1AG01118
    "SAMSUNG HD(502H|10[23]S|15[34]U)I",
    "", "", ""
  },
  { "SAMSUNG SpinPoint F3", // tested with HD502HJ/1AJ100E4
    "SAMSUNG HD(502H|754J|103S)J",
    "", "", ""
  },
  { "Seagate Barracuda SpinPoint F3", // tested with ST1000DM005 HD103SJ/1AJ100E5
    "ST[0-9DM]* HD(502H|754J|103S)J",
    "", "", ""
  },
  { "SAMSUNG SpinPoint F3 EG", // tested with HD503HI/1AJ100E4, HD153WI/1AN10002
    "SAMSUNG HD(253G|(324|503)H|754J|105S|(153|203)W)I",
    "", "", ""
  },
  { "SAMSUNG SpinPoint F3 RE", // tested with HE103SJ/1AJ30001
    "SAMSUNG HE(502H|754J|103S)J",
    "", "", ""
  },
  { "Seagate Samsung Spinpoint F4", // tested with ST250DM001 HD256GJ/1AR10001
    "ST(250|320)DM001 HD(256G|322G|323H)J",
    "", "", ""
  },
  { "SAMSUNG SpinPoint F4 EG (AF)",// tested with HD204UI/1AQ10001(buggy|fixed)
    "SAMSUNG HD(155|204)UI",
    "", // 1AQ10001
    "Using smartmontools or hdparm with this\n"
    "drive may result in data loss due to a firmware bug.\n"
    "****** THIS DRIVE MAY OR MAY NOT BE AFFECTED! ******\n"
    "Buggy and fixed firmware report same version number!\n"
    "See the following web page for details:\n"
    "https://www.smartmontools.org/wiki/SamsungF4EGBadBlocks",
    ""
  },
  { "Seagate Samsung SpinPoint F4 EG (AF)", // later sold as Barracuda Green,
      // tested with ST2000DL004 HD204UI/1AQ10001
    "ST2000DL004 HD204UI",
    "", "", ""
  },
  { "SAMSUNG SpinPoint S250", // tested with HD200HJ/KF100-06
    "SAMSUNG HD(162|200|250)HJ",
    "", "", ""
  },
  { "SAMSUNG SpinPoint T133", // tested with HD300LJ/ZT100-12, HD400LJ/ZZ100-14, HD401LJ/ZZ100-15
    "SAMSUNG HD(250KD|(30[01]|320|40[01])L[DJ])",
    "", "", ""
  },
  { "SAMSUNG SpinPoint T166", // tested with HD252KJ/CM100-11, HD501LJ/CR100-1[01]
    "SAMSUNG HD(080G|160H|252K|32[01]K|403L|50[01]L)J",
    "", "",
    "-v 197,increasing" // at least HD501LJ/CR100-11
  },
  { "SAMSUNG SpinPoint P120", // VF100-37 firmware, tested with SP2514N/VF100-37
    "SAMSUNG SP(16[01]3|2[05][01]4)[CN]",
    "VF100-37",
    "",
    "-F samsung3"
  },
  { "SAMSUNG SpinPoint P120", // other firmware, tested with SP2504C/VT100-33
    "SAMSUNG SP(16[01]3|2[05][01]4)[CN]",
    "",
    "May need -F samsung3 enabled; see manual for details.",
    ""
  },
  { "SAMSUNG SpinPoint P80 SD", // tested with HD160JJ/ZM100-33, SAMSUNG HD080HJ/P/ZH100-34
    "SAMSUNG HD(080H|120I|160J)J(/P)?",
    "", "", ""
  },
  { "SAMSUNG SpinPoint P80", // BH100-35 firmware, tested with SP0842N/BH100-35
    "SAMSUNG SP(0451|08[0124]2|12[0145]3|16[0145]4)[CN]",
    "BH100-35",
    "",
    "-F samsung3"
  },
  { "SAMSUNG SpinPoint P80", // firmware *-35 or later
    "SAMSUNG SP(0451|08[0124]2|12[0145]3|16[0145]4)[CN]",
    ".*-3[5-9]",
    "May need -F samsung3 enabled; see manual for details.",
    ""
  },
  { "SAMSUNG SpinPoint P80", // firmware *-25...34, tested with
      // SP0401N/TJ100-30, SP1614C/SW100-25 and -34
    "SAMSUNG SP(04[05]1|08[0124]2|12[0145]3|16[0145]4)[CN]",
    ".*-(2[5-9]|3[0-4])",
    "",
    "-v 9,halfminutes -v 198,increasing"
  },
  { "SAMSUNG SpinPoint P80", // firmware *-23...24, tested with
    // SP0802N/TK100-23,
    // SP1213N/TL100-23,
    // SP1604N/TM100-23 and -24
    "SAMSUNG SP(0451|08[0124]2|12[0145]3|16[0145]4)[CN]",
    ".*-2[34]",
    "",
    "-v 9,halfminutes -F samsung2"
  },
  { "SAMSUNG SpinPoint P80", // unknown firmware
    "SAMSUNG SP(0451|08[0124]2|12[0145]3|16[0145]4)[CN]",
    "",
    "May need -F samsung2 or -F samsung3 enabled; see manual for details.",
    ""
  },
  { "SAMSUNG SpinPoint M40/60/80", // tested with HM120IC/AN100-16, HM160JI/AD100-16
    "SAMSUNG HM(0[468]0H|120I|1[026]0J)[CI]",
    "",
    "",
    "-v 9,halfminutes"
  },
  { "SAMSUNG SpinPoint M5", // tested with HM160HI/HH100-12
    "SAMSUNG HM(((061|080)G|(121|160)H|250J)I|160HC)",
    "", "", ""
  },
  { "SAMSUNG SpinPoint M6", // tested with HM320JI/2SS00_01 M6
    "SAMSUNG HM(251J|320[HJ]|[45]00L)I",
    "", "", ""
  },
  { "SAMSUNG SpinPoint M7", // tested with HM500JI/2AC101C4
    "SAMSUNG HM(250H|320I|[45]00J)I",
    "", "", ""
  },
  { "SAMSUNG SpinPoint M7E (AF)", // tested with HM321HI/2AJ10001, HM641JI/2AJ10001
    "SAMSUNG HM(161G|(251|321)H|501I|641J)I",
    "", "", ""
  },
  { "Seagate Samsung SpinPoint M7E", // tested with ST640LM000 HM641JI/2AJ10001
    "ST(160|250|320|500|640)LM00[01] HM[0-9]*[GHIJ]I",
    "", "", ""
  },
  { "SAMSUNG SpinPoint M7U (USB)", // tested with HM252HX/2AC101C4
    "SAMSUNG HM(162H|252H|322I|502J)X",
    "", "", ""
  },
  { "SAMSUNG SpinPoint M8 (AF)", // tested with HN-M101MBB/2AR10001
    "SAMSUNG HN-M(250|320|500|640|750|101)MBB",
    "", "", ""
  },
  { "Seagate Samsung SpinPoint M8 (AF)", // tested with
      // ST750LM022 HN-M750MBB/2AR10001, ST320LM001 HN-M320MBB/2AR10002,
      // APPLE HDD ST500LM012/2BA30003
    "ST(250|320|500|640|750|1000)LM0[012][124] HN-M[0-9]*MBB|"
    "APPLE HDD ST500LM012",
    "", "", ""
  },
  { "SAMSUNG SpinPoint M8U (USB)", // tested with HN-M500XBB/2AR10001
    "SAMSUNG HN-M(320|500|750|101)XBB",
    "", "", ""
  },
  { "Seagate Samsung SpinPoint M8U (USB)", // tested with ST1000LM025 HN-M101ABB/2AR10001,
      // ST1000LM025 HN-M101ABB/2BA30003 (0x04e8:0x61b6)
    "ST(250|320|500|640|750|1000)LM0[012][3459] HN-M[0-9]*ABB",
    "", "", ""
  },
  { "Seagate Samsung SpinPoint M9T", // tested with ST2000LM003 HN-M201RAD/2BC10003
      // (Seagate Expansion Portable)
    "ST(1500|2000)LM0(03|04|06|07|10) HN-M[0-9]*RAD",
    "", "", ""
  },
  { "Seagate Mobile HDD", // tested with ST1000LM035-1RK172/ACM1,
     // ST1000LM035-1RK172/ACM2, ST1000LM035-1RK172/EB01 (0x1005:0xc004),
     // ST2000LM007-1R8174/SBK2
    "ST(2000LM0(07|09|10)|1000LM03[578])-.*",
    "", "", ""
  },
  // Flash accelerated, no SMART info in the specs
  // ST1000LX015-1U7172/SDM1
  { "Seagate FireCuda 2.5",
    "ST(500|1000|2000)LX0(01|15|25)-.*",
    "", "", "-v 240,msec24hour32 "
  },
  { "Seagate FireCuda 3.5", // ST2000DX002-2DV164/CC41
    "ST[12]000DX002-.*",
    "", "", "-v 240,msec24hour32 "
  },
  { "Seagate Samsung SpinPoint M9TU (USB)", // tested with ST1500LM008 HN-M151AAD/2BC10001
      // (0x04e8:0x61b5), ST2000LM005 HN-M201AAD2BC10001 (0x04e8:0x61b4)
    "ST(1500|2000)LM00[58] HN-M[0-9]*AAD",
    "", "", ""
  },
  { "Seagate FreePlay", // tested with ST1500LM003-9YH148/CC94
    // from FreeAgent GoFlex Enclosure.
    "ST(1500LM003|1000LM010|1000LM002)-.*",
    "", "", ""
  },
  { "SAMSUNG SpinPoint MP5", // tested with HM250HJ/2AK10001
    "SAMSUNG HM(250H|320H|500J|640J)J",
    "", "", ""
  },
  { "SAMSUNG SpinPoint MT2", // tested with HM100UI/2AM10001
    "SAMSUNG HM100UI",
    "", "", ""
  },
  { "SAMSUNG HM100UX (S2 Portable)", // tested with HM100UX/2AM10001
    "SAMSUNG HM100UX",
    "", "", ""
  },
  { "SAMSUNG SpinPoint M", // tested with MP0402H/UC100-11
    "SAMSUNG MP0(302|402|603|804)H",
    "",
    "",
    "-v 9,halfminutes"
  },
  { "SAMSUNG SpinPoint N3U-3 (USB)", // tested with
      // SAMSUNG HS25YJZ/3AU10-01 (0x18a5:0x0227, reports 4KiB LPS/LLS. ticket #159),
      // SAMSUNG HS20YJZ/3AU10-01 (0x04e8:0x2f06, reports 512B sectors, Debian Bug 964032)
    "SAMSUNG HS(122H|2[05]YJ)Z",
    "", "", ""
  },
  { "SK hynix SATA SSDs",
    "SK ?hynix (SC(210|300|308|311|313|401)|SH920) .*|" // tested with
      // SK hynix SC210 mSATA 256GB/20002L00,
      // SKhynix SC300 HFS256G32MND-3210A/20131P00,
      // SK hynix SC308 SATA 256GB/30000P10,
      // SK hynix SC308 SATA 128GB/30001P10,
      // SK hynix SC311 SATA 512GB/70000P10,
      // SK hynix SC313 HFS256G32TNF-N3A0A/70000P10,
      // SK hynix SC401 SATA 512GB/90000121,
      // SK hynix SH920 mSATA 256GB/1010BL00
    "HFS(128|256|512)G3[29A]MN[BD]-(2200|3[23]10)A|" // SC210, tested with
      // HFS128G32MND-2200A/20200L00, HFS512G32MND-3210A/20100P00,
      // HFS512G39MND-3310A/20002P00, HFS256G3AMNB-2200A/1010BL00
    "HFS(128|256|512)G3[29]MND-3(312|510)A|" // SC300, tested with HFS256G32MND-3312A/20001P00,
      // HFS512G39MND-3510A/20400P00
    "HFS(128|256|512)G39TND-N210A|" // SC308, tested with HFS128G39TND-N210A/30001P10
    "HFS(120|250|500)G32TND-N1A2A|" // SL308, tested with HFS500G32TND-N1A2A/30000P10
    "HFS(128|256|512)G32TNF-N3A0A|" // SC313, tested with HFS256G32TNF-N3A0A/70000P10
    // HFS480G32FEH-BA10A/DD02 (Dell)
    "SHGS31-(250|500|1000)GS-2", // S31, tested with SHGS31-1000GS-2/90000Q00
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
    "-v 5,raw48,Retired_Block_Count "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 100,raw48,Total_Erase_Count "
    "-v 168,raw48,Min_Erase_Count "
    "-v 169,raw48,Max_Erase_Count "
    "-v 170,raw48,Unknown_SK_hynix_Attrib "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Wear_Leveling_Count "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
  //"-v 175,raw48,Program_Fail_Count_Chip "
    "-v 176,raw48,Unused_Rsvd_Blk_Cnt_Tot "
  //"-v 177,raw48,Wear_Leveling_Count "
  //"-v 178,raw48,Used_Rsvd_Blk_Cnt_Chip "
  //"-v 179,raw48,Used_Rsvd_Blk_Cnt_Tot "
    "-v 180,raw48,Erase_Fail_Count "
    "-v 181,raw48,Non4k_Aligned_Access "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 188,raw48,Command_Timeout "
    "-v 191,raw48,Unknown_SK_hynix_Attrib " // SC210
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 195,raw48,Hardware_ECC_Recovered "
  //"-v 196,raw16(raw16),Reallocated_Event_Count "
  //"-v 198,raw48,Offline_Uncorrectable "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 201,raw48,Percent_Lifetime_Remain "
  //"-v 204,raw48,Soft_ECC_Correction "
    "-v 212,raw48,Phy_Error_Count "
    "-v 231,raw48,SSD_Life_Left "
    "-v 234,raw48,Unknown_SK_hynix_Attrib "
    "-v 236,raw48,Unknown_SK_hynix_Attrib " // SC311, SC313
    "-v 238,raw48,Unknown_SK_hynix_Attrib " // SC401
    "-v 241,raw48,Total_Writes_GB " // SC31: ~GB, not GiB (#1517)
    "-v 242,raw48,Total_Reads_GB "
    "-v 243,raw48,Total_Media_Writes "
    "-v 249,raw48,NAND_Writes_GiB " // SC311, SC313
    "-v 250,raw48,Read_Retry_Count "
  },
  { "SK hynix SATA SSDs",
    "HFS(480|960|1T9|3T8)G3[2E]FEH-[7B][4A]10A|" // tested with HFS480G32FEH-7410A/90037Q00,
      // HFS480G32FEH-BA10A/DD02 (Dell), HFS1T9G32FEH-BA10A/DD02 (Dell)
    "HFS(480|960|1T9|3T8)G3H2X069N|" // tested with HFS480G3H2X069N/DZ00 (Dell)
    "SK HYNIX SE5110 (480|960|1920|3840)GB ZIRCON LITE 3DTLC", // tested with
      // SK HYNIX SE5110 480GB ZIRCON LITE 3DTLC/410A5Z00
      // SK HYNIX SE5110 960GB ZIRCON LITE 3DTLC/410A5Z00
      // SK HYNIX SE5110 1920GB ZIRCON LITE 3DTLC/410A5Z00
      // SK HYNIX SE5110 3840GB ZIRCON LITE 3DTLC/410A5Z00
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
    "-v 5,raw48,Retired_Block_Count "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
  //"-v 13,raw48,Read_Soft_Error_Rate "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Max_Erase_Count "
    "-v 174,raw48,Unexpected_Pwr_Loss_Cnt "
    "-v 175,raw48,Program_Fail_Count "
    "-v 176,raw48,Erase_Fail_Count "
    "-v 177,raw48,Endurance_Limit_Met "
    "-v 178,raw48,Used_Rsrvd_Blk_Cnt_Wrst "
    "-v 179,raw48,Used_Rsrvd_Blk_Cnt_Tot "
    "-v 180,raw48,E2E_Error_Det_Corr_Rate "
    "-v 181,raw48,Program_Fail_Count "
    "-v 182,raw48,Erase_Fail_Count "
    "-v 183,raw48,SATA_Downshift_Count "
  //"-v 184,raw48,End-to-End_Error "
  //"-v 187,raw48,Reported_Uncorrect "
  //"-v 188,raw48,Command_Timeout "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw48,ECC_on_the_Fly_Rate "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 201,raw48,Uncorr_Soft_Read_Err_Rt "
    "-v 202,raw48,Exception_Mode_Status "
    "-v 204,raw48,Soft_ECC_Correction_Rt "
    "-v 231,raw48,SSD_Life_Left "
    "-v 234,raw48,Lifetime_NAND_Prg_GiB " // ?
    "-v 235,raw48,Lifetime_Writes_GiB "
    "-v 241,raw48,Lifetime_NAND_Prg_GiB "
    "-v 242,raw48,Lifetime_Reads_GiB "
    "-v 245,raw48,SSD_Life_Left "
    "-v 250,raw48,Read_Retry_Count "
  },
  { "Maxtor Fireball 541DX",
    "Maxtor 2B0(0[468]|1[05]|20)H1",
    "",
    "",
    "-v 9,minutes -v 194,unknown"
  },
  { "Maxtor Fireball 3",
    "Maxtor 2F0[234]0[JL]0",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 1280 ATA",  // no self-test log, ATA2-Fast
    "Maxtor 8(1280A2|2160A4|2560A4|3840A6|4000A6|5120A8)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 2160 Ultra ATA",
    "Maxtor 8(2160D2|3228D3|3240D3|4320D4|6480D6|8400D8|8455D8)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 2880 Ultra ATA",
    "Maxtor 9(0510D4|0576D4|0648D5|0720D5|0840D6|0845D6|0864D6|1008D7|1080D8|1152D8)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 3400 Ultra ATA",
    "Maxtor 9(1(360|350|202)D8|1190D7|10[12]0D6|0840D5|06[48]0D4|0510D3|1(350|202)E8|1010E6|0840E5|0640E4)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax D540X-4G",
    "Maxtor 4G(120J6|160J[68])",
    "",
    "",
    "-v 9,minutes -v 194,unknown"
  },
  { "Maxtor DiamondMax D540X-4K",
    "MAXTOR 4K(020H1|040H2|060H3|080H4)",
    "", "", ""
  },
  { "Maxtor DiamondMax Plus D740X",
    "MAXTOR 6L0(20[JL]1|40[JL]2|60[JL]3|80[JL]4)",
    "", "", ""
  },
  { "Maxtor DiamondMax Plus 5120 Ultra ATA 33",
    "Maxtor 9(0512D2|0680D3|0750D3|0913D4|1024D4|1360D6|1536D6|1792D7|2048D8)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax Plus 6800 Ultra ATA 66",
    "Maxtor 9(2732U8|2390U7|204[09]U6|1707U5|1366U4|1024U3|0845U3|0683U2)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax D540X-4D",
    "Maxtor 4D0(20H1|40H2|60H3|80H4)",
    "",
    "",
    "-v 9,minutes -v 194,unknown"
  },
  { "Maxtor DiamondMax 16",
    "Maxtor 4(R0[68]0[JL]0|R1[26]0L0|A160J0|R120L4)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 4320 Ultra ATA",
    "Maxtor (91728D8|91512D7|91303D6|91080D5|90845D4|90645D3|90648D[34]|90432D2)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 17 VL",
    "Maxtor 9(0431U1|0641U2|0871U2|1301U3|1741U4)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 20 VL",
    "Maxtor (94091U8|93071U6|92561U5|92041U4|91731U4|91531U3|91361U3|91021U2|90841U2|90651U2)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax VL 30",  // U: ATA66, H: ATA100
    "Maxtor (33073U4|32049U3|31536U2|30768U1|33073H4|32305H3|31536H2|30768H1)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 36",
    "Maxtor (93652U8|92739U6|91826U4|91369U3|90913U2|90845U2|90435U1)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 40 ATA 66",
    "Maxtor 9(0684U2|1024U2|1362U3|1536U3|2049U4|2562U5|3073U6|4098U8)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax Plus 40 (Ultra ATA 66 and Ultra ATA 100)",
    "Maxtor (54098[UH]8|53073[UH]6|52732[UH]6|52049[UH]4|51536[UH]3|51369[UH]3|51024[UH]2)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 40 VL Ultra ATA 100",
    "Maxtor 3(1024H1|1535H2|2049H2|3073H3|4098H4)( B)?",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax Plus 45 Ulta ATA 100",
    "Maxtor 5(4610H6|4098H6|3073H4|2049H3|1536H2|1369H2|1023H2)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 60 ATA 66",
    "Maxtor 9(1023U2|1536U2|2049U3|2305U3|3073U4|4610U6|6147U8)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 60 ATA 100",
    "Maxtor 9(1023H2|1536H2|2049H3|2305H3|3073H4|4098H6|4610H6|6147H8)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax Plus 60",
    "Maxtor 5T0(60H6|40H4|30H3|20H2|10H1)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 80",
    "Maxtor (98196H8|96147H6)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 536DX",
    "Maxtor 4W(100H6|080H6|060H4|040H3|030H2)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax Plus 8",
    "Maxtor 6(E0[234]|K04)0L0",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 10 (ATA/133 and SATA/150)",
    "Maxtor 6(B(30|25|20|16|12|10|08)0[MPRS]|L(080[MLP]|(100|120)[MP]|160[MP]|200[MPRS]|250[RS]|300[RS]))0",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 10 (SATA/300)",
    "Maxtor 6V(080E|160E|200E|250F|300F|320F)0",
    "", "", ""
  },
  { "Maxtor DiamondMax Plus 9",
    "Maxtor 6Y((060|080|120|160)L0|(060|080|120|160|200|250)P0|(060|080|120|160|200|250)M0)",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor DiamondMax 11",
    "Maxtor 6H[45]00[FR]0",
    "", "", ""
  },
  { "Maxtor DiamondMax 17",
    "Maxtor 6G(080L|160[PE])0",
    "", "", ""
  },
  { "Seagate Maxtor DiamondMax 20",
    "MAXTOR STM3(40|80|160)[28]1[12]0?AS?",
    "", "", ""
  },
  { "Seagate Maxtor DiamondMax 21", // tested with MAXTOR STM3250310AS/3.AAF
    "MAXTOR STM3(80[28]15|160215|250310|(250|320)820|320620|500630)AS?",
    "", "", ""
  },
  { "Seagate Maxtor DiamondMax 22", // fixed firmware
    "(MAXTOR )?STM3(500320|750330|1000340)AS?",
    "MX1A", // https://knowledge.seagate.com/articles/en_US/FAQ/207969en
    "", ""
  },
  { "Seagate Maxtor DiamondMax 22", // fixed firmware
    "(MAXTOR )?STM3(160813|320614|640323|1000334)AS?",
    "MX1B", // https://knowledge.seagate.com/articles/en_US/FAQ/207975en
    "", ""
  },
  { "Seagate Maxtor DiamondMax 22", // buggy firmware
    "(MAXTOR )?STM3(500320|750330|1000340)AS?",
    "MX15",
    "There are known problems with these drives,\n"
    "AND THIS FIRMWARE VERSION IS AFFECTED,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207969en",
    ""
  },
  { "Seagate Maxtor DiamondMax 22", // unknown firmware
    "(MAXTOR )?STM3(160813|32061[34]|500320|640323|750330|10003(34|40))AS?",
    "",
    "There are known problems with these drives,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207969en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207975en",
    ""
  },
  { "Seagate Maxtor DiamondMax 23", // new firmware
    "STM3((160|250)31|(320|500)41|(750|1000)52)8AS?",
    "CC3[D-Z]",
    "", ""
  },
  { "Seagate Maxtor DiamondMax 23", // unknown firmware
    "STM3((160|250)31|(320|500)41|(750|1000)52)8AS?",
    "",
    "A firmware update for this drive may be available,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/213911en",
    ""
  },
  { "Maxtor MaXLine Plus II",
    "Maxtor 7Y250[PM]0",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor MaXLine II",
    "Maxtor [45]A(25|30|32)0[JN]0",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor MaXLine III (ATA/133 and SATA/150)",
    "Maxtor 7L(25|30)0[SR]0",
    "",
    "",
    "-v 9,minutes"
  },
  { "Maxtor MaXLine III (SATA/300)",
    "Maxtor 7V(25|30)0F0",
    "", "", ""
  },
  { "Maxtor MaXLine Pro 500",  // There is also a 7H500R0 model, but I
    "Maxtor 7H500F0",               // haven't added it because I suspect
    "",                               // it might need vendoropts_9_minutes
    "", ""                            // and nobody has submitted a report yet
  },
  { "", // HITACHI_DK14FA-20B
    "HITACHI_DK14FA-20B",
    "",
    "",
    "-v 9,minutes -v 193,loadunload"
  },
  { "HITACHI Travelstar DK23XX/DK23XXB",
    "HITACHI_DK23..-..B?",
    "",
    "",
    "-v 9,minutes -v 193,loadunload"
  },
  { "Hitachi Endurastar J4K20/N4K20 (formerly DK23FA-20J)",
    "(HITACHI_DK23FA-20J|HTA422020F9AT[JN]0)",
    "",
    "",
    "-v 9,minutes -v 193,loadunload"
  },
  { "Hitachi Endurastar J4K30/N4K30",
    "HE[JN]4230[23]0F9AT00",
    "",
    "",
    "-v 9,minutes -v 193,loadunload"
  },
  { "Hitachi Travelstar C4K60",  // 1.8" slim drive
    "HTC4260[23]0G5CE00|HTC4260[56]0G8CE00",
    "",
    "",
    "-v 9,minutes -v 193,loadunload"
  },
  { "IBM Travelstar 4GT",
    "IBM-DTCA-2(324|409)0",
    "", "", ""
  },
  { "IBM Travelstar 6GN",
    "IBM-DBCA-20(324|486|648)0",
    "", "", ""
  },
  { "IBM Travelstar 25GS, 18GT, and 12GN",
    "IBM-DARA-2(25|18|15|12|09|06)000",
    "", "", ""
  },
  { "IBM Travelstar 14GS",
    "IBM-DCYA-214000",
    "", "", ""
  },
  { "IBM Travelstar 4LP",
    "IBM-DTNA-2(180|216)0",
    "", "", ""
  },
  { "IBM Travelstar 48GH, 30GN, and 15GN",
    "(IBM-|Hitachi )?IC25(T048ATDA05|N0(30|20|15|12|10|07|06|05)ATDA04)-.",
    "", "", ""
  },
  { "IBM Travelstar 32GH, 30GT, and 20GN",
    "IBM-DJSA-2(32|30|20|10|05)",
    "", "", ""
  },
  { "IBM Travelstar 4GN",
    "IBM-DKLA-2(216|324|432)0",
    "", "", ""
  },
  { "IBM/Hitachi Travelstar 60GH and 40GN",
    "(IBM-|Hitachi )?IC25(T060ATC[SX]05|N0[4321]0ATC[SX]04)-.",
    "", "", ""
  },
  { "IBM/Hitachi Travelstar 40GNX",
    "(IBM-|Hitachi )?IC25N0[42]0ATC[SX]05-.",
    "", "", ""
  },
  { "Hitachi Travelstar 80GN",
    "(Hitachi )?IC25N0[23468]0ATMR04-.",
    "", "", ""
  },
  { "Hitachi Travelstar 4K40",
    "(Hitachi )?HTS4240[234]0M9AT00",
    "", "", ""
  },
  { "Hitachi Travelstar 4K120",
    "(Hitachi )?(HTS4212(60|80|10|12)H9AT00|HTS421260G9AT00)",
    "", "", ""
  },
  { "Hitachi Travelstar 5K80",
    "(Hitachi )?HTS5480[8642]0M9AT00",
    "", "", ""
  },
  { "Hitachi Travelstar 5K100",
    "(Hitachi )?HTS5410[1864]0G9(AT|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar E5K100",
    "(Hitachi )?HTE541040G9(AT|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar 5K120",
    "(Hitachi )?HTS5412(60|80|10|12)H9(AT|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar 5K160",
    "(Hitachi |HITACHI )?HTS5416([468]0|1[26])J9(AT|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar E5K160",
    "(Hitachi )?HTE5416(12|16|60|80)J9(AT|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar 5K250",
    "(Hitachi |HITACHI )?HTS5425(80|12|16|20|25)K9(A3|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar 5K320", // tested with HITACHI HTS543232L9SA00/FB4ZC4EC,
    // Hitachi HTS543212L9SA02/FBBAC52F
    "(Hitachi |HITACHI )?HT(S|E)5432(80|12|16|25|32)L9(A3(00)?|SA0[012])",
    "", "", ""
  },
  { "Hitachi/HGST Travelstar Z5K320", // tested with Hitachi HTS543232A7A384/ES2OA70K
    "(Hitachi|HGST) HT[ES]5432(16|25|32)A7A38[145]",
    "", "", ""
  },
  { "Hitachi Travelstar 5K500.B", // tested with Hitachi HTS545050B9SA00/PB4OC60X,
      // Hitachi HTS545025B9SA02/PB2AC60W
    "(Hitachi )?HT[ES]5450(12|16|25|32|40|50)B9(A30[01]|SA0[02])",
    "", "", ""
  },
  { "Hitachi/HGST Travelstar Z5K500", // tested with HGST HTS545050A7E380/GG2OAC90,
      // Hitachi HTS545032A7E380/GGBOA7A0, HGST HTS545050A7E680/GR2OA230,
      // APPLE HDD HTS545050A7E362/GG2AB990
    "(Hitachi|HGST|APPLE HDD) HT[ES]5450(25|32|50)A7E(362|38[01]|680)",
    "", "", ""
  },
  { "Hitachi/HGST Travelstar 5K750", // tested with Hitachi HTS547575A9E384/JE4OA60A,
      // APPLE HDD HTS547550A9E384/JE3AD70F
    "(Hitachi|APPLE HDD) HT[ES]5475(50|64|75)A9E38[14]",
    "", "", ""
  },
  { "HGST Travelstar 5K1000", // tested with HGST HTS541010A9E680/JA0OA560,
      // HGST HTS541075A9E680/JA2OA560
    "HGST HT[ES]5410(64|75|10)A9E68[01]",
    "", "", ""
  },
  { "HGST Travelstar Z5K1000", // tested with HGST HTS541010A7E630/SE0OA4A0,
      // HGST HTS541010B7E610/01.01A01
    "HGST HTS5410(75|10)[AB]7E6(10|3[015])",
    "", "", ""
  },
  { "HGST Travelstar 5K1500", // tested with HGST HTS541515A9E630/KA0OA500
    "HGST HT[ES]541515A9E63[015]",
    "", "", ""
  },
  { "Hitachi Travelstar 7K60",
    "(Hitachi )?HTS726060M9AT00",
    "", "", ""
  },
  { "Hitachi Travelstar E7K60",
    "(Hitachi )?HTE7260[46]0M9AT00",
    "", "", ""
  },
  { "Hitachi Travelstar 7K100",
    "(Hitachi )?HTS7210[168]0G9(AT|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar E7K100",
    "(Hitachi )?HTE7210[168]0G9(AT|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar 7K200", // tested with HITACHI HTS722016K9SA00/DCDZC75A
    "(Hitachi |HITACHI )?HTS7220(80|10|12|16|20)K9(A3|SA)00",
    "", "", ""
  },
  { "Hitachi Travelstar 7K320", // tested with HITACHI HTS723216L9SA60/FC2ZC50B,
    // HTS723225L9A360/FCDOC30F, HTS723216L9A362/FC2OC39F
    "(Hitachi |HITACHI )?HT[ES]7232(80|12|16|25|32)L9(A300|A36[02]|SA6[01])",
    "", "", ""
  },
  { "Hitachi Travelstar Z7K320", // tested with HITACHI HTS723232A7A364/EC2ZB70B
    "(HITACHI )?HT[ES]7232(16|25|32)A7A36[145]",
    "", "", ""
  },
  { "Hitachi Travelstar 7K500", // tested with Hitachi HTS725050A9A360/PC4OC70D,
    // HITACHI HTS725032A9A364/PC3ZC70F
    "(Hitachi |HITACHI )?HT[ES]7250(12|16|25|32|50)A9A36[02-5]",
    "", "", ""
  },
  { "Hitachi/HGST Travelstar Z7K500", // tested with HITACHI HTS725050A7E630/GH2ZB390,
      // HGST HTS725050A7E630/GH2OA420, HGST HTS725050A7E630/GH2OA530
    "(HITACHI|HGST) HT[ES]7250(25|32|50)A7E63[015]",
    "", "", ""
  },
  { "Hitachi/HGST Travelstar 7K750", // tested with Hitachi HTS727550A9E364/JF3OA0E0,
      // Hitachi HTS727575A9E364/JF4OA0D0
    "(Hitachi|HGST) HT[ES]7275(50|64|75)A9E36[14]",
    "", "", ""
  },
  { "HGST Travelstar 7K1000", // tested with HGST HTS721010A9E630/JB0OA3B0
    // HGST HTS721075A9E630/JB2OA3J0
    "HGST HT[ES]7210(10|75)A9E63[01]",
    "", "", ""
  },
  { "IBM Deskstar 14GXP and 16GP",
    "IBM-DTTA-3(7101|7129|7144|5032|5043|5064|5084|5101|5129|5168)0",
    "", "", ""
  },
  { "IBM Deskstar 25GP and 22GXP",
    "IBM-DJNA-3(5(101|152|203|250)|7(091|135|180|220))0",
    "", "", ""
  },
  { "IBM Deskstar 37GP and 34GXP",
    "IBM-DPTA-3(5(375|300|225|150)|7(342|273|205|136))0",
    "", "", ""
  },
  { "IBM/Hitachi Deskstar 120GXP",
    "(IBM-)?IC35L((020|040|060|080|120)AVVA|0[24]0AVVN)07-[01]",
    "", "", ""
  },
  { "IBM/Hitachi Deskstar GXP-180",
    "(IBM-)?IC35L(030|060|090|120|180)AVV207-[01]",
    "", "", ""
  },
  { "Hitachi CinemaStar 5K320", // tested with Hitachi HCS5C3225SLA380/STBOA37H
    "Hitachi HCS5C32(25|32)SLA380",
    "", "", ""
  },
  { "Hitachi CinemaStar 5K1000", // Hitachi HCS5C1010CLA382/JC4OA3EA
    "Hitachi HCS5C10(10|75|50|32|25|16)CLA382",
    "", "", ""
  },
  { "Hitachi Deskstar 5K3000", // tested with HDS5C3030ALA630/MEAOA5C0,
      // Hitachi HDS5C3020BLE630/MZ4OAAB0 (OEM, Toshiba Canvio Desktop)
    "(Hitachi )?HDS5C30(15|20|30)(ALA|BLE)63[02].*",
    "", "", ""
  },
  { "Hitachi/HGST Deskstar 5K4000", // tested with HDS5C4040ALE630/MPAOA250
      // HGST HDS5C4040ALE630/MPAOA580
    "(Hitachi |HGST )?HDS5C40(30|40)ALE63[01].*",
    "", "", ""
  },
  { "Hitachi Deskstar 7K80",
    "(Hitachi )?HDS7280([48]0PLAT20|(40)?PLA320|80PLA380).*",
    "", "", ""
  },
  { "Hitachi Deskstar 7K160",
    "(Hitachi )?HDS7216(80|16)PLA[3T]80.*",
    "", "", ""
  },
  { "Hitachi Deskstar 7K250",
    "(Hitachi )?HDS7225((40|80|12|16)VLAT20|(12|16|25)VLAT80|(80|12|16|25)VLSA80)",
    "", "", ""
  },
  { "Hitachi Deskstar 7K250 (SUN branded)",
    "HITACHI HDS7225SBSUN250G.*",
    "", "", ""
  },
  { "Hitachi Deskstar T7K250",
    "(Hitachi )?HDT7225((25|20|16)DLA(T80|380))",
    "", "", ""
  },
  { "Hitachi Deskstar 7K400",
    "(Hitachi )?HDS724040KL(AT|SA)80",
    "", "", ""
  },
  { "Hitachi Deskstar 7K500",
    "(Hitachi )?HDS725050KLA(360|T80)",
    "", "", ""
  },
  { "Hitachi Deskstar P7K500",
    "(Hitachi )?HDP7250(16|25|32|40|50)GLA(36|38|T8)0",
    "", "", ""
  },
  { "Hitachi Deskstar T7K500",
    "(Hitachi )?HDT7250(25|32|40|50)VLA(360|380|T80)",
    "", "", ""
  },
  { "Hitachi Deskstar 7K1000",
    "(Hitachi )?HDS7210(50|75|10)KLA330",
    "", "", ""
  },
  { "Hitachi Deskstar 7K1000.B",
    "(Hitachi )?HDT7210((16|25)SLA380|(32|50|64|75|10)SLA360)",
    "", "", ""
  },
  { "Hitachi Deskstar 7K1000.C", // tested with Hitachi HDS721010CLA330/JP4OA3MA,
      // Hitachi HDS721025CLA682/JP1OA41A
    "(Hitachi )?HDS7210((16|25)CLA[36]82|(32|50)CLA[36]62|(64|75|10)CLA[36]3[02])",
    "", "", ""
  },
  { "Hitachi Deskstar 7K1000.D", // tested with HDS721010DLE630/MS2OA5Q0
    "Hitachi HDS7210(25|32|50|75|10)DLE630",
    "", "", ""
  },
  { "Hitachi Deskstar E7K1000", // tested with HDE721010SLA330/ST6OA31B
    "Hitachi HDE7210(50|75|10)SLA330",
    "", "", ""
  },
  { "Hitachi Deskstar 7K2000", // tested with HDS722020ALA330 RSD HUA/JKAOA31E
    "(Hitachi )?HDS722020ALA330( RSD HUA)?",
    "", "", ""
  },
  { "Hitachi Deskstar 7K3000", // tested with Hitachi HDS723030ALA640/MKAOA3B0,
      // Hitachi HDS723030BLE640/MX6OAAB0
    "Hitachi HDS7230((15|20)BLA642|30ALA640|30BLE640)",
    "", "", ""
  },
  { "Hitachi/HGST Deskstar 7K4000", // tested with Hitachi HDS724040ALE640/MJAOA250,
      // HGST HDS724040ALE640/MJAOA580
    "(Hitachi|HGST) HDS724040ALE640",
    "", "", ""
  },
  { "HGST Deskstar NAS", // tested with HGST HDN724040ALE640/MJAOA5E0,
      // HGST HDN726050ALE610/APGNT517, HGST HDN726060ALE610/APGNT517
      // HGST HDN726040ALE614/APGNW7JH, HGST HDN726060ALE614/K1HE594D
      // HGST HDN728080ALE604/A4GNW91X
    "HGST HDN72(40[34]|60[456]|808)0ALE6(04|1[04]|40)",
    "", "", ""
  //"-v 22,raw48,Helium_Level" // HDN728080ALE604
  },
  { "Hitachi/HGST Ultrastar 5K3000", // tested with Hitachi HUA5C3030ALA640/MEAOA800
    "(Hitachi |HGST )?HUA5C30(20|30)ALA64[01]",
    "", "", ""
  },
  { "Hitachi Ultrastar A7K1000", // tested with
    // HUA721010KLA330      44X2459 42C0424IBM/GKAOAB4A,,
    // Hitachi HUA721075KLA330/GK8OA70M,
    // HITACHI HUA721075KLA330/GK8OA90A
    "(Hitachi |HITACHI )?HUA7210(50|75|10)KLA330.*",
    "", "", ""
  },
  { "Hitachi Ultrastar A7K2000", // tested with
    // HUA722010CLA330      43W7629 42C0401IBM
    "(Hitachi )?HUA7220(50|10|20)[AC]LA33[01].*",
    "", "", ""
  },
  { "Hitachi Ultrastar 7K3000", // tested with Hitachi HUA723030ALA640/MKAOA580,
      // Hitachi HUA723020ALA641/MK7OA840, HUA723020ALA640/MK7OAAA0
    "(Hitachi )?HUA7230(20|30)ALA64[01]",
    "", "", ""
  },
  { "Hitachi/HGST Ultrastar 7K4000", // tested with Hitachi HUS724040ALE640/MJAOA3B0,
      // HGST HUS724040ALE640/MJAOA580, HGST HUS724020ALA640/MF6OAA70,
      // HUS724030ALA640/MF8OAAZ0, HITACHI HUS724040ALE640/MJAONS04,
      // HGST HUS724045ALE640/MJBOA5G0
    "(Hitachi |HITACHI |HGST )?HUS7240([234]0|45)AL[AE]64[01]",
    "", "", ""
  },
  { "Hitachi/HGST Ultrastar 7K2",
    "(Hitachi|HGST) HUS722T[12]TALA604",
    "", "",
    "-v 16,raw48,Gas_Gauge"
  },
  { "HGST Ultrastar 7K6000", // tested with HGST HUS726060ALE614/APGNW517
    "HGST HUS7260[2456]0AL[AEN]61[014]",
    "", "", ""
  },
  { "HGST Ultrastar HC310/320", // tested with HGST HUS726T6TALE6L4/VKGNW40H,
      // HGST HUS728T8TALE6L4/V8GNW460, HGST HUS726T4TALA6L1/VLGNX41C
    "HGST HUS72(6T[46]|8T8)TAL[AE]6L[14]",
    "", "", ""
  },
  { "HGST Ultrastar He6", // tested with HGST HUS726060ALA640/AHGNT1E2
    "HGST HUS726060ALA64[01]",
    "", "", ""
  //"-v 22,raw48,Helium_Level"
  },
  { "HGST Ultrastar He8", // tested with HGST HUH728060ALE600/GR2OA230
    "HGST HUH7280(60|80)AL[EN]60[014]",
    "", "", ""
  //"-v 22,raw48,Helium_Level"
  },
  { "HGST Ultrastar He10", // tested with HGST HUH7210100ALE600/0F27452
    "HGST HUH7210(08|10)AL[EN]60[014]",
    "", "", ""
  //"-v 22,raw48,Helium_Level"
  },
  { "Western Digital Ultrastar (He10/12)", // WD white label, tested with
      // WDC WD80EMAZ-00WJTA0/83.H0A83 (Easystore 0x1058:0x25fb),
      // WDC WD80EZAZ-11TDBA0/83.H0A83, WDC WD100EMAZ-00WJTA0/83.H0A83,
      // WDC WD100EZAZ-11TDBA0/83.H0A83, WDC WD120EMAZ-11BLFA0/81.00A81
      // WDC WD140EDFZ-11A0VA0/81.00A81 (Easystore 0x1058:0x25fb)
      // WDC WD140EDGZ-11B2DA2/85.00A85, WDC WD140EDGZ-11B1PA0/85.00A85
      // WDC WD120EDAZ-11F3RA0/81.00A81, WDC WD80EDAZ-11TA3A0/81.00A81
      // WDC WD40EDAZ-11SLVB0/80.00A80, WDC WD160EDGZ-11CMXA0/85.00A85 (My Book 0x1058:0x25ee)
    "WDC WD(40|80|100|120|140|160)E([MZ]A|DA|DF|DG)Z-.*",
    "", "", ""
  //"-v 22,raw48,Helium_Level" // not: WD80EDAZ, WD40EDAZ
  },
  { "HGST Ultrastar DC HC520 (He12)", // tested with HGST HUH721212ALE600/LEGNT3D0
    "HGST HUH721212AL[EN]60[014]",
    "", "", ""
  //"-v 22,raw48,Helium_Level"
  },
  { "Western Digital Ultrastar DC HC530", // tested with
      // WDC  WUH721414ALE604/LDAZW110, WDC  WUH721414ALE6L4/LDGNW07G
    "WDC  ?WUH721414ALE6[0L]4",
    "", "",
  //"-v 22,raw48,Helium_Level "
    "-v 188,raw16 "
  },
  { "Western Digital Ultrastar DC HC550", // tested with WDC  WUH721818ALE6L4/PCGNW110,
      // WUH721818ALE6L4/PCGAW232, WDC  WUH721818ALN6L4/PCGNW088
    "(WDC  ?)?WUH72181[68]AL[EN]6[0L][0146]",
    "", "", ""
  //"-v 22,raw48,Helium_Level"
  },
  { "Western Digital Ultrastar DC HC560", // tested with WDC  WUH722020ALN604/PQGNW108
    // WDC WUH722020BLE6L4,
    // WDC WD200EDGZ-11BLDS0/85.00A85 (White label, Elements 0x1058:0x25a3)
    "(WDC  ?)?WUH722020[AB]L[EN]6[0L][014]|"
    "WDC WD200EDGZ-.*",
    "", "",
  //"-v 22,raw48,Helium_Level "
    "-v 82,raw16,Head_Health_Score "
    "-v 90,hex48,NAND_Master"
  },
  { "Western Digital Ultrastar DC HC570", // tested with WUH722222ALE604
    "(WDC  ?)?WUH722222[AB]L[EN]6[0L]4",
    "", "",
  //"-v 22,raw48,Helium_Level "
    "-v 71,raw16,Milli_Micro_Actuator "
    "-v 82,raw16,Head_Health_Score "
    "-v 90,hex48,NAND_Master"
  },
  { "Western Digital Ultrastar DC HC580", // tested with WDC  WUH722424ALE6L4/LVGNWF10
    "(WDC  ?)?WUH72242[24]ALE6L[14]",
    "", "",
  //"-v 22,raw48,Helium_Level "
    "-v 71,raw16,Milli_Micro_Actuator "
    "-v 90,hex48,NAND_Master"
  },
  { "Western Digital Ultrastar DC HC650", // tested with WDC  WSH722020ALE6L0/PCGMT421
    "(WDC  ?)?WSH7220(20|VC)AL[EN]6[0L][0146]",
    "", "", ""
  //"-v 22,raw48,Helium_Level"
  },
  { "Western Digital Ultrastar DC HC670", // WSH722626ALE604
    "(WDC  ?)?WSH722222[AB]L[EN]6[0L]4",
    "", "",
  //"-v 22,raw48,Helium_Level "
    "-v 71,raw16,Milli_Micro_Actuator "
    "-v 82,raw16,Head_Health_Score "
    "-v 90,hex48,NAND_Master"
  },
  { "HGST MegaScale 4000", // tested with HGST HMS5C4040ALE640/MPAOA580
    "HGST HMS5C4040[AB]LE64[01]", // B = DC 4000.B
    "", "", ""
  },
  { "Toshiba 2.5\" HDD (10-20 GB)",
    "TOSHIBA MK(101[67]GAP|15[67]GAP|20(1[678]GAP|(18|23)GAS))",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD (30-60 GB)",
    "TOSHIBA MK((6034|4032)GSX|(6034|4032)GAX|(6026|4026|4019|3019)GAXB?|(6025|6021|4025|4021|4018|3025|3021|3018)GAS|(4036|3029)GACE?|(4018|3017)GAP)",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD (80 GB and above)",
    "TOSHIBA MK(80(25GAS|26GAX|32GAX|32GSX)|10(31GAS|32GAX)|12(33GAS|34G[AS]X)|2035GSS)",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..37GSX", // tested with TOSHIBA MK1637GSX/DL032C
    "TOSHIBA MK(12|16)37GSX",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..46GSX", // tested with TOSHIBA MK1246GSX/LB213M
    "TOSHIBA MK(80|12|16|25)46GSX",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..50GACY", // tested with TOSHIBA MK8050GACY/TF105A
    "TOSHIBA MK8050GACY",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..34GSX", // tested with TOSHIBA MK8034GSX/AH301E
    "TOSHIBA MK(80|12|10)34GSX",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..32GSX", // tested with TOSHIBA MK1032GSX/AS021G
    "TOSHIBA MK(10|80|60|40)32GSX",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..51GSY", // tested with TOSHIBA MK1251GSY/LD101D
    "TOSHIBA MK(80|12|16|25)51GSY",
    "",
    "",
    "-v 9,minutes"
  },
  { "Toshiba 2.5\" HDD MK..52GSX", // tested with TOSHIBA MK3252GSX/LV010A
    "TOSHIBA MK(80|12|16|25|32)52GSX",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..55GSX", // tested with TOSHIBA MK5055GSX/FG001A, MK3255GSXF/FH115B
    "TOSHIBA MK(12|16|25|32|40|50)55GSXF?",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..56GSY", // tested with TOSHIBA MK2556GSYF/LJ001D
    "TOSHIBA MK(16|25|32|50)56GSYF?",
    "",
    "",
    "-v 9,minutes"
  },
  { "Toshiba 2.5\" HDD MK..59GSXP (AF)",
    "TOSHIBA MK(32|50|64|75)59GSXP?",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..59GSM (AF)",
    "TOSHIBA MK(75|10)59GSM",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..61GSY[N]", // tested with TOSHIBA MK5061GSY/MC102E, MK5061GSYN/MH000A,
      // TOSHIBA MK2561GSYN/MH000D
    "TOSHIBA MK(16|25|32|50|64)61GSYN?",
    "",
    "",
    "-v 9,minutes" // TOSHIBA MK2561GSYN/MH000D
  },
  { "Toshiba 2.5\" HDD MK..61GSYB", // tested with TOSHIBA MK5061GSYB/ME0A
    "TOSHIBA MK(16|25|32|50|64)61GSYB",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..65GSX", // tested with TOSHIBA MK5065GSX/GJ003A, MK3265GSXN/GH012H,
      // MK5065GSXF/GP006B, MK2565GSX H/GJ003A
    "TOSHIBA MK(16|25|32|50|64)65GSX[FN]?( H)?", // "... H" = USB ?
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..75GSX", // tested with TOSHIBA MK7575GSX/GT001C
    "TOSHIBA MK(32|50|64|75)75GSX",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MK..76GSX/GS001A", // tested with TOSHIBA MK2576GSX/GS001A
    "TOSHIBA MK(16|25|32|50|64)76GSX",
    "GS001A",
    "", ""
  },
  { "Toshiba 2.5\" HDD MK..76GSX", // tested with TOSHIBA MK3276GSX/GS002D
    "TOSHIBA MK(16|25|32|50|64)76GSX",
    "",
    "",
    "-v 9,minutes"
  },
  { "Toshiba 2.5\" HDD MQ01ABB...", // tested with TOSHIBA MQ01ABB200/AY000U
    "TOSHIBA MQ01ABB(100|150|200)",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ01ABC...", // tested with TOSHIBA MQ01ABC150/AQ001U
    "TOSHIBA MQ01ABC(100|150|200)",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ01ABD...", // tested with TOSHIBA MQ01ABD100/AX001U,
      // TOSHIBA MQ01ABD100/AX1R4C, TOSHIBA MQ01ABD100V/AX001Q
    "TOSHIBA MQ01ABD(025|032|050|064|075|100)V?",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ01ABF...", // tested with TOSHIBA MQ01ABF050/AM001J,
      // TOSHIBA MQ01ABF032/AM001J
    "TOSHIBA MQ01ABF(032|050|075|100)",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ01UBB... (USB 3.0)", // tested with TOSHIBA MQ01UBB200/AY000U (0x0480:0xa100),
      // TOSHIBA MQ01UBB200/34MATMZ5T (0x05ac:0x8406)
    "TOSHIBA MQ01UBB200",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ01UBD... (USB 3.0)", // tested with TOSHIBA MQ01UBD050/AX001U (0x0480:0xa007),
      // TOSHIBA MQ01UBD100/AX001U (0x0480:0x0201, 0x0480:0xa200),
      // TOSHIBA MQ01UBD050/AX101U (0x0480:0xa202)
    "TOSHIBA MQ01UBD(050|075|100)",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ04UBF... (USB 3.0)", // tested with TOSHIBA MQ04UBF100/JU000U (0x0480:0xa202)
    "TOSHIBA MQ04UBF100",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ04UBD...", // tested with TOSHIBA MQ04UBD200/68U2T2VWT
    "TOSHIBA MQ04UBD200",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ03ABB...", // tested with TOSHIBA MQ03ABB300
    "TOSHIBA MQ03ABB[23]00",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ03UBB...", // tested with TOSHIBA MQ03UBB200/37I7T0NJT
    "TOSHIBA MQ03UBB(300|200|250)",
    "", "", ""
  },
  { "Toshiba 2.5\" HDD MQ04UBB... (USB, SMR)", // tested with TOSHIBA MQ04UBB400/JS000U,
      // TOSHIBA MQ04UBB400/JS0B0U (0x0480:0xa301) ('Device managed zones', no TRIM support)
    "TOSHIBA MQ04UBB[24]00",
    "", "", ""
  },
  { "Toshiba 3.5\" HDD MK.002TSKB", // tested with TOSHIBA MK1002TSKB/MT1A
    "TOSHIBA MK(10|20)02TSKB",
    "", "", ""
  },
  { "Toshiba 3.5\" MG03ACAxxx(Y) Enterprise HDD", // tested with TOSHIBA MG03ACA100/FL1A
    "TOSHIBA MG03ACA[1234]00Y?",
    "", "", ""
  },
  { "Toshiba MD04ACA... Enterprise HDD", // tested with TOSHIBA MD04ACA500/FP1A
    "TOSHIBA MD04ACA[2-6]00N?",
    "", "", ""
  },
  { "Toshiba MG04ACA... Enterprise HDD", // tested with TOSHIBA MG04ACA600A/FS2B,
      // TOSHIBA MG04ACA400NY/FK5D (Dell)
    "TOSHIBA MG04ACA[1-6]00[AEN]Y?",
    "", "", ""
  },
  { "Toshiba MG05ACA... Enterprise Capacity HDD", // tested with TOSHIBA MG05ACA800E/GX2A
    "TOSHIBA MG05ACA800[AE]",
    "", "", ""
  },
  { "Toshiba MG06ACA... Enterprise Capacity HDD", // tested with TOSHIBA MG06ACA800E/0109,
      // TOSHIBA MG06ACA800E/4303, TOSHIBA MG06ACA10TE/0103,
    "TOSHIBA MG06ACA([68]00|10T)[AE]Y?",
    "", "", ""
  },
  { "Toshiba MG07ACA... Enterprise Capacity HDD", // tested with TOSHIBA MG07ACA14TE/0101
    "TOSHIBA MG07ACA1[24]T[AE]Y?",
    "", "", ""
  //"-v 23,raw48,Helium_Condition_Lower "
  //"-v 24,raw48,Helium_Condition_Upper"
  },
  { "Toshiba MG08ACA... Enterprise Capacity HDD", // tested with TOSHIBA MG08ACA14TE/0102,
      // TOSHIBA MG08ACA16TE/0102
    "TOSHIBA MG08ACA1[46]T[AE]Y?",
    "", "", ""
  //"-v 23,raw48,Helium_Condition_Lower "
  //"-v 24,raw48,Helium_Condition_Upper"
  },
  { "Toshiba MG08ADA... Enterprise Capacity HDD", // tested with TOSHIBA MG08ADA800E/0101,
      // TOSHIBA MG08ADA800E/4303, TOSHIBA MG08ADA800E/4304
    "TOSHIBA MG08ADA[468]00[AEN]Y?",
    "", "", ""
  },
  { "Toshiba MG09ACA... Enterprise Capacity HDD", // tested with TOSHIBA MG09ACA18TE/0102,
      // "MG09ACA12TE          01GV181D7A01906LEN/BB3A"
    "(TOSHIBA )?MG09ACA1[02468]T[AE]Y?( .*LEN)?",
    "", "",
  //"-v 23,raw48,Helium_Condition_Lower "
  //"-v 24,raw48,Helium_Condition_Upper "
    "-v 27,raw48,MAMR_Health_Monitor"
  },
  { "Toshiba MG10ACA... Enterprise Capacity HDD", // tested with TOSHIBA MG10ACA20TE/0102
    "TOSHIBA MG10ACA20T[AE]Y?",
    "", "",
  //"-v 23,raw48,Helium_Condition_Lower "
  //"-v 24,raw48,Helium_Condition_Upper "
    "-v 27,raw48,MAMR_Health_Monitor"
  },
  { "Toshiba MG10ADA... Enterprise Capacity HDD", // tested with TOSHIBA MG10ADA10TE/0101
    "TOSHIBA MG10ADA([12468]00|10T)[EN]",
    "", "",
  //"-v 23,raw48,Helium_Condition_Lower "
  //"-v 24,raw48,Helium_Condition_Upper "
    "-v 27,raw48,MAMR_Health_Monitor"
  },
  { "Toshiba MG10AFA... Enterprise Capacity HDD", // tested with TOSHIBA MG10AFA22TE/0102
    "TOSHIBA MG10AFA22T[AE]Y?",
    "", "",
  //"-v 23,raw48,Helium_Condition_Lower "
  //"-v 24,raw48,Helium_Condition_Upper "
    "-v 27,raw48,MAMR_Health_Monitor"
  },
  { "Toshiba MG11 Cloud-scale Capacity HDD", // tested with TOSHIBA MG11ACA24TE/0102
    "TOSHIBA MG11AC[AP](1[468]|2[024])TEY?", // ACP = self-encrypting device (SED)
    "", "",                                  // TEY = sanitize instant erase (SIE)
  //"-v 23,raw48,Helium_Condition_Lower "
  //"-v 24,raw48,Helium_Condition_Upper "
    "-v 27,raw48,MAMR_Health_Monitor"
  },
  { "Toshiba 3.5\" DT01ABA... Desktop HDD", // tested with TOSHIBA DT01ABA300/MZ6OABB0
    "TOSHIBA DT01ABA(100|150|200|300)",
    "", "", ""
  },
  { "Toshiba 3.5\" DT01ACA... Desktop HDD", // tested with TOSHIBA DT01ACA100/MS2OA750,
      // TOSHIBA DT01ACA200/MX4OABB0, TOSHIBA DT01ACA300/MX6OABB0
    "TOSHIBA DT01ACA(025|032|050|075|100|150|200|300)",
    "", "", ""
  },
  { "Toshiba N300/MN NAS HDD", // tested with TOSHIBA HDWQ140/FJ1M, TOSHIBA HDWN160/FS1M,
      // TOSHIBA HDWN180/GX2M, TOSHIBA HDWG440/0601 (4TB), TOSHIBA HDWG480/0601 (8TB),
      // TOSHIBA HDWG11A/0603 (10TB), TOSHIBA HDWG21C/0601 (12TB), TOSHIBA HDWG21E/0601 (14TB),
      // TOSHIBA MN07ACA12T/0601, TOSHIBA MN08ACA14T/0601, TOSHIBA HDWG51J/0104 (18TB)
    "TOSHIBA HDW([GNQ]1[468]0|G(440|480|11A|21[CE]|31[EG]|51[EJ]))|" // 31G: 16TB
    "TOSHIBA MN0(4ACA400|6ACA([68]00|10T)|7ACA1[24]T|8ACA1[46]T)",
    "", "",
  //"-v 23,raw48,Helium_Condition_Lower " // ] >= 12TB
  //"-v 24,raw48,Helium_Condition_Upper " // ]
    "-v 27,raw48,MAMR_Health_Monitor" // HDWG51J/0104
  },
  { "Toshiba P300 (CMR)", // tested with TOSHIBA HDWD120/MX4OACF0
    "TOSHIBA HDWD1(05|10|20|30)",
    "", "", ""
  },
  { "Toshiba P300 (SMR)", // tested with TOSHIBA HDWD240/KQ000A
    "TOSHIBA HDWD2[246]0",
    "", "", ""
  },
  { "Toshiba S300 (SMR)", // tested with TOSHIBA HDWT860/KQ0H1L
    "TOSHIBA HDWT(7[24]|8[46])0",
    "", "", ""
  },
  { "Toshiba X300", // tested with TOSHIBA HDWE160/FS2A, TOSHIBA HDWF180/GX0B
      // TOSHIBA HDWR480/0601
    "TOSHIBA HDW(E1[456]0|[FR]180|R(4[468]0|11A|21[CE]|31[EG]|51J))", // 4n0:nTB, 11A:10TB,
      // 21C:12TB, 21E:14TB, 31E:14TB, 31G:16TB, 51J:18TB
    "", "", ""
  //"-v 23,raw48,Helium_Condition_Lower " // ] >= 12TB
  //"-v 24,raw48,Helium_Condition_Upper"  // ]
  },
  { "Toshiba L200 (CMR)",
    "TOSHIBA HDW[JK]1(05|10)",
    "", "", ""
  },
  { "Toshiba L200 (SMR)", // tested with TOSHIBA HDWL110/JU000A. TOSHIBA HDWL120/JT000A
    "TOSHIBA HDWL1[12]0",
    "", "", ""
  },
  { "Toshiba 1.8\" HDD",
    "TOSHIBA MK[23468]00[4-9]GA[HL]",
    "", "", ""
  },
  { "Toshiba 1.8\" HDD MK..29GSG",
    "TOSHIBA MK(12|16|25)29GSG",
    "", "", ""
  },
  { "", // TOSHIBA MK6022GAX
    "TOSHIBA MK6022GAX",
    "", "", ""
  },
  { "Toshiba HK4R Series SSD", // TOSHIBA THNSN8960PCSE/8EET6101,
      // TOSHIBA THNSN81Q92CSE/8ENP6101
    "TOSHIBA THNSN8(120P|240P|480P|960P|1Q92)CSE",
    "", "",
    "-v 167,raw48,SSD_Protect_Mode "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 169,raw48,Bad_Block_Count "
    "-v 173,raw48,Erase_Count "
    "-v 241,raw48,Host_Writes_32MiB "
    "-v 242,raw48,Host_Reads_32MiB"
  },
  { "Toshiba HG6 Series SSD", // TOSHIBA THNSNJ512GCST/JTRA0102
    // https://www.farnell.com/datasheets/1852757.pdf
    // TOSHIBA THNSFJ256GCSU/JULA1102
    // TOSHIBA THNSFJ256GDNU A/JYLA1102
    "TOSHIBA THNS[NF]J(060|128|256|512)G[BCAM8VD][SCN][TU].*",
    "", "",
    "-v 167,raw48,SSD_Protect_Mode "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 169,raw48,Bad_Block_Count "
    "-v 173,raw48,Erase_Count "
  },
  { "", // TOSHIBA MK6409MAV
    "TOSHIBA MK6409MAV",
    "", "", ""
  },
  { "Toshiba MKx019GAXB (SUN branded)",
    "TOS MK[34]019GAXB SUN[34]0G",
    "", "", ""
  },
  { "Seagate Momentus",
    "ST9(20|28|40|48)11A",
    "", "", ""
  },
  { "Seagate Momentus 42",
    "ST9(2014|3015|4019)A",
    "", "", ""
  },
  { "Seagate Momentus 4200.2", // tested with ST960812A/3.05
    "ST9(100822|808210|60812|50212|402113|30219)A",
    "", "", ""
  },
  { "Seagate Momentus 5400.2",
    "ST9(808211|6082[12]|408114|308110|120821|10082[34]|8823|6812|4813|3811)AS?",
    "", "", ""
  },
  { "Seagate Momentus 5400.3",
    "ST9(4081[45]|6081[35]|8081[15]|100828|120822|160821)AS?",
    "", "", ""
  },
  { "Seagate Momentus 5400.3 ED",
    "ST9(4081[45]|6081[35]|8081[15]|100828|120822|160821)AB",
    "", "", ""
  },
  { "Seagate Momentus 5400.4",
    "ST9(120817|(160|200|250)827)AS",
    "", "", ""
  },
  { "Seagate Momentus 5400.5",
    "ST9((80|120|160)310|(250|320)320)AS",
    "", "", ""
  },
  { "Seagate Momentus 5400.6",
    "ST9(80313|160(301|314)|(12|25)0315|250317|(320|500)325|500327|640320)ASG?",
    "", "",
    "-F xerrorlba" // ST9500325AS/0002SDM1 (ticket #1094)
  },
  { "Seagate Momentus 5400.7",
    "ST9(160316|(250|320)310|(500|640)320)AS",
    "", "", ""
  },
  { "Seagate Momentus 5400.7 (AF)", // tested with ST9640322AS/0001BSM2
      // (device reports 4KiB LPS with 1 sector offset)
    "ST9(320312|400321|640322|750423)AS",
    "", "", ""
  },
  { "Seagate Momentus 5400 PSD", // Hybrid drives
    "ST9(808212|(120|160)8220)AS",
    "", "", ""
  },
  { "Seagate Momentus 7200.1",
    "ST9(10021|80825|6023|4015)AS?",
    "", "", ""
  },
  { "Seagate Momentus 7200.2",
    "ST9(80813|100821|120823|160823|200420)ASG?",
    "", "", ""
  },
  { "Seagate Momentus 7200.3",
    "ST9((80|120|160)411|(250|320)421)ASG?",
    "", "", ""
  },
  { "Seagate Momentus 7200.4", // tested with ST9500420AS/0002SDM1
    "ST9(160412|250410|320423|500420)ASG?",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 -v 188,raw16 "
    "-v 195,raw24/raw32,ECC_On_the_Fly_Count "
    "-v 240,msec24hour32"
  },
  { "Seagate Momentus 7200 FDE.2",
    "ST9((160413|25041[12]|320426|50042[12])AS|(16041[489]|2504[16]4|32042[67]|500426)ASG)",
    "", "", ""
  },
  { "Seagate Momentus 7200.5", // tested with ST9750420AS/0001SDM5, ST9750420AS/0002SDM1
    "ST9(50042[34]|64042[012]|75042[02])ASG?",
    "", "", ""
  },
  { "Seagate Momentus XT", // fixed firmware
    "ST9(2505610|3205620|5005620)AS",
    "SD2[68]", // https://knowledge.seagate.com/articles/en_US/FAQ/215451en
    "", ""
  },
  { "Seagate Momentus XT", // buggy firmware, tested with ST92505610AS/SD24
    "ST9(2505610|3205620|5005620)AS",
    "SD2[45]",
    "These drives may corrupt large files,\n"
    "AND THIS FIRMWARE VERSION IS AFFECTED,\n"
    "see the following web pages for details:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/215451en\n"
    "https://superuser.com/questions/313447/seagate-momentus-xt-corrupting-files-linux-and-mac",
    ""
  },
  { "Seagate Momentus XT", // unknown firmware
    "ST9(2505610|3205620|5005620)AS",
    "",
    "These drives may corrupt large files,\n"
    "see the following web pages for details:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/215451en\n"
    "https://superuser.com/questions/313447/seagate-momentus-xt-corrupting-files-linux-and-mac",
    ""
  },
  { "Seagate Momentus XT (AF)", // tested with ST750LX003-1AC154/SM12
    "ST750LX003-.*",
    "", "", ""
  },
  { "Seagate Momentus Thin", // tested with ST320LT007-9ZV142/0004LVM1
    "ST(160|250|320)LT0(07|09|11|14)-.*",
    "", "", ""
  },
  { "Seagate Laptop HDD", // tested with ST500LT012-9WS142/0001SDM1,
      // ST500LM021-1KJ152/0002LIM1, ST500LM021-1KJ152/0003LIM1, ST4000LM016-1N2170/0003
    "ST((25|32|50)0LT0(12|15|25)|(32|50)0LM0(10|21)|[34]000LM016)-.*",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 -v 188,raw16"
  },
  { "Seagate Laptop SSHD", // tested with ST500LM000-1EJ162/SM11
    "ST(500|1000)LM0(00|14)-.*",
    "", "", ""
  },
  { "Seagate Medalist 1010, 1720, 1721, 2120, 3230 and 4340",  // ATA2, with -t permissive
    "ST3(1010|1720|1721|2120|3230|4340)A",
    "", "", ""
  },
  { "Seagate Medalist 2110, 3221, 4321, 6531, and 8641",
    "ST3(2110|3221|4321|6531|8641)A",
    "", "", ""
  },
  { "Seagate U4",
    "ST3(2112|4311|6421|8421)A",
    "", "", ""
  },
  { "Seagate U5",
    "ST3(40823|30621|20413|15311|10211)A",
    "", "", ""
  },
  { "Seagate U6",
    "ST3(8002|6002|4081|3061|2041)0A",
    "", "", ""
  },
  { "Seagate U7",
    "ST3(30012|40012|60012|80022|120020)A",
    "", "", ""
  },
  { "Seagate U8",
    "ST3(4313|6811|8410|4313|13021|17221)A",
    "", "", ""
  },
  { "Seagate U9", // tested with ST3160022ACE/9.51
    "ST3(80012|120025|160022)A(CE)?",
    "", "", ""
  },
  { "Seagate U10",
    "ST3(20423|15323|10212)A",
    "", "", ""
  },
  { "Seagate UX",
    "ST3(10014A(CE)?|20014A)",
    "", "", ""
  },
  { "Seagate Barracuda ATA",
    "ST3(2804|2724|2043|1362|1022|681)0A",
    "", "", ""
  },
  { "Seagate Barracuda ATA II",
    "ST3(3063|2042|1532|1021)0A",
    "", "", ""
  },
  { "Seagate Barracuda ATA III",
    "ST3(40824|30620|20414|15310|10215)A",
    "", "", ""
  },
  { "Seagate Barracuda ATA IV",
    "ST3(20011|30011|40016|60021|80021)A",
    "", "", ""
  },
  { "Seagate Barracuda ATA V",
    "ST3(12002(3A|4A|9A|3AS)|800(23A|15A|23AS)|60(015A|210A)|40017A)",
    "", "", ""
  },
  { "Seagate Barracuda 5400.1",
    "ST340015A",
    "", "", ""
  },
  { "Seagate Barracuda 7200.7 and 7200.7 Plus", // tested with "ST380819AS          39M3701 39M0171 IBM"/3.03
    "ST3(200021A|200822AS?|16002[13]AS?|12002[26]AS?|1[26]082[78]AS|8001[13]AS?|8081[79]AS|60014A|40111AS|40014AS?)( .* IBM)?",
    "", "", ""
  },
  { "Seagate Barracuda 7200.8",
    "ST3(400[68]32|300[68]31|250[68]23|200826)AS?",
    "", "", ""
  },
  { "Seagate Barracuda 7200.9",
    "ST3(402111?|80[28]110?|120[28]1[0134]|160[28]1[012]|200827|250[68]24|300[68]22|(320|400)[68]33|500[68](32|41))AS?.*",
    "", "", ""
  },
  { "Seagate Barracuda 7200.10", // tested with GB0160EAFJE/HPG0
    "ST3((80|160)[28]15|200820|250[34]10|(250|300|320|400)[68]20|360320|500[68]30|750[68]40)AS?|"
    "GB0160EAFJE", // HP OEM
    "", "", ""
  },
  { "Seagate Barracuda 7200.11", // unaffected firmware
    "ST3(160813|320[68]13|500[368]20|640[36]23|640[35]30|750[36]30|1000(333|[36]40)|1500341)AS?",
    "CC.?.?", // https://knowledge.seagate.com/articles/en_US/FAQ/207957en
    "", ""
  },
  { "Seagate Barracuda 7200.11", // fixed firmware
    "ST3(500[368]20|750[36]30|1000340)AS?",
    "SD1A", // https://knowledge.seagate.com/articles/en_US/FAQ/207951en
    "", ""
  },
  { "Seagate Barracuda 7200.11", // fixed firmware
    "ST3(160813|320[68]13|640[36]23|1000333|1500341)AS?",
    "SD[12]B", // https://knowledge.seagate.com/articles/en_US/FAQ/207957en
    "", ""
  },
  { "Seagate Barracuda 7200.11", // buggy or fixed firmware
    "ST3(500[368]20|640[35]30|750[36]30|1000340)AS?",
    "(AD14|SD1[5-9]|SD81)",
    "There are known problems with these drives,\n"
    "THIS DRIVE MAY OR MAY NOT BE AFFECTED,\n"
    "see the following web pages for details:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207951en\n"
    "https://bugs.debian.org/cgi-bin/bugreport.cgi?bug=632758",
    ""
  },
  { "Seagate Barracuda 7200.11", // unknown firmware
    "ST3(160813|320[68]13|500[368]20|640[36]23|640[35]30|750[36]30|1000(333|[36]40)|1500341)AS?",
    "",
    "There are known problems with these drives,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207951en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207957en",
    ""
  },
  { "Seagate Barracuda 7200.12", // new firmware, tested with ST3500418AS/HP34
    "ST3(160318|250318|320418|50041[08]|750528|1000528)AS",
    "CC4[9A-Z]|HP34", // HP34: 180 Unknown_HDD_Attribute
    "", ""
  },
  { "Seagate Barracuda 7200.12", // unknown firmware
    "ST3(160318|250318|320418|50041[08]|750528|1000528)AS",
    "",
    "A firmware update for this drive may be available,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/213891en",
    ""
  },
  { "Seagate Barracuda 7200.12", // tested with ST3160316AS/JC45, ST3250312AS/JC45,
      // ST3500413AS/JC47, ST3500413AS/JC4B, ST3750525AS/JC4B, ST31000524AS/JC45,
      // ST31000524AS/JC4B
    "ST3(160318|25031[128]|320418|50041[038]|750(518|52[358])|100052[348]|320413|160316)AS",
    "", "", ""
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Barracuda XT", // tested with ST32000641AS/CC13,
      // ST4000DX000-1C5160/CC42
    "ST(3(2000641|3000651)AS|4000DX000-.*)",
    "", "", ""
  },
  { "Seagate Barracuda 7200.14 (AF)", // new firmware, tested with
      // ST3000DM001-9YN166/CC4H, ST3000DM001-9YN166/CC9E
    "ST(1000|1500|2000|2500|3000)DM00[1-3]-9YN16.",
    "CC(4[H-Z]|[5-9A-Z]..*)", // >= "CC4H"
    "",
    "-v 188,raw16 -v 240,msec24hour32" // tested with ST3000DM001-9YN166/CC4H
  },
  { "Seagate Barracuda 7200.14 (AF)", // old firmware, tested with
      // ST1000DM003-9YN162/CC46
    "ST(1000|1500|2000|2500|3000)DM00[1-3]-9YN16.",
    "CC4[679CG]",
    "A firmware update for this drive is available,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/223651en",
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Barracuda 7200.14 (AF)", // unknown firmware
    "ST(1000|1500|2000|2500|3000)DM00[1-3]-9YN16.",
    "",
    "A firmware update for this drive may be available,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/223651en",
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Barracuda 7200.14 (AF)", // different part number, tested with
      // ST1000DM003-1CH162/CC47, ST1000DM003-1CH162/CC49, ST2000DM001-1CH164/CC24,
      // ST1000DM000-9TS15E/CC92, APPLE HDD ST3000DM001/AP15 (no attr 240),
      // APPLE HDD ST1000DM003/AP18
    "ST(1000|1500|2000|2500|3000)DM00[0-3]-.*|"
    "APPLE HDD ST([13]000DM00[13])",
    "", "",
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Barracuda 7200.14 (AF)", // < 1TB, tested with ST250DM000-1BC141
    "ST(250|320|500|750)DM00[0-3]-.*",
    "", "",
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate BarraCuda 3.5 (CMR)", // tested with ST1000DM010-2EP102/CC43, ST3000DM008-2DM166/CC26
    "ST(500DM009|1000DM010|2000DM00[67]|3000DM00[89]|4000DM005)-.*",
    "", "",
    "-v 200,raw48,Pressure_Limit "
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate BarraCuda 3.5 (SMR)", // tested with ST2000DM008-2FR102/0001,
      // ST4000DM004-2CV104/0001 (TRIM: no), ST4000DM005-2DP166/0001, ST8000DM004-2CX188/0001
    "ST(2000DM00[58]|3000DM007|[48]000DM004|6000DM003)-.*",
    "", "",
    "-v 9,msec24hour32 " // ST4000DM004-2CV104/0001
    "-v 200,raw48,Pressure_Limit "
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Desktop HDD.15", // tested with ST4000DM000-1CD168/CC43, ST5000DM000-1FK178/CC44,
      // ST6000DM001-1XY17Z/CC48
    "ST[4568]000DM00[012]-.*",
    "", "",
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Desktop SSHD", // tested with ST2000DX001-1CM164/CC43
    "ST[124]000DX001-.*",
    "", "",
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Barracuda LP", // new firmware
    "ST3(500412|1000520|1500541|2000542)AS",
    "CC3[5-9A-Z]",
    "",
    "" // -F xerrorlba ?
  },
  { "Seagate Barracuda LP", // unknown firmware
    "ST3(500412|1000520|1500541|2000542)AS",
    "",
    "A firmware update for this drive may be available,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/213915en",
    "-F xerrorlba" // tested with ST31000520AS/CC32
  },
  { "Seagate Barracuda Green (AF)", // new firmware
    "ST((10|15|20)00DL00[123])-.*",
    "CC(3[2-9A-Z]|[4-9A-Z]..*)", // >= "CC32"
    "", ""
  },
  { "Seagate Barracuda Green (AF)", // unknown firmware
    "ST((10|15|20)00DL00[123])-.*",
    "",
    "A firmware update for this drive may be available,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/218171en",
    ""
  },
  { "Seagate Barracuda ES",
    "ST3(250[68]2|32062|40062|50063|75064)0NS",
    "", "", ""
  },
  { "Seagate BarraCuda 2.5", // tested with ST2000LM015-2E8174/SDM1,
      // ST4000LM024-2AN17V/0001, ST5000LM000-2AN170/0001, ST1000LM049-2GH172/SDM1
      // 7200rpm: ST500LM034, ST1000LM049
    "ST(500LM03[04]|1000LM04[89]|2000LM015|[34]000LM024|5000LM000)-.*",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 "
    "-v 183,raw48,SATA_Downshift_Count "
    "-v 188,raw16"
  },
  { "Seagate Barracuda ES.2", // fixed firmware
    "ST3(25031|50032|75033|100034)0NS",
    "SN[01]6|"         // https://knowledge.seagate.com/articles/en_US/FAQ/207963en
    "MA(0[^7]|[^0].)",
    "",
    "-F xerrorlba" // tested with ST31000340NS/SN06
  },
  { "Seagate Barracuda ES.2", // buggy firmware (Dell)
    "ST3(25031|50032|75033|100034)0NS",
    "MA07",
    "There are known problems with these drives,\n"
    "AND THIS FIRMWARE VERSION IS AFFECTED,\n"
    "contact Dell support for a firmware update.",
    ""
  },
  { "Seagate Barracuda ES.2", // unknown firmware
    "ST3(25031|50032|75033|100034)0NS",
    "",
    "There are known problems with these drives,\n"
    "see the following Seagate web pages:\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207931en\n"
    "https://knowledge.seagate.com/articles/en_US/FAQ/207963en",
    ""
  },
  { "Seagate BarraCuda Pro", // tested with ST4000DM006-2G5107/DN02, ST8000DM0004-1ZC11G/DN01,
      // ST10000DM0004-1ZC101/DN01, // ST12000DM0007-2GR116/DN01
    "ST(2000DM009|4000DM006|6000DM004|8000DM00(5|04)|10000DM0004|12000DM0007)-.*",
    "", "",
    "-v 9,msec24hour32 -v 188,raw16 "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate Constellation (SATA)", // tested with ST9500530NS/SN03
    "ST9(160511|500530)NS",
    "", "", ""
  },
  { "Seagate Constellation ES (SATA)", // tested with ST31000524NS/SN11,
      // MB0500EAMZD/HPG1
    "ST3(50051|100052|200064)4NS|"
    "MB0500EAMZD", // HP OEM
    "", "", ""
  },
  { "Seagate Constellation ES (SATA 6Gb/s)", // tested with ST1000NM0011/SN02,
      // MB1000GCEEK/HPG1
    "ST(5|10|20)00NM0011|"
    "MB1000GCEEK", // HP OEM
    "", "", ""
  },
  { "Seagate Constellation ES.2 (SATA 6Gb/s)", // tested with ST32000645NS/0004, ST33000650NS,
      // "ST33000650NS         81Y9799 81Y3865IBM/BB3A", MB3000EBKAB/HPG6,
    "ST3(2000645|300065[012])NS( .*IBM)?|"
    "MB3000EBKAB", // HP OEM
    "", "", ""
  },
  { "Seagate Constellation ES.3", // tested with ST1000NM0033-9ZM173/0001,
      // ST4000NM0033-9ZM170/SN03, MB1000GCWCV/HPGC, MB4000GCWDC/HPGE
    "ST[1234]000NM00[35]3-.*|"
    "MB[14]000GCW(CV|DC)", // HP OEM
    "", "", ""
  },
  { "Seagate Constellation CS", // tested with ST3000NC000/CE02, ST3000NC002-1DY166/CN02
    "ST(1000|2000|3000)NC00[0-3](-.*)?",
    "", "", ""
  },
  { "Seagate Constellation.2 (SATA)", // 2.5", tested with ST91000640NS/SN02, MM1000GBKAL/HPGB
    "ST9(25061|50062|100064)[012]NS|" // *SS = SAS
    "MM1000GBKAL", // HP OEM
    "", "", ""
  },
  // ST6000NM0004, ST6000NM0024, ST6000NM0044, ST6000NM0084, ST5000NM0024,
  // ST5000NM0044, ST4000NM0024, ST4000NM0044, ST2000NM0024, ST2000NM0044
  // ST4000NM0035, ST3000NM0005, ST2000NM0055, ST1000NM0055, ST4000NM0045,
  // ST3000NM0015, ST2000NM0065, ST1000NM0065, ST4000NM0105, ST3000NM0055
  { "Seagate Enterprise Capacity 3.5 HDD", // tested with ST6000NM0024-1HT17Z/SN02,
      // ST10000NM0016-1TT101/SNB0
      // ST4000NM0085-1YY107/ZC11SXPH
      // ST8000NM0045-1RL112/NN02
      // ST6000NM0004-1FT17Z/NN01
      // ST4000NM0035-1V4107/TNC3
      // ST1000NM0055-1V410C/TN02
      // ST8000NM0055-1RM112/SN04
      // ST10000NM0156-2AA111/SS05, ST4000NM0245-1Z2107/SS05
    "ST([1234568]|10)000NM0[012][0-68][456]-.*", // *[069]4 = 4Kn
    "", "",
    "-v 200,raw48,Pressure_Limit "
    "-v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Enterprise Capacity 3.5 HDD", // V5.1, ms in attribute 9
    "ST[12]000NM0008-.*", // tested with ST1000NM0008-2F2100/SN01
    "", "",
    "-v 9,msec24hour32 -v 188,raw16 -v 240,msec24hour32"
  },
  { "Seagate Enterprise Capacity 3.5 HDD v7 SED", // tested with ST12000NM0127/G005
    "ST12000NM01[12]7",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 "
    "-v 195,raw24/raw32,Hardware_ECC_Recovered "
  },
  { "Seagate Exos 5E8", // tested with ST8000AS0003-2HH188/0003
    "ST8000AS0003-.*",
    "", "",
    "-v 9,msec24hour32 -v 240,msec24hour32"
  },
  // ST1000NM000A, ST1000NM002A, ST2000NM000A, ST2000NM001A, ST2000NM002A,
  // ST3000NM000A, ST3000NM004A, ST4000NM000A, ST4000NM001A, ST4000NM002A,
  // ST4000NM006A, ST4000NM010A, ST4000NM012A, ST4000NM013A, ST6000NM002A,
  // ST6000NM021A, ST6000NM022A, ST6000NM025A, ST6000NM026A, ST8000NM000A,
  // ST8000NM002A, ST8000NM004A, ST8000NM008A, ST8000NM009A, ST8000NM016A
  { "Seagate Exos 7E8", // tested with ST4000NM000A-2HZ100/TN03, ST6000NM021A-2R7101/SN02,
      // ST8000NM000A-2KE101/SN02, OOS6000G/OOS1
    "ST[123468]000NM0(0[01234689]|1[0236]|2[1256])A-.*|"
    "OOS6000G", // 6TB refurbished and rebranded
    "", "",
    "-v 18,raw48,Head_Health "
    "-v 188,raw16 "
    "-v 240,msec24hour32"
  },
  { "Seagate Exos X12", // tested with ST12000NM0007-2A1101/SN02
    "ST12000NM00[01]7-.*", // *17 = SED
    "", "",
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate Exos X14", // tested with ST12000NM0008-2H3101/SN02,
      // ST12000NM0538-2K2101/CMA2 (OEM?)
    "ST(14000NM04[24]8|14000NM0(01|25)8|12000NM0(00|24|53)8|10000NM0(47|56)8)-.*",
    "", "",
    "-v 18,raw48,Head_Health "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate Exos X16", // tested with ST10000NM001G-2MW103/SN02
      // ST14000NM001G-2KJ103/SN02, ST14000NM001G-2KJ1037/SN04, ST16000NM001G-2KK103/SN02,
      // ST16000NM001G-2KK103/SN03
    "ST1[0246]000NM00[13]G-.*",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 "
    "-v 18,raw48,Head_Health "
    "-v 188,raw16 "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate Exos X18", // tested with ST12000NM000J-2TY103/SN02,
      // ST16000NM000J-2TW103/SC02, ST18000NM000J-2TV103/SN01, .../SN02,
      // ST18000NM002J-2TV133/PAL7 (Dell)
    "ST1(0000NM0(18|20)G|[2468]000NM00[012]J)-.*",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 "
    "-v 18,raw48,Head_Health "
    "-v 188,raw16 "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate Exos X20/X22", // tested with ST20000NM007D-3DJ103/SN01, .../SN03,
      // ST22000NM001E-3HM103/SN03, OOS20000G/OOS1,
      // ST16000NM000D-3PC101/SN01 (re-certified),
      // ST16000NM000E-3NV101/ZZF1 (re-certified)
    "ST(16|18|20)000NM00[0347]D-.*|" // X20
    "ST(16|2[02])000NM00[01]E-.*|" // X22
    "OOS20000G", // 20TB refurbished and rebranded
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 "
    "-v 18,raw48,Head_Health "
    "-v 188,raw16 "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate Exos X24", // tested with ST24000NM002H-3KS133/SE03,
      // ST24000NM000C-3WD103/SN02 (30TB HAMR recertified to 24TB CMR ?)
    "ST((12|16|20|24)000NM002H|24000NM000C)-.*",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 "
    "-v 18,raw48,Head_Health "
    "-v 188,raw16 "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  // new models: ST8000VN0002, ST6000VN0021, ST4000VN000
  //             ST8000VN0012, ST6000VN0031, ST4000VN003
  // tested with ST8000VN0002-1Z8112/ZA13YGNF
  { "Seagate NAS HDD", // tested with ST2000VN000-1H3164/SC42, ST3000VN000-1H4167/SC43
    "ST([234]000VN000|[468]000VN00(02|21|12|31|3))-.*",
    "", "", ""
  },
  // ST8000NE0001, ST8000NE0011, ST6000VN0001, ST6000VN0011, ST5000VN0001,
  // ST5000VN0011, ST4000VN0001, ST4000VN0011, ST3000VN0001, ST3000VN0011,
  // ST2000VN0001, ST2000VN0011
  // tested with ST8000NE0001-1WN112/PNA2
  { "Seagate Enterprise NAS HDD",
    "ST(8000NE|[65432]000VN)00[01]1-.*",
    "", "", ""
  },
  { "Seagate IronWolf", // tested with ST2000VN003-3CW102/SC60, ST3000VN007-2E4166/SC60,
      // ST4000VN006-3CW104/SC60,
      // ST4000VN008-2DR166/SC60, ST6000VN001-2BB186/SC60, ST6000VN0033-2EE110/SC60,
      // ST6000VN0041-2EL11C/SC61, ST8000VN0022-2EL112/SC61, ST10000VN000-3AK101/SC60,
      // ST10000VN0004-1ZD101/SC60, ST10000VN0004-2GS11L/SC60, ST12000VN0007-2GS116/SC60,
      // ST12000VN0008-2JH101/SC60, ST16000VN001-2RV103/SC60
    "ST([123468]|1[0246])000VN00(0?[0234678]|1|22|33|41)-.*",
    "", "",
    "-v 18,raw48,Head_Health "
    "-v 188,raw16 "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate IronWolf Pro", // tested with ST4000NE0025-2EW107/EN02,
      // ST6000NE000-2KR101/EN01, ST8000NE001-2M7101/EN01, ST8000NE0004-1ZF11G/EN01,
      // ST8000NE0021-2EN112/EN02, ST12000NT001-3LX101/EN01, ST16000NE000-2RW103/EN02,
      // ST16000NT001-3LV101/EN01, ST18000NE000-3G6101/EN01, ST18000NT001-3LU101/EN01,
    "ST([24]000NE00([01]|25)|6000NE00(0|23)|8000NE00([01]|0[48]|21))-.*|"
    "ST(1[02468]|2[02])000NE(000[478]?)-.*|"
    "ST([2468]|1[02468]|2[02])000NT001-.*",
    "", "",
    "-v 18,raw48,Head_Health " // ST16000NE000, ST18000NT001
    "-v 188,raw16 "
    "-v 200,raw48,Pressure_Limit "
    "-v 240,msec24hour32"
  },
  { "Seagate Archive HDD (SMR)", // tested with ST8000AS0002-1NA17Z/AR13
    "ST[568]000AS00[01][12]-.*",
    "", "", ""
  },
  { "Seagate Pipeline HD 5900.1",
    "ST3(160310|320[34]10|500(321|422))CS",
    "", "", ""
  },
  { "Seagate Pipeline HD 5900.2", // tested with ST31000322CS/SC13
    "ST3(160316|250[34]12|320(311|413)|500(312|414)|1000(322|424))CS",
    "", "", ""
  },
  { "Seagate Video 3.5 HDD", // tested with ST4000VM000-1F3168/SC23, SC25
    "ST(10|15|20|30|40)00VM00[023]-.*",
    "", "", ""
  },
  { "Seagate Medalist 17240, 13030, 10231, 8420, and 4310",
    "ST3(17240|13030|10231|8420|4310)A",
    "", "", ""
  },
  { "Seagate Medalist 17242, 13032, 10232, 8422, and 4312",
    "ST3(1724|1303|1023|842|431)2A",
    "", "", ""
  },
  { "Seagate NL35",
    "ST3(250623|250823|400632|400832|250824|250624|400633|400833|500641|500841)NS",
    "", "", ""
  },
  { "Seagate SV35.2",
    "ST3(160815|250820|320620|500630|750640)[AS]V",
    "", "", ""
  },
  { "Seagate SV35.3", // tested with ST3500320SV/SV16
    "ST3(500320|750330|1000340)SV",
    "", "", ""
  },
  { "Seagate SV35.5", // tested with ST31000525SV/CV12
    "ST3(250311|500410|1000525)SV",
    "", "", ""
  },
  // ST6000VX0001,ST6000VX0011,ST5000VX0001,ST5000VX0011,ST4000VX000
  // ST4000VX002, ST3000VX002, ST2000VX003, ST1000VX001, ST1000VX002
  // ST3000VX000, ST3000VX004, ST2000VX000, ST2000VX004, ST1000VX000
  { "Seagate Surveillance", // tested with ST1000VX001-1HH162/CV11, ST2000VX000-9YW164/CV12,
      // ST4000VX000-1F4168/CV14, ST2000VX003-1HH164/CV12
    "ST([1-5]000VX00[01234]1?|31000526SV|3500411SV)(-.*)?",
    "", "", ""
  },
  { "Seagate SkyHawk", // tested with ST3000VX010-2H916L/CV11, ST4000VX016-3CV104/CV10,
      // ST6000VX0023-2EF110/SC60
    "ST(1000VX005|2000VX008|3000VX0(09|10)|4000VX0(07|16)|6000VX00(1|23)|8000VX00(4|22))-.*",
    "", "",
    "-v 9,msec24hour32 " // CV* Firmware only?
    "-v 240,msec24hour32"
  },
  { "Seagate DB35", // tested with ST3250823ACE/3.03, ST3300831SCE/3.03
    "ST3(200826|250823|300831|400832)[AS]CE",
    "", "", ""
  },
  { "Seagate DB35.2", // tested with ST3160212SCE/3.ACB
    "ST3(802110|120213|160212|200827|250824|300822|400833|500841)[AS]CE",
    "", "", ""
  },
  { "Seagate DB35.3",
    "ST3(750640SCE|((80|160)215|(250|320|400)820|500830|750840)[AS]CE)",
    "", "", ""
  },
  { "Seagate EE25.2", // tested with ST980818SM/3.AAB
    "ST9[3468]081[78][AS]M",
    "", "",
    "-v 7,raw24/raw32 "
    "-v 195,raw24/raw32,ECC_On_the_Fly_Count"
  },
  { "Seagate LD25.1", // tested with ST9402115AS/3.01
    "ST9(20217|402115)AS",
    "", "",
    "-v 1,raw24/raw32 -v 7,raw24/raw32 "
    "-v 195,raw24/raw32,ECC_On_the_Fly_Count"
  },
  { "Seagate LD25.2", // tested with ST940210AS/3.ALC
    "ST9(40|80)210AS?",
    "", "", ""
  },
  { "Seagate ST1.2 CompactFlash", // tested with ST68022CF/3.01
    "ST6[468]022CF",
    "", "", ""
  },
  { "Seagate Nytro XF1230 SATA SSD", // tested with XF1230-1A0480/ST200354
    "XF1230-1A(0240|0480|0960|1920)",
    "", "",
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 180,raw48,End_to_End_Err_Detect "
    "-v 183,raw48,SATA_Downshift_Count "
    "-v 189,raw48,SSD_Health_Flags "
    "-v 190,raw48,SATA_Error_Ct "
    "-v 201,raw48,Read_Error_Rate "
    "-v 231,raw48,SSD_Life_Left_Perc "
    "-v 234,raw48,Lifetime_Nand_Gb "
    "-v 241,raw48,Total_Writes_GiB "
    "-v 242,raw48,Total_Reads_GiB "
    "-v 245,raw48,Read_Error_Rate "
  },
  { "Seagate IronWolf 110 SATA SSD", //Written to Seagate documentation
    "ZA(240|480|960|1920|3840)NM10001",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 100,raw48,Flash_GB_Erased "
    "-v 102,raw48,Lifetime_PS4_Entry_Ct "
    "-v 103,raw48,Lifetime_PS3_Exit_Ct "
    "-v 170,raw48,Grown_Bad_Block_Ct "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Avg_Program/Erase_Ct "
    "-v 174,raw48,Unexpected_Pwr_Loss_Ct "
    "-v 177,raw16,Wear_Range_Delta "
    "-v 183,hex56,SATA_Downshift_Count "
    "-v 187,raw48,Uncorrectable_ECC_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw16(raw16),RAISE_ECC_Cor_Ct "
    "-v 198,raw48,Uncor_Read_Error_Ct "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 230,raw56,Drv_Life_Protect_Status "
    "-v 231,hex56,SSD_Life_Left "
  //"-v 232,raw48,Available_Reservd_Space "
    "-v 233,raw48,Lifetime_Wts_To_Flsh_GB "
    "-v 241,raw48,Lifetime_Wts_Frm_Hst_GB "
    "-v 242,raw48,Lifetime_Rds_Frm_Hst_GB "
    "-v 243,hex56,Free_Space "
  },
  { "Seagate IronWolf (Pro) 125 SSDs", // IronWolf_Pro_125_SSD_Product_Manual_100866982_A.pdf
                                       // IronWolf_125_SSD_Product_Manual_100866980_C.pdf
    "Seagate IronWolf ZA(250|500|1000|2000|4000)NM10002-.*|" // tested with
      // Seagate IronWolf ZA500NM10002-2ZG101/SU3SC013
    "Seagate IronWolfPro ZA(240|480|960|1920|3840)NX10001-.*", // tested with
      // Seagate IronWolfPro ZA3840NX10001-2ZH104/SU4SC01B
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 16,raw48,Spare_Blocks_Available "
    "-v 17,raw48,Spare_Blocks_Remaining "
    "-v 168,raw48,SATA_PHY_Error_Count "
    "-v 170,raw16,Early/Later_Bad_Blck_Ct "
    "-v 173,raw16,Max/Avg/Min_Erase_Ct "
    "-v 174,raw48,Unexpect_Power_Loss_Ct "
    "-v 177,raw16,Wear_Range_Delta "
  //"-v 192,raw48,Power-Off_Retract_Count "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 218,raw48,SATA_CRC_Error_Count "
    "-v 231,raw48,SSD_Life_Left "
    "-v 232,hex48,Read_Failure_Blk_Ct "
    "-v 233,raw48,Flash_Writes_GiB "
    "-v 234,raw48,NAND_Reads_Sectors "
    "-v 235,raw48,Flash_Writes_Sectors "
    "-v 241,raw48,Host_Writes_GiB "
    "-v 242,raw48,Host_Reads_GiB "
    "-v 246,hex64,Write_Protect_Detail " // prevents interpretation of bogus threshold 255 (ticket #1396)
    "-v 247,raw48,Health_Check_Timer "
  },
  { "Seagate Nytro SATA SSD", //Written to Seagate documentation
    // tested with XA960LE10063, XA960LE10063
    "XA(240|480|960|1920|3840)[LM]E10(00|02|04|06|08|10)3",
    "", "",
  //"-v 1,raw48,Raw_Read_Error_Rate "
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct "
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 100,raw48,Flash_GB_Erased "
    "-v 102,raw48,Lifetime_PS4_Entry_Ct "
    "-v 103,raw48,Lifetime_PS3_Exit_Ct "
    "-v 170,raw48,Grown_Bad_Block_Ct "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Avg_Program/Erase_Ct "
    "-v 174,raw48,Unexpected_Pwr_Loss_Ct "
    "-v 177,raw16,Wear_Range_Delta "
    "-v 183,hex56,SATA_Downshift_Count "
    "-v 187,raw48,Uncorrectable_ECC_Ct "
  //"-v 194,tempminmax,Temperature_Celsius "
    "-v 195,raw16(raw16),RAISE_ECC_Cor_Ct "
    "-v 198,raw48,Uncor_Read_Error_Ct "
  //"-v 199,raw48,UDMA_CRC_Error_Count "
    "-v 230,raw56,Drv_Life_Protect_Status "
    "-v 231,hex56,SSD_Life_Left "
  //"-v 232,raw48,Available_Reservd_Space "
    "-v 233,raw48,Lifetime_Wts_To_Flsh_GB "
    "-v 241,raw48,Lifetime_Wts_Frm_Hst_GB "
    "-v 242,raw48,Lifetime_Rds_Frm_Hst_GB "
    "-v 243,hex56,Free_Space "
  },
  { "WD Blue / Red / Green SSDs", // tested with WDC WDS250G1B0A-00H9H0/X41000WD,
      // WDC WDS250G1B0A-00H9H0/X41100WD, WDC WDS100T1B0A-00H9H0,
      // WDC WDS120G2G0A-00JH30/UE360000, WDC WDS240G2G0A-00JH30/UF300000,
      // WDC WDS500G2B0A-00SM50/X61130WD, WDC WDS200T2B0A-00SM50/X61130WD,
      // WDC WDS200T2B0A/X61190WD, WDC WDS120G1G0A-00SS50/Z3311000
      // WDC  WDS500G2B0A-00SM50/401000WD,
      // WDC WDBNCE2500PNC/X61130WD, WDC WDBNCE0010PNC-WRSN/X41110WD,
      // WDC  WDS200T1R0A-68A4W0/411000WR, WDC  WDS400T1R0A-68A4W0/411000WR
    "WDC WDBNCE(250|500|00[124])0PNC(-.*)?|" // Blue 3D
    "WDC  ?WDS((120|240|250|400|480|500)G|[124]00T)(1B|2B|1G|2G|[12]R)0[AB](-.*)?|"
      // *B* = Blue, *G* = Green, *2B* = Blue 3D NAND, *[12]R* = Red SA500
    "WD (Blue|Red) SA5[01]0 2\\.5 ((25|50|100)0G|[24]T)B|" // tested with
      // WD Blue SA510 2.5 1000GB/52008100, WD Blue SA510 2.5 4TB/530309WD,
      // WD Red SA500 2.5 4TB/540400WD,
      // WD Red SA500 2.5 4TB/540500WD (printed label: WDS400T2R0A-68CKB0)
    "SanDisk Portable SSD", // tested with SanDisk Portable SSD/UM5004RL
                            // (Sandisk SDSSDE30-2T00, 0x0781:0x55b0)
    "", "",
  //"-v 5,raw16(raw16),Reallocated_Sector_Ct " // Reassigned Block Count
  //"-v 9,raw24(raw8),Power_On_Hours "
  //"-v 12,raw48,Power_Cycle_Count "
    "-v 165,raw48,Block_Erase_Count "
    "-v 166,raw48,Minimum_PE_Cycles_TLC "
    "-v 167,raw48,Max_Bad_Blocks_per_Die "
    "-v 168,raw48,Maximum_PE_Cycles_TLC "
    "-v 169,raw48,Total_Bad_Blocks "
    "-v 170,raw48,Grown_Bad_Blocks "
    "-v 171,raw48,Program_Fail_Count "
    "-v 172,raw48,Erase_Fail_Count "
    "-v 173,raw48,Average_PE_Cycles_TLC "
    "-v 174,raw48,Unexpected_Power_Loss "
  //"-v 184,raw48,End-to-End_Error " // Detection/Correction Count
  //"-v 187,raw48,Reported_Uncorrect " // Uncorrectable Errors
  //"-v 188,raw48,Command_Timeout "
  //"-v 194,tempminmax,Temperature_Celsius "
  //"-v 199,raw48,UDMA_CRC_Error_Count " // SATA CRC Errors
    "-v 230,hex48,Media_Wearout_Indicator " // Maybe hex16
  //"-v 232,raw48,Available_Reservd_Space"
    "-v 233,raw48,NAND_GB_Written_TLC "
    "-v 234,raw48,NAND_GB_Written_SLC "
    "-v 241,raw48,Host_Writes_GiB "
    "-v 242,raw48,Host_Reads_GiB "
    "-v 244,raw48,Temp_Throttle_Status "
  },
  { "Western Digital Protege",
  /* Western Digital drives with this comment all appear to use Attribute 9 in
   * a  non-standard manner.  These entries may need to be updated when it
   * is understood exactly how Attribute 9 should be interpreted.
   * UPDATE: this is probably explained by the WD firmware bug described in the
   * smartmontools FAQ */
    "WDC WD([2468]00E|1[26]00A)B-.*",
    "", "", ""
  },
  { "Western Digital Caviar",
  /* Western Digital drives with this comment all appear to use Attribute 9 in
   * a  non-standard manner.  These entries may need to be updated when it
   * is understood exactly how Attribute 9 should be interpreted.
   * UPDATE: this is probably explained by the WD firmware bug described in the
   * smartmontools FAQ */
    "WDC WD(2|3|4|6|8|10|12|16|18|20|25)00BB-.*",
    "", "", ""
  },
  { "Western Digital Caviar WDxxxAB",
  /* Western Digital drives with this comment all appear to use Attribute 9 in
   * a  non-standard manner.  These entries may need to be updated when it
   * is understood exactly how Attribute 9 should be interpreted.
   * UPDATE: this is probably explained by the WD firmware bug described in the
   * smartmontools FAQ */
    "WDC WD(3|4|6|8|25)00AB-.*",
    "", "", ""
  },
  { "Western Digital Caviar WDxxxAA",
  /* Western Digital drives with this comment all appear to use Attribute 9 in
   * a  non-standard manner.  These entries may need to be updated when it
   * is understood exactly how Attribute 9 should be interpreted.
   * UPDATE: this is probably explained by the WD firmware bug described in the
   * smartmontools FAQ */
    "WDC WD...?AA(-.*)?",
    "", "", ""
  },
  { "Western Digital Caviar WDxxxBA",
  /* Western Digital drives with this comment all appear to use Attribute 9 in
   * a  non-standard manner.  These entries may need to be updated when it
   * is understood exactly how Attribute 9 should be interpreted.
   * UPDATE: this is probably explained by the WD firmware bug described in the
   * smartmontools FAQ */
    "WDC WD...BA",
    "", "", ""
  },
  { "Western Digital Caviar AC", // add only 5400rpm/7200rpm (ata33 and faster)
    "WDC AC((116|121|125|225|132|232)|([1-4][4-9][0-9])|([1-4][0-9][0-9][0-9]))00[A-Z]?.*",
    "", "", ""
  },
  { "Western Digital Caviar SE",
  /* Western Digital drives with this comment all appear to use Attribute 9 in
   * a  non-standard manner.  These entries may need to be updated when it
   * is understood exactly how Attribute 9 should be interpreted.
   * UPDATE: this is probably explained by the WD firmware bug described in the
   * smartmontools FAQ
   * UPDATE 2: this does not apply to more recent models, at least WD3200AAJB */
    "WDC WD(4|6|8|10|12|16|18|20|25|30|32|40|50)00(JB|PB)-.*",
    "", "", ""
  },
  { "Western Digital Caviar Blue EIDE",  // WD Caviar SE EIDE
    /* not completely accurate: at least also WD800JB, WD(4|8|20|25)00BB sold as Caviar Blue */
    "WDC WD(16|25|32|40|50)00AAJB-.*",
    "", "", ""
  },
  { "Western Digital Caviar Blue EIDE",  // WD Caviar SE16 EIDE
    "WDC WD(25|32|40|50)00AAKB-.*",
    "", "", ""
  },
  { "Western Digital RE EIDE",
    "WDC WD(12|16|25|32)00SB-.*",
    "", "", ""
  },
  { "Western Digital PiDrive Foundation Edition", // WDC WD3750LMCW-11D9GS3
    "WDC WD(3750|2500)LMCW-.*",
    "", "", ""
  },
  { "Western Digital Caviar Serial ATA",
    "WDC WD(4|8|20|32)00BD-.*",
    "", "", ""
  },
  { "Western Digital Caviar SE Serial ATA", // tested with WDC WD3000JD-98KLB0/08.05J08
    "WDC WD(4|8|12|16|20|25|30|32|40)00(JD|KD|PD)-.*",
    "", "", ""
  },
  { "Western Digital Caviar SE Serial ATA",
    "WDC WD(8|12|16|20|25|30|32|40|50)00JS-.*",
    "", "", ""
  },
  { "Western Digital Caviar SE16 Serial ATA",
    "WDC WD(16|20|25|32|40|50|75)00KS-.*",
    "", "", ""
  },
  { "Western Digital Caviar Blue Serial ATA",  // WD Caviar SE Serial ATA
    /* not completely accurate: at least also WD800BD, (4|8)00JD sold as Caviar Blue */
    "WDC WD((8|12|16|25|32)00AABS|(8|12|16|25|32|40|50)00AAJS)-.*",
    "", "", ""
  },
  { "Western Digital Caviar Blue (SATA)",  // WD Caviar SE16 Serial ATA
      // tested with WD1602ABKS-18N8A0/DELL/02.03B04
    "WDC WD((16|20|25|32|40|50|64|75)00AAKS|1602ABKS|10EALS)-.*",
    "", "", ""
  },
  { "Western Digital Blue (CMR)", // tested with WDC WD5000AZLX-00K4KA0/80.00A80,
      // WDC WD10EZEX-00RKKA0/80.00A80, WDC WD10EZEX-75M2NA0/01.01A01,
      // WDC WD40EZRZ-00WN9B0/80.00A80, WDC WD80EAZZ-00BKLB0/80.00A80,
      // APPLE HDD WDC WD10EALX-408EA0/07.01D03
    "(APPLE HDD )?WDC WD((25|32|50)00AAKX|5000AZ(LX|RZ)|7500A(AL|ZE)X|[123468]0E(ALX|A[ARZ]Z|Z[AE]X|ZRZ))-.*",
    "", "", ""
  },
  { "Western Digital Blue (SMR)", // tested with WDC WD40EZAZ-00SF3B0/80.00A80 (TRIM: zeroed)
    "WDC WD[2346]0EZ(AZ|BX)-.*",
    "", "", ""
  },
  { "Western Digital RE Serial ATA",
    "WDC WD(12|16|25|32)00(SD|YD|YS)-.*",
    "", "", ""
  },
  { "Western Digital RE2 Serial ATA",
    "WDC WD((40|50|75)00(YR|YS|AYYS)|(16|32|40|50)0[01]ABYS)-.*",
    "", "", ""
  },
  { "Western Digital RE2-GP",
    "WDC WD(5000AB|7500AY|1000FY)PS-.*",
    "", "", ""
  },
  { "Western Digital RE3 Serial ATA", // tested with WDC WD7502ABYS-02A6B0/03.00C06,
      // WD1002FBYS-12/03.M0300
    "(WDC )?WD((25|32|50|75)02A|(75|10)02F)BYS-.*",
    "", "", ""
  },
  { "Western Digital RE4", // tested with WDC WD2003FYYS-18W0B0/01.01D02,
      // WDC WD1003FBYZ-010FB0/01.01V03
      // WDC WD5003ABYZ-011FA0/01.01S03
    "WDC WD((25|50)03ABY[XZ]|1003FBY[XZ]|(15|20)03FYYS)-.*",
    "", "", ""
  },
  { "Western Digital RE4-GP", // tested with WDC WD2002FYPS-02W3B0/04.01G01,
      // WD2003FYPS-27W9B0/01.01D02
    "(WDC )?WD200[23]FYPS-.*",
    "", "", ""
  },
  { "Western Digital Re", // tested with WDC WD1004FBYZ-01YCBB0/RR02,
      // WDC WD2000FYYZ-01UL1B0/01.01K01, WDC WD2000FYYZ-01UL1B1/01.01K02,
      // WDC WD4000FYYZ-01UL1B2/01.01K03, WD2000FYYX/00.0D1K2,
      // WDC WD1004FBYZ-01YCBB1/RR04
      // WD4000FYYZ, WD4000FDYZ, WD3000FYYZ, WD3000FDYZ, WD2000FYYZ, WD2000FDYZ
      // WD2004FBYZ, WD1004FBYZ
    "WDC WD((1004|2004)FBYZ|([234]000)FDYZ|[234]000FYYZ|2000FYYX)-.*",
    "", "",
    "-v 16,raw48,Total_LBAs_Read" // WDC WD1004FBYZ-01YCBB1/RR04
  },
  { "Western Digital Re+", // tested with WDC WD6005FRPZ-01S9PB0/01.0RRE1
    "WDC WD[56]005FRPZ-.*",
    "", "",
    "-v 16,raw48,Unknown_WDC_Attribute" // WDC WD6005FRPZ-01S9PB0/01.0RRE1
  },
  { "Western Digital Se", // tested with WDC WD2000F9YZ-09N20L0/01.01A01
    // WD6001F9YZ, WD5001F9YZ, WD4000F9YZ, WD3000F9YZ, WD2000F9YZ, WD1002F9YZ
    "WDC WD(1002|2000|3000|4000|5001|6001)F9YZ-.*",
    "", "", ""
  },
  { "Western Digital Caviar Green", // tested with WDC WD7500AADS-00M2B0/01.00A01,
      // WDC WD10EADX/77.04D77
    "WDC WD((50|64|75)00AA[CV]S|(50|64|75)00AADS|10EA[CV]S|(10|15|20)EAD[SX])-.*",
    "",
    "",
    "-F xerrorlba" // tested with WDC WD7500AADS-00M2B0/01.00A01
  },
  { "Western Digital Caviar Green (AF)",
    "WDC WD(((64|75|80)00AA|(10|15|20)EA|(25|30)EZ)R|20EAC)S-.*",
    "", "", ""
  },
  { "Western Digital Green", // tested with
      // WDC WD10EZRX-00A8LB0/01.01A01, WDC WD20EZRX-00DC0B0/80.00A80,
      // WDC WD30EZRX-00MMMB0/80.00A80, WDC WD40EZRX-00SPEB0/80.00A80,
      // WDC WD60EZRX-00MVLB1/80.00A80, WDC WD5000AZRX-00A8LB0/01.01A01
    "WDC WD(5000AZ|7500AA|(10|15|20)EA|(10|20|25|30|40|50|60)EZ)RX-.*",
    "", "", ""
  },
  { "Western Digital Caviar Black", // tested with WDC WD7501AAES/06.01D06
    "WDC WD((500|640)1AAL|7501AA[EL]|1001FA[EL]|2001FAS)S-.*|"
    "WDC WD(2002|7502|1502|5003|1002|5002)(FAE|AAE|AZE|AAL)X-.*", // could be
    // WD2002FAEX, WD7502AAEX, WD1502FAEX, WD5003AZEX, WD1002FAEX, WD5002AALX
    "", "", "-F xerrorlba" // WDC WD6401AALS-00L3B2/01.03B01 (ticket #1558)
  },
  { "Western Digital Black", // tested with
      // WDC WD1003FZEX-00MK2A0/01.01A01, WDC WD3001FAEX-00MJRA0/01.01L01,
      // WDC WD3003FZEX-00Z4SA0/01.01A01, WDC WD4001FAEX-00MJRA0/01.01L01
      // WDC WD4003FZEX-00Z4SA0/01.01A01, WDC WD5003AZEX-00RKKA0/80.00A80,
      // WDC WD4004FZWX-00GBGB0/81.H0A81, WDC WD4005FZBX-00K5WB0/01.01A01
    "WDC WD(6001|2003|5001|1003|4003|4004|4005|5003|3003|3001)(FZW|FZE|FZB|AZE)X-.*|" // could be
    // new series  WD6001FZWX WD2003FZEX WD5001FZWX WD1003FZEX
    //             WD4003FZEX WD5003AZEX WD3003FZEX WD4004FZWX
    "WDC WD(4001|3001|2002|1002|5003|7500|5000|3200|2500|1600)(FAE|AZE)X-.*",
    // old series: WD4001FAEX WD3001FAEX WD2002FAEX WD1002FAEX  WD5003AZEX
    "", "", ""
  },
  { "Western Digital Black (SMR)", // ticket #1313
    "WDC WD10SPSX-.*",
    "", "", ""
  },
  { "Western Digital AV ATA", // tested with WDC WD3200AVJB-63J5A0/01.03E01
    "WDC WD(8|16|25|32|50)00AV[BJ]B-.*",
    "", "", ""
  },
  { "Western Digital AV SATA",
    "WDC WD(16|25|32)00AVJS-.*",
    "", "", ""
  },
  { "Western Digital AV-GP",
    "WDC WD((16|25|32|50|64|75)00AV[CDV]S|(10|15|20)EV[CDV]S)-.*",
    "", "", ""
  },
  { "Western Digital AV-GP (AF)", // tested with WDC WD10EURS-630AB1/80.00A80,
      // WDC WD10EUCX-63YZ1Y0/51.0AB52, WDC WD20EURX-64HYZY0/80.00A80
    "WDC WD(5000AUDX|7500AURS|10EUCX|(10|15|20|25|30)EUR[SX])-.*",
    "", "", ""
  },
  { "Western Digital AV", // tested with DC WD10JUCT-63CYNY0/01.01A01
    "WDC WD((16|25|32|50)00BU[CD]|5000LUC|10JUC)T-.*",
    "", "", ""
  },
  { "Western Digital Raptor",
    "WDC WD((360|740|800)GD|(360|740|800|1500)ADF[DS])-.*",
    "", "", ""
  },
  { "Western Digital Raptor X",
    "WDC WD1500AHFD-.*",
    "", "", ""
  },
  { "Western Digital VelociRaptor", // tested with WDC WD1500HLHX-01JJPV0/04.05G04
    "WDC WD(((800H|(1500|3000)[BH]|1600H|3000G)LFS)|((1500|3000|4500|6000)[BH]LHX))-.*",
    "", "", ""
  },
  { "Western Digital VelociRaptor (AF)", // tested with WDC WD1000DHTZ-04N21V0/04.06A00
    "WDC WD(2500H|5000B|5000H|1000D)HTZ-.*",
    "", "", ""
  },
  { "Western Digital Scorpio EIDE",
    "WDC WD(4|6|8|10|12|16)00(UE|VE)-.*",
    "", "", ""
  },
  { "Western Digital Scorpio Blue EIDE", // tested with WDC WD3200BEVE-00A0HT0/11.01A11
    "WDC WD(4|6|8|10|12|16|25|32)00BEVE-.*",
    "", "", ""
  },
  { "Western Digital Scorpio Serial ATA",
    "WDC WD(4|6|8|10|12|16|25)00BEAS-.*",
    "", "", ""
  },
  { "Western Digital Scorpio Blue Serial ATA", // tested with WDC WD3200BEVS-08VAT2/14.01A14
    "WDC WD((4|6|8|10|12|16|25|32)00BEVS|(8|12|16|25|32|40|50|64)00BEVT|7500KEVT|10TEVT)-.*",
    "", "", ""
  },
  { "Western Digital Scorpio Blue Serial ATA (AF)", // tested with
      // WDC WD10JPVT-00A1YT0/01.01A01
    "WDC WD((16|25|32|50|64|75)00BPVT|10[JT]PVT)-.*",
    "", "", ""
  },
  { "Western Digital Scorpio Black", // tested with WDC WD5000BEKT-00KA9T0/01.01A01
    "WDC WD(8|12|16|25|32|50)00B[EJ]KT-.*",
    "", "", ""
  },
  { "Western Digital Scorpio Black (AF)",
    "WDC WD(50|75)00BPKT-.*",
    "", "", ""
  },
  { "Western Digital Red (CMR)", // tested with // WDC WD80EZZX-11CSGA0/83.H0A03 (My Book 0x1058:0x25ee),
      // WDC WD120EMFZ-11A6JA0/81.00A81 (Easystore 0x1058:0x25fb)
      // WDC WD160EMFZ-11AFXA0/81.00A81,
    "WDC WD(7500BFCX|80EZZX|1[26]0EMFZ)-.*",
    "", "", ""
  //"-v 22,raw48,Helium_Level" // WD120EMFZ, WD160EMFZ
  },
  { "Western Digital Red (SMR)", // ticket #1313, tested with WDC WD60EFAX-68SHWN0/82.00A82
    "WDC WD[2346]0EFAX-.*",
    "", "", ""
  },
  { "Western Digital Red Plus", // tested with WDC WD80EFAX-68LHPN0/83.H0A83.
      // WDC WD10JFCX-68N6GN0/01.01A01, WDC WD20EFZX-68AWUN0/81.00B81,
      // WDC WD30EFRX-68EUZN0/82.00A82, WDC WD30EFZX-68AWUN0/81.00B81,
      // WDC WD40EFPX-68C6CN0/81.00A81, WDC WD40EFRX-68WT0N0/80.00A80,
      // WDC WD40EFZX-68AWUN0/81.00B81,
      // WDC WD60EFRX-68MYMN1/82.00A82, WDC WD60EFPX-68C5ZN0/81.00A81,
      // WDC WD80EFZX-68UW8N0/83.H0A83, WDC WD10EFRX-68JCSN0/01.01A01
      // WDC WD80EFBX-68AZZN0/85.00A85, WDC WD101EFAX-68LDBN0/81.00A81,
      // WDC WD101EFBX-68B0AN0/85.00A85, WDC WD100EFAX-68LHPN0/83.H0A83,
      // WDC WD120EFAX-68UNTN0/81.00A81, WDC WD120EFBX-68B0EN0/85.00A85,
      // WDC WD140EFFX-68VBXN0/81.00A81
    "WDC WD(10JFCX|[1-6]0EFRX|[2-8]0EFPX|[23468]0E[FZ](ZX|ZZ)|(80|10[01]|1[24]0|1[68]1)(JFC|EF[ABFRG])X)-.*",
    "", "", ""
  //"-v 22,raw48,Helium_Level" // WD80EFAX, WD80EFZX, WD100EFAX, >= 12TB
  },
  { "Western Digital Red Pro", // tested with WDC WD2001FFSX-68JNUN0/81.00A81,
      // WDC WD6002FFWX-68TZ4N0/83.H0A83, WDC WD101KFBX-68R56N0/83.H0A03,
      // WDC WD102KFBX-68M95N0/83.00A83, WDC WD121KFBX-68EF5N0/83.00A83,
      // WDC WD141KFGX-68FH9N0/83.00A83, WDC WD142KFGX-68AFPN0/83.00A83,
      // WDC WD161KFGX-68AFPN0/83.00A83, WDC WD181KFGX-68AFPN0/83.00A83,
      // WDC WD201KFGX-68BKJN0/83.00A83, WDC WD4005FFBX-68CAUN0/83.00A83
    "WDC WD([2-68]00[1235]FF[BSW]|1[02][12]KFB|(1[468]|20)[12]KFG)X-.*",
    "", "",
  //"-v 22,raw48,Helium_Level " // not WD102KFBX
    "-v 90,hex48,NAND_Master" // WD201KFGX
  },
  { "Western Digital Purple (Pro)", // tested with WDC WD40PURX-64GVNY0/80.00A80,
      // WDC WD40PURZ-85TTDY0/80.00A80
      // WDC WD80PUZX-64NEAY0/80.H0A80
      // WDC WD121PURP-85B5SY0/82.00A82
    "WDC WD[1234568](0|[0248]1)PU[RZ][PXZ]-.*",
    "", "", ""
  //"-v 22,raw48,Helium_Level" // WD121PURP-85B5SY0, WD80PUZX-64NEAY0
  },
  { "Western Digital Gold", // tested with WDC WD1005FBYZ-01YCBB2/RR07,
      // WDC WD1005VBYZ-02RRWB2/RR07, WDC WD2005VBYZ-02RRWB2/RR07
      // WDC WD2005FBYZ-01YCBB2/RR07, WDC WD4002FYYZ-01B7CB0/01.01M02,
      // WDC WD4003FRYZ-01F0DB0/01.01H01, WDC WD6003FRYZ-01F0DB0/01.01H01,
      // WDC WD8003FRYZ-01JPDB1/01.01H02, WDC WD8004FRYZ-01VAEB0/01.01H01,
      // WDC WD102KRYZ-01A5AB0/01.01H01, WDC WD121KRYZ-01W0RB0/01.01H01,
      // WDC WD141KRYZ-01C66B0/01.01H01, WDC WD161KRYZ-01AGBB0/01.01H01
    "WDC WD([12]005[FV]B|4002FY|4003FR|600[23]FR|800[234]FR|([12][02468]1|102)KR)YZ-.*",
    "", "", ""
  //"-v 22,raw48,Helium_Level" // WD121KRYZ, WD141KRYZ
  },
  { "Western Digital Blue Mobile", // tested with WDC WD5000LPVX-08V0TT2/03.01A03,
      // WDC WD10JPVX-75JC3T0/0301A03,  WDC WD10JPVX-22JC3T0/01.01A01,
      // WDC WD20NPVZ-00WFZT0/01.01A01
    "WDC WD(3200LPCX|5000[BL]P[CV]X|7500BPVX|10JP[VZ]X|(15|20)NPVZ)-.*",
    "", "", ""
  },
  { "Western Digital Blue Mobile (SMR)", // ticket #1313, tested with
      // WDC WD10SPZX-22Z10T0/01.01A01, WDC WD10SPZX-21Z10T0/02.01A02,
      // WDC WD20SPZX-22CRAT0/01.01A01, WDC WD20SPZX-22UA7T0/01.01A01
    "WDC WD[12]0SPZX-.*",
    "", "", ""
  },
  { "Western Digital Green Mobile", // tested with WDC WD20NPVX-00EA4T0/01.01A01
    "WDC WD(15|20)NPV[TX]-.*",
    "", "", ""
  },
  { "Western Digital Black Mobile", // tested with WDC WD7500BPKX-22HPJT0/01.01A01,
      // WDC WD10JPLX-00MBPT0/01.01H01
    "WDC WD((16|25|32)00BEK[TX]|(25|32|50|75)00(BPK|LPL)X|10JPLX)-.*",
    "", "", ""
  },
  { "Western Digital Elements / My Passport (USB)", // tested with WDC WD5000BMVW-11AMCS0/01.01A01
    "WDC WD(25|32|40|50)00BMV[UVW]-.*",  // *W-* = USB 3.0
    "", "", ""
  },
  { "Western Digital Elements / My Passport (USB, AF)", // tested with
      // WDC WD5000KMVV-11TK7S1/01.01A01,
      // WDC WD5000LMVW-11CKRS0/01.01A01 (0x1058:0x07ae),
      // WDC WD5000LMVW-11VEDS0/01.01A01 (0x1058:0x0816),
      // WDC WD7500BMVW-11AJGS2/01.01A01,
      // WDC WD10JMVW-11AJGS2/01.01A01 (0x1058:0x10b8),
      // WDC WD10JMVW-11AJGS4/01.01A01 (0x1058:0x25a0/25a2),
      // WDC WD10JMVW-11S5XS1/01.01A01,
      // WDC WD10SMZW-11Y0TS0/01.01A01,
      // WDC WD10TMVW-11ZSMS5/01.01A01,
      // WDC WD20NMVW-11AV3S2/01.01A01 (0x1058:0x0822),
      // WDC WD20NMVW-11AV3S3/01.01A01 (0x1058:0x0837),
      // WDC WD20NMVW-11EDZS6/01.01A01 (0x1058-0x259f),
      // WDC WD20NMVW-11EDZS7/01.01A01 (0x1058:0x259d/25a1),
      // WDC WD20NMVW-11W68S0/01.01A01,
      // WDC WD20NMVW-59AV3S3/01.01A01 (0x1058:0x107d),
      // WDC WD30NMVW-11C3NS4/01.01A01,
      // WDC WD40NMZW-11GX6S1/01.01A01 (0x1058:0x2599/25e2/25fa)
      // WDC WD50NDZW-11A8JS1/01.01A01 (0x1058:0x2627)
      // WDC WD50NDZW-11MR8S1/02.01A02
      // WDC WD40NDZM-59A8KS1/01.01A01
    "WDC WD((5000[LK]|7500[BK]|10[JST]|[234]0N)M|50ND|40ND)[VZ][VWM]-.*", // *W-* = USB 3.0
    // Model numbers with "M" suffix denote the use of USB-C receptacles instead of Micro-B.
    "", "", ""
  },
  { "Quantum Bigfoot", // tested with TS10.0A/A21.0G00, TS12.7A/A21.0F00
    "QUANTUM BIGFOOT TS(10\\.0|12\\.7)A",
    "", "", ""
  },
  { "Quantum Fireball lct15",
    "QUANTUM FIREBALLlct15 ([123]0|22)",
    "", "", ""
  },
  { "Quantum Fireball lct20",
    "QUANTUM FIREBALLlct20 [1234]0",
    "", "", ""
  },
  { "Quantum Fireball CX",
    "QUANTUM FIREBALL CX10.2A",
    "", "", ""
  },
  { "Quantum Fireball CR",
    "QUANTUM FIREBALL CR(4.3|6.4|8.4|13.0)A",
    "", "", ""
  },
  { "Quantum Fireball EX", // tested with QUANTUM FIREBALL EX10.2A/A0A.0D00
    "QUANTUM FIREBALL EX(3\\.2|6\\.4|10\\.2)A",
    "", "", ""
  },
  { "Quantum Fireball ST",
    "QUANTUM FIREBALL ST(3.2|4.3|4300)A",
    "", "", ""
  },
  { "Quantum Fireball SE",
    "QUANTUM FIREBALL SE4.3A",
    "", "", ""
  },
  { "Quantum Fireball Plus LM",
    "QUANTUM FIREBALLP LM(10.2|15|20.[45]|30)",
    "", "", ""
  },
  { "Quantum Fireball Plus AS",
    "QUANTUM FIREBALLP AS(10.2|20.5|30.0|40.0|60.0)",
    "", "", ""
  },
  { "Quantum Fireball Plus KX",
    "QUANTUM FIREBALLP KX27.3",
    "", "", ""
  },
  { "Quantum Fireball Plus KA",
    "QUANTUM FIREBALLP KA(9|10).1",
    "", "", ""
  },

  ////////////////////////////////////////////////////
  // USB ID entries
  ////////////////////////////////////////////////////

  // 0x0080 (JMicron/Toshiba ?)
  { "USB: ; JMicron JMS578",
    "0x0080:0x0578",
    "", // 0x0104
    "",
    "-d sat"
  },
  { "USB: ; ",
    "0x0080:0xa001",
    "", // ORICO 2588US3: 0x0101, 0x0203
    "",
    "-d sat"
  },
  // Blueendless
  { "USB: Blueendless; Initio",
    "0x0204:0x3639", // U23QC
    "",
    "",
    "-d sat"
  },
  // 0x0350 (?)
  { "USB: ViPowER USB3.0 Storage; ",
    "0x0350:0x0038",
    "", // 0x1905
    "",
    "-d sat,12" // ATA output registers missing
  },
  // Hewlett-Packard
  { "USB: HP Personal Media Drive; ",
    "0x03f0:0x070c",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: HP x911w; ",
    "0x03f0:0x0c5c",
    "",
    "",
     "-d sat"
  },
  { "USB: HP Desktop HD BD07; ", // 2TB
    "0x03f0:0xbd07",
    "",
    "",
    "-d sat"
  },
  // ALi
  { "USB: ; ALi M5621", // USB->PATA
    "0x0402:0x5621",
    "",
    "",
    "" // unsupported
  },
  // VIA
  { "USB: Connectland BE-USB2-35BP-LCM; VIA VT6204",
    "0x040d:0x6204",
    "",
    "",
    "" // unsupported
  },
  // Buffalo / Melco
  { "USB: Buffalo; ",
    "0x0411:0x0(157|181|1ce|1[df]9|1e[7a]|240|251|27e)", // 0x0157: HD-PEU2, 0x0181: HD-PVU2,
      // 0x01ce: Duo, 0x01d9: HD-PCTU2 (0x0108), 0x01e7: HD-PNTU3, 0x01ea: HD-LBU2,
      // 0x01f9: HD-PZU3 (0x0100), 0x0240: HD-PCFU3, 0x0251: HD-PNFU3, 0x027e: HD-LC3
    "",
    "",
    "-d sat"
  },
  { "USB: Buffalo SSD-PSTA/N; ASMedia",
    "0x0411:0x039d",
    "",
    "",
    "-d sntasmedia"
  },
  // LG Electronics
  { "USB: LG Mini HXD5; JMicron",
    "0x043e:0x70f1",
    "", // 0x0100
    "",
    "-d usbjmicron"
  },
  // Hitachi / Renesas
  { "USB: ; Renesas uPD720231A", // USB2/3->SATA
    // 0x0229: Pi-102 Raspberry Pi USB to mSATA Converter Board
    // 0x022a: DeLock 62652 converter SATA 6GB/s > USB 3.0
    "0x045b:0x022[9a]",
    "",
    "",
    "-d sat"
  },
  // Philips
  { "USB: Philips; ", // SDE3273FC/97 2.5" SATA HDD enclosure
    "0x0471:0x2021",
    "", // 0x0103
    "",
    "-d sat"
  },
  // Toshiba
  { "USB: Toshiba Canvio 500GB; SunPlus",
    "0x0480:0xa004",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: Toshiba; ",
    "0x0480:0x....",
    "",
    "",
    "-d sat"
  },
  // Cypress
  { "USB: ; Cypress CY7C68300A (AT2)",
    "0x04b4:0x6830",
    "0x0001",
    "",
    "" // unsupported
  },
  { "USB: ; Cypress CY7C68300B/C (AT2LP)",
    "0x04b4:0x6830",
    "0x0240",
    "",
    "-d usbcypress"
  },
  // Fujitsu
  { "USB: Fujitsu; ",
    "0x04c5:0x(11bc|201d|2028)", "", // 0x11bc (0x0101), 0x201d: DeLock 42475 (0x0001),
    "", // 0x2028: Zalman ZM-VE300 (0x0001)
    ""
    "-d sat"
  },
  // Myson Century
  { "USB: ; Myson Century CS8818",
    "0x04cf:0x8818",
    "", // 0xb007
    "",
    "" // unsupported
  },
  // Samsung
  { "USB: Samsung S2 Portable; JMicron",
    "0x04e8:0x1f0[568a]", // 0x1f0a: SAMSUNG HN-M101XBB
    "",
    "",
    "-d usbjmicron" // 0x1f0a: works also with "-d sat"
  },
  { "USB: Samsung S1; JMicron",
    "0x04e8:0x2f0[36]", // 0x2f03: S1 Portable, 0x2f06: S1 Mini (SAMSUNG HS20YJZ/3AU10-01)
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: Samsung Portable SSD T7; ASMedia ASM2362",
    "0x04e8:0x(4001|61fb)", // 0x61fb: T7 Shield
    "", // 0x0100
    "",
    "-d sntasmedia"
  },
  { "USB: Samsung Story Station; ",
    "0x04e8:0x5f0[56]",
    "",
    "",
    "-d sat"
  },
  { "USB: Samsung G2 Portable; JMicron",
    "0x04e8:0x6032",
    "0x0000",
    "",
    "-d usbjmicron" // ticket #132
  },
  { "USB: Samsung G2 Portable; ",
    "0x04e8:0x6032",
    "0x...[1-9]", // >= 0x0001
    "",
    "-d sat"
  },
  { "USB: Samsung Story Station 3.0; ",
    "0x04e8:0x6052",
    "",
    "",
    "-d sat"
  },
  { "USB: Samsung Story Station 3.0; ",
    "0x04e8:0x6054",
    "",
    "",
    "-d sat"
  },
  { "USB: Samsung M2 Portable 3.0; ",
    "0x04e8:0x60c5",
    "",
    "",
    "-d sat"
  },
  { "USB: Samsung D3 Station; ",
    "0x04e8:0x612[45]", // 3TB, 4TB
    "", // 0x200, 0x202
    "",
    "-d sat"
  },
  { "USB: Samsung M3 Portable USB 3.0; ", // 1.5/2TB: SpinPoint M9TU
    "0x04e8:0x61b[3456]", // 500MB, 2TB, 1.5TB, 1TB
    "", // 0x0e00
    "",
    "-d sat"
  },
  { "USB: Samsung S3 Portable; ",
    "0x04e8:0x61c8", // ST1000LM025 HN-M101ABB
    "", // 0x1301
    "",
    "-d sat"
  },
  { "USB: Samsung Portable SSD T5; ",
    "0x04e8:0x61f5",
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: Samsung Portable SSD T9; ASMedia ASM2362",
    "0x04e8:0x61fd",
    "", // 0x0100
    "",
    "-d sntasmedia"
  },
  { "USB: Samsung; ",
    "0x04e8:0x8003", // USB3 Adapter from SSD EVO 850 Starter Kit
    "", // 0x0100
    "",
    "-d sat"
  },
  // Sony
  { "USB: Sony HD-E1; ",
    "0x054c:0x05bf", //  Sony HD-E1B - 1TB USB3.0
    "", // 0x6610
    "",
    "-d sat"
  },
  // Sunplus
  { "USB: ; SunPlus",
    "0x04fc:0x0c05",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: ; SunPlus SPDIF215",
    "0x04fc:0x0c15",
    "", // 0xf615
    "",
    "-d usbsunplus"
  },
  { "USB: ; SunPlus SPDIF225", // USB+SATA->SATA
    "0x04fc:0x0c25",
    "", // 0x0103
    "",
    "-d usbsunplus"
  },
  // Intrinsix
  { "USB: ; Intrinsix",
    "0x0578:0x0578",
    "", // 0x0202
    "",
    "-d sat" // ATA output registers missing
  },
  // Iomega
  { "USB: Iomega Prestige Desktop USB 3.0; ",
    "0x059b:0x0070",
    "", // 0x0004
    "",
    "-d sat" // ATA output registers missing
  },
  { "USB: Iomega LPHD080-0; ",
    "0x059b:0x0272",
    "",
    "",
    "-d usbcypress"
  },
  { "USB: Iomega MDHD500-U; JMicron",
    "0x059b:0x0274",
    "", // 0x0000
    "",
    "-d usbjmicron,0"
  },
  { "USB: Iomega MDHD500-U; ",
    "0x059b:0x0275",
    "", // 0x0001
    "",
    "" // unsupported
  },
  { "USB: Iomega; JMicron",
    "0x059b:0x027[78]",  // 0x0277: MDHD-UE, 0x0278: LDHD-UPS
    "", // 0x0000
    "",
    "-d usbjmicron"
  },
  { "USB: Iomega LDHD-UP; Sunplus",
    "0x059b:0x0370",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: Iomega; JMicron",
    "0x059b:0x0(47[05]|57[15])", // 0x0470: LPHD-UP, 0x0475: GDHDU2 (0x0100),
      // 0x0575: LDHD-UP
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: Iomega; JMicron",
    "0x059b:0x047a",
    "", // 0x0100
    "",
    "-d sat" // works also with "-d usbjmicron"
  },
  // LaCie
  { "USB: LaCie hard disk (FA Porsche design);",
    "0x059f:0x0651",
    "",
    "",
    "" // unsupported
  },
  { "USB: LaCie d2 Quadra; Oxford OXUF934SSA-LQAG ", // USB+IEEE1394+eSATA->SATA
    "0x059f:0x0828",
    "",
    "",
    "-d sat"
  },
  { "USB: LaCie hard disk; JMicron",
    "0x059f:0x0951",
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: LaCie Rugged Triple Interface; ",
    "0x059f:0x100c",
    "", // 0x0001
    "",
    "-d sat"
  },
  { "USB: LaCie Desktop Hard Drive;",
    "0x059f:0x1010",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: LaCie Desktop Hard Drive; ",
    "0x059f:0x101[68]", // 0x1016: SAMSUNG HD103UJ
    "", // 0x0001
    "",
    "-d sat"
  },
  { "USB: LaCie Desktop Hard Drive; JMicron",
    "0x059f:0x1019",
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: LaCie Rugged Hard Drive; JMicron",
    "0x059f:0x101d",
    "", // 0x0001
    "",
    "-d usbjmicron,x"
  },
  { "USB: LaCie Little Disk USB2; JMicron",
    "0x059f:0x1021",
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: LaCie hard disk; ",
    "0x059f:0x1029",
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: Lacie rikiki; JMicron",
    "0x059f:0x102a",
    "",
    "",
    "-d usbjmicron,x"
  },
  { "USB: LaCie D2 USB3; LucidPort USB300 ",
    "0x059f:0x103d",
    "",
    "",
    "-d sat"
  },
  { "USB: LaCie rikiki USB 3.0; ",
    "0x059f:0x10(49|57)",
    "",
    "",
    "-d sat"
  },
  { "USB: LaCie minimus USB 3.0; ",
    "0x059f:0x104a",
    "",
    "",
    "-d sat"
  },
  { "USB: LaCie Rugged Mini USB 3.0; ",
    "0x059f:0x1051",
    "", // 0x0000
    "",
    "-d sat"
  },
  { "USB: LaCie P9230 (LAC302002); ",
    "0x059f:0x1053",
    "", // 0x0000
    "",
    "-d sat"
  },
  { "USB: LaCie Rugged Mini HDD; ",
    "0x059f:0x106b",
    "",
    "",
    "-d sat"
  },
  { "USB: LaCie; ", // 0x1070: ASMedia 1053 ?
    "0x059f:0x10(6f|7[05]|b8)", // 0x0x10b8: d2 PROFESSIONAL
    "", // 6f/70/b8=0x0001, 75=0x0000
    "",
    "-d sat"
  },
  // In-System Design
  { "USB: ; In-System/Cypress ISD-300A1",
    "0x05ab:0x0060",
    "", // 0x1101
    "",
    "-d usbcypress"
  },
  // Apple
  { "USB: Apple; ",
    "0x05ac:0x8406", // TOSHIBA MQ01UBB200
    "",
    "",
    "-d sat"
  },
  // Genesys Logic
  { "USB: ; Genesys Logic GL881E",
    "0x05e3:0x0702",
    "",
    "",
    "" // unsupported
  },
  { "USB: ; Genesys Logic",
    "0x05e3:0x(07(18|3[15]|61)|2013)", // 0x0718(0x0041): Requires '-T permissive',
    "", // 0x0731: Genesys Logic GL3310, Chieftec USB 3.0 2.5" case, 0x0735(0x1003): ?,
    "", // 0x0761(0x2402): Other World Computing SATA Adapter PA023U3,
        // 0x2013(0x0100): Sharkoon QuickPort Duo Clone USB 3.1 Type-C
    "-d sat"
  },
  // Micron
  { "USB: Micron USB SSD; ",
    "0x0634:0x0655",
    "",
    "",
    "" // unsupported
  },
  // Prolific
  { "USB: ; Prolific PL2507", // USB->PATA
    "0x067b:0x2507",
    "",
    "",
    "-d usbjmicron,0" // Port number is required
  },
  { "USB: ; Prolific PL2571/2771/2773/2775", // USB->SATA, USB3->SATA,
    "0x067b:0x(2571|277[135])",              // USB3+eSATA->SATA, USB3->2xSATA
    "",
    "",
    "-d usbprolific"
  },
  { "USB: ; Prolific PL3507", // USB+IEEE1394->PATA
    "0x067b:0x3507",
    "", // 0x0001
    "",
    "-d usbjmicron,p"
  },
  // Imation
  { "USB: Imation ; ", // Imation Odyssey external USB dock
    "0x0718:0x1000",
    "", // 0x5104
    "",
    "-d sat"
  },
  // Jess-Link
  { "USB: Packard Bell Carbon; SunPlus",
    "0x0766:0x0017",
    "", // 0x0108
    "",
    "-d usbsunplus"
  },
  // Logitec
  { "USB: Logitec LGB-4BNHUC; ",
    "0x0789:0x0296",
    "",
    "",
    "-d sat"
  },
  // SanDisk
  { "USB: SanDisk; ",
    "0x0781:0x55(8[08]|b0)", // 0x5580: SanDisk SDCZ80 (SanDisk pSSD)
    "", // 0x55b0: Sandisk SDSSDE30-2T00 (SanDisk Portable SSD)
    "",
    "-d sat"
  },
  { "USB: SanDisk Extreme; ASMedia ASM2362",
    "0x0781:0x55ae", // SanDisk Extreme (Western Digital SN580E 1TB)
    "", // 0x3008
    "",
    "-d sntasmedia"
  },
  // Freecom
  { "USB: ; Innostor IS631", // No Name USB3->SATA Enclosure
    "0x07ab:0x0621",
    "",
    "",
    "-d sat"
  },
  { "USB: Freecom; ",
    "0x07ab:0xfc17",
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: Freecom Quattro 3.0; ", // USB3.0+IEEE1394+eSATA->SATA
    "0x07ab:0xfc77",
    "",
    "",
    "-d sat"
  },
  { "USB: Freecom Mobile Drive XXS; JMicron",
    "0x07ab:0xfc88",
    "", // 0x0101
    "",
    "-d usbjmicron,x"
  },
  { "USB: Freecom Hard Drive XS; Sunplus",
    "0x07ab:0xfc8e",
    "", // 0x010f
    "",
    "-d usbsunplus"
  },
  { "USB: Freecom; ", // Intel labeled
    "0x07ab:0xfc8f",
    "", // 0x0000
    "",
    "-d sat"
  },
  { "USB: Freecom Classic HD 120GB; ",
    "0x07ab:0xfccd",
    "",
    "",
    "" // unsupported
  },
  { "USB: Freecom; JMicron", // 0xfc85: Freecom FHD-2 Pro / JMicron JM20316
    "0x07ab:0xfc(85|d[6a])",
    "",
    "",
    "-d usbjmicron"
  },
  // Fast Point Technologies
  { "USB: ; ",
    "0x0850:0x00(03|31)",
    "", // 0x0100
    "",
    "-d sat"
  },
  // 0x0860 (?)
  { "USB: ; ",
    "0x0860:0x0001",
    "", // 0x0100
    "",
    "-d sat"
  },
  // Oxford Semiconductor, Ltd
  { "USB: ; Oxford",
    "0x0928:0x0000",
    "",
    "",
    "" // unsupported
  },
  { "USB: ; Oxford OXU921DS",
    "0x0928:0x0002",
    "",
    "",
    "" // unsupported
  },
  { "USB: ; Oxford", // Zalman ZM-VE200
    "0x0928:0x0010",
    "", // 0x0304
    "",
    "-d sat"
  },
  // Toshiba
  { "USB: Toshiba PX1270E-1G16; Sunplus",
    "0x0930:0x0b03",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: Toshiba PX1396E-3T01; Sunplus", // similar to Dura Micro 501
    "0x0930:0x0b09",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: Toshiba Stor.E Steel; Sunplus",
    "0x0930:0x0b11",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: Toshiba Stor.E; ",
    "0x0930:0x0b1[9ab]",
    "", // 0x0001
    "",
    "-d sat"
  },
  { "USB: Toshiba; Sunplus",
    "0x0930:0xa002",
    "", // 0x0103
    "",
    "-d usbsunplus"
  },
  // Lumberg, Inc.
  { "USB: Toshiba Stor.E; Sunplus",
    "0x0939:0x0b1[56]",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: Toshiba Stor.E D10; Initio INIC-1610PL",
    "0x0939:0x0b13",
    "",
    "",
    "-d sat,12"
  },
  // Kingston
  { "USB: Kingston DataTraveller; ",
    "0x0951:0x177f",
    "",
    "",
    "-d sat,12"
  },
  { "USB: Kingston; ",
    "0x0951:0x1780", // XS1000
    "", // 0x100
    "",
    "-d sat"
  },
  // Apricorn
  { "USB: Apricorn; ",
    "0x0984:0x0(040|301|320)", // 0x0040: Apricorn SATA Wire
    "", // 0x0301 (0x0201): Corsair SSD & HDD Cloning Kit
    "", // 0x0320 (0x0133): Apricorn EZ-UP3 (Initio INIC-3607)
    "-d sat"
  },
  // Neodio Technologies
  { "USB: Neodio; Initio INIC-1810PL",
    "0x0aec:0x3050",
    "", // 0x0100
    "",
    "-d sat"
  },
  // Asus (?)
  { "USB: ; ",
    "0x0b05:0x17f8", // ASUSTek T100TA
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: ; ASMedia ASM236x",
    "0x0b05:0x1932", // Asus ROG Strix Arion enclosure
    "", // 0x0100
    "",
    "-d sntasmedia"
  },
  // Seagate
  { "USB: Seagate External Drive; Cypress",
    "0x0bc2:0x0503",
    "", // 0x0240
    "",
    "-d usbcypress"
  },
  { "USB: Seagate FreeAgent; ",
    "0x0bc2:0x(3008|50(31|a1))",
    "",
    "",
    "-d sat,12" // 0x50a1: "-d sat" does not work (ticket #151)
  },
  { "USB: Seagate FireCuda Gaming SSD; ASMedia ASM2364",
    "0x0bc2:0xaa1a",
    "", // 0x100
    "",
    "-d sntasmedia"
  },
  { "USB: Seagate; ",
    "0x0bc2:0x....",
    "",
    "",
    "-d sat"
  },
  // Realtek
  { "USB: ; Realtek RTL9201", // USB->SATA
    "0x0bda:0x9201",
    "", // 0xf200
    "",
    "-d sat"
  },
  { "USB: ; Realtek RTL9210", // USB->PCIe (NVMe)
    "0x(0bda|0dd8):0x9210", // 0x0bda: Realtek, 0x0dd8: Netac WH51
    "", // 0x2100
    "",
    "-d sntrealtek"
  },
  { "USB: ; Realtek RTL9211", // USB->PCIe (NVMe) or SATA
    "0x(0bda|2eb9):0x9211", // 0x0bda: guessed, 0x2eb9: Sabrent EC-WPTF
    ".*", // fall through to next entry and report ambiguous result
    "",
    "-d sntrealtek" // NVMe or ...
  },
  { "USB: ; Realtek RTL9211",
    "0x(0bda|2eb9):0x9211",
    "",
    "",
    "" // ... SATA (unsupported)
  },
  { "USB: ; Realtek RTL9220", // USB->PCIe (NVMe) or SATA
    "0x0bda:0x9220",
    "",
    "",
    "-d sntrealtek" // ... SATA (requires `-d sat`)
  },
  // Addonics
  { "USB: Addonics HDMU3; ", // (ticket #609)
    "0x0bf6:0x1001",
    "", // 0x0100
    "",
    ""
  },
  // Dura Micro
  { "USB: Dura Micro; Cypress",
    "0x0c0b:0xb001",
    "", // 0x1110
    "",
    "-d usbcypress"
  },
  { "USB: Dura Micro; Initio",
    "0x0c0b:0xb136",
    "", // 0x0108
    "",
    "-d sat"
  },
  { "USB: Dura Micro 509; Sunplus",
    "0x0c0b:0xb159",
    "", // 0x0103
    "",
    "-d usbsunplus"
  },
  // Maxtor
  { "USB: Maxtor OneTouch 200GB; ",
    "0x0d49:0x7010",
    "",
    "",
    "" // unsupported
  },
  { "USB: Maxtor OneTouch; ",
    "0x0d49:0x7300",
    "", // 0x0121
    "",
    "-d sat"
  },
  { "USB: Maxtor OneTouch 4; ",
    "0x0d49:0x7310",
    "", // 0x0125
    "",
    "-d sat"
  },
  { "USB: Maxtor OneTouch 4 Mini; ",
    "0x0d49:0x7350",
    "", // 0x0125
    "",
    "-d sat"
  },
  { "USB: Maxtor BlackArmor Portable; ",
    "0x0d49:0x7550",
    "",
    "",
    "-d sat"
  },
  { "USB: Maxtor Basics Desktop; ",
    "0x0d49:0x7410",
    "", // 0x0122
    "",
    "-d sat"
  },
  { "USB: Maxtor Basics Portable; ",
    "0x0d49:0x7450",
    "", // 0x0122
    "",
    "-d sat"
  },
  // Jess-Link International
  { "USB: ; Cypress", // Medion HDDrive2Go
    "0x0dbf:0x9001",
    "", // 0x0240
    "",
    "-d usbcypress"
  },
  // Oyen Digital
  { "USB: Oyen Digital MiniPro USB 3.0; ",
    "0x0dc4:0x020a",
    "",
    "",
    "-d sat"
  },
  // Netac Technology
  { "USB: Netac Z Slim; ",
    "0x0dd8:0x0562",
    "", // 0x1101
    "",
    "-d sat"
  },
  // Cowon Systems, Inc.
  { "USB: Cowon iAudio X5; ",
    "0x0e21:0x0510",
    "",
    "",
    "-d usbcypress"
  },
  // TerraMaster (?)
  { "USB: ; ",
    "0x1000:0x1352", // TerraMaster D5-300C 5-Bay Box
    "",
    "",
    "-d sat"
  },
  // Apacer
  { "USB: Apacer; ",
    "0x1005:0xc004", // Apacer AC633
    "",
    "",
    "-d sat"
  },
  // iRiver
  { "USB: iRiver iHP-120/140 MP3 Player; Cypress",
    "0x1006:0x3002",
    "", // 0x0100
    "",
    "-d usbcypress"
  },
  // Western Digital
  { "USB: WD My Passport (IDE); Cypress",
    "0x1058:0x0701",
    "", // 0x0240
    "",
    "-d usbcypress"
  },
  { "USB: Western Digital; ASMedia ASM236x",
    "0x1058:0x266e", // WD Elements SE SSD
    "",
    "",
    "-d sntasmedia"
  },
  { "USB: Western Digital; ",
    "0x1058:0x....",
    "",
    "",
    "-d sat"
  },
  // Atech Flash Technology
  { "USB: ; Atech", // Kingston
    "0x11b0:0x6(298|388)",
    "", // 0x0108, 0x5408
    "",
    "-d sat"
  },
  // Brain Actuated Technologies
  { "USB: ; Atech", // ICY BOX 2x Raid enclosure IB-RD2253-U31
    "0x1234:0x5678",
    "", // 0x0100
    "",
    "-d sat"
  },
  // ADATA
  { "USB: ADATA; ",
    "0x125f:0xa(1[135]|21|31|3[57]|68|7[56]|8[35])a", // 0xa11a: Classic CH11 1TB, 0xa13a: NH13 1TB,
    "", // 0xa15a: HD710 1TB, 0xa21a: HV610 (0x4504), 0xa31a: HV620 2TB (0x0100),
    "", // 0xa35a: HD650 2TB (0x6503), 0xa37a: Silverstone MS10 M.2 (0x3103), 0xa75a: HD710P 4TB,
        // 0xa68a: SD600, 0xa76a: ED600 (0x0204), 0xa83a: HD330 (0x0100),
        // 0xa85a: HD680 (0x100)
    "-d sat"
  },
  { "USB: ADATA; Cypress",
    "0x125f:0xa9[34]a", // 0xa93a: SH93 (0x0150)
    "",
    "",
    "-d usbcypress"
  },
  // 0x1352 (?)
  { "USB: ; ",
    "0x1352:0xa006", // TerraMaster D2-320
    "", // 0x0100
    "",
    "-d sat"
  },
  // Initio
  { "USB: ; Initio",
    "0x13fd:0x(054|1(04|15))0", // 0x0540: Initio 316000
    "", // 0x1040 (0x0106): USB->SATA+PATA, Chieftec CEB-25I
    "", // 0x1150: Initio 6Y120L0, CoolerMaster XCraft RX-3HU
    "" // unsupported
  },
  { "USB: ; Initio",
    "0x13fd:0x16[45]0",
    "", // 0x1640: 0x0864, 0x1650: 0x0436
    "",
    "-d sat,12" // some SMART commands fail, see ticket #295
  },
  { "USB: ; Initio",
    "0x13fd:0x....",
    "",
    "",
    "-d sat"
  },
  // Phison
  { "USB: ; ",
    "0x13fe:0x6500", // TeamGroup C212 USB flash drive
    "", // 0x0110
    "",
    "-d sntasmedia" // limited info only
  },
  // Super Top
  { "USB: Super Top generic enclosure; ",
    "0x14cd:0x6116",
    "", // 0x0150, older report suggests -d usbcypress
    "", // 0x0160 also reported as unsupported
    "-d sat"
  },
  // JMicron
  { "USB: ; JMicron JMS539", // USB2/3->SATA (old firmware)
    "0x152d:0x0539",
    "0x0100",      // 1.00, various devices support -d usbjmicron
    "",            // 1.00, SSI SI-1359RUS3 supports -d sat,
    ""             //       -d usbjmicron may disconnect drive (ticket #552)
  },
  { "USB: ; JMicron JMS539", // USB2/3->SATA (new firmware)
    "0x152d:0x0539",
    "0x020[56]|"   //  2.05, ZTC USB 3.0 enclosure (ticket #338)
    "0x28(01|03|12)", // 28.01, DATOptic U3eSATA (USB3.0 bridge with port multiplier)
    "",               // 28.03, Mediasonic ProBox HF2-SU3S2 Rev 2 (port multiplier, ticket #504)
    "-d sat"          // 28.12, Mediasonic ProBox H82-SU3S2 (port multiplier)
  },
  { "USB: ; JMicron ", // USB->SATA->4xSATA (port multiplier)
    "0x152d:0x0551",   // JMS539? (old firmware may use 0x152d:0x0539, ticket #552)
    "", // 0x0100
    "",
    "-d usbjmicron,x"
  },
  { "USB: ; JMicron",
    "0x152d:0x0561",
    "", // 0x0003, ODROID CloudShell 2
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS562", // USB2/3+eSATA->2xSATA, USB2/3->3xSATA (RAID0/1)
    "0x152d:0x0562",
    "", // 0x0106, Fantec QB-X2US3R (ticket #966)
    "", // only ATA IDENTIFY works, SMART commands don't work
    "-d sat"
  },
  { "USB: ; JMicron", // USB2/3->2xSATA
    "0x152d:0x0565",
    "", // 0x9114, Akasa DuoDock X (ticket #607)
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS567", // USB2/3->SATA
    "0x152d:0x0567",
    "", // 0x0114
    "", // 0x0205, 2.05, Mediasonic ProBox HF2-SU3S2 Rev 3 (port multiplier, ticket #504)
    "-d sat"
  },
  { "USB: ; JMicron JMS578", // USB->SATA
    "0x152d:0x0578",
    "", // 0x0100, 0x0204
    "",
    "-d sat"
  },
  { "USB: ; JMicron",
    "0x152d:0x05(79|80)", // 0x0579(0x0100): Intenso External
    "", // 0x0100, 0x0201
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS581", // USB->SATA+PCIe (NVMe)
    "0x152d:0x0581",
    "", // 0x4204
    "",
    "-d sntjmicron/sat"
  },
  { "USB: ; JMicron JMS583", // USB->PCIe (NVMe)
    "0x152d:0x[0a]583",
    "", // 0x214
    "",
    "-d sntjmicron"
  },
  { "USB: OCZ THROTTLE OCZESATATHR8G; JMicron JMF601",
    "0x152d:0x0602",
    "",
    "",
    "" // unsupported
  },
  { "USB: ; JMicron",
    "0x152d:0x1337",
    "", // 0x0508, Digitus DA-71106
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS561", // USB2/3->2xSATA
    "0x152d:0x[19]561", // 0x1561(0x0106), Sabrent USB 3.0 Dual Bay SATA Dock
    "",  // 0x9561(0x0105), Orico 6629US3-C USB 3.0 Dual Bay SATA Dock
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS576", // USB3.1->SATA
    "0x152d:0x[01]576",
    "", // 0x0204, ICY BOX IB-223U3a-B
    "",
    "-d sat"
  },
  { "USB: ; JMicron JM20329", // USB->SATA
    "0x152d:0x2329",
    "", // 0x0100
    "",
    "-d usbjmicron"
  },
  { "USB: ; JMicron JM20336", // USB+SATA->SATA, USB->2xSATA
    "0x152d:0x2336",
    "", // 0x0100
    "",
    "-d usbjmicron,x"
  },
  { "USB: Generic JMicron adapter; JMicron",
    "0x152d:0x2337",
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: ; JMicron JM20337/8", // USB->SATA+PATA, USB+SATA->PATA
    "0x152d:0x2338",
    "", // 0x0100
    "",
    "-d usbjmicron"
  },
  { "USB: ; JMicron JM20339", // USB->SATA
    "0x152d:0x2339",
    "", // 0x0100
    "",
    "-d usbjmicron,x"
  },
  { "USB: ; JMicron", // USB+SATA->SATA
    "0x152d:0x2351",  // e.g. Verbatim Portable Hard Drive 500Gb
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: ; JMicron", // USB->SATA
    "0x152d:0x2352",
    "", // 0x0100
    "",
    "-d usbjmicron,x"
  },
  { "USB: ; JMicron", // USB->SATA
    "0x152d:0x2509",
    "0x0100", // old firmware
    "",
    "-d usbjmicron,x"
  },
  { "USB: ; JMicron", // USB->SATA
    "0x152d:0x2509",
    "0x0107", // newer firmware supports SAT
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS566", // USB3->SATA
    "0x152d:0x2566", // e.g. Chieftec CEB-7035S
    "", // 0x0114
    "",
    "-d usbjmicron,x"
  },
  { "USB: ; JMicron JMS567", // USB3->SATA
    "0x152d:0x2567",
    "", // 0x0117, Chieftec CEB-7053S
    "",
    "-d sat"
  },
  { "USB: ; JMicron",
    "0x152d:0x2590",
    "", // 0x0x8105 (ticket #550)
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS567", // USB2/3->SATA
    "0x152d:0x3562",
    "", // 0x0310, StarTech S358BU33ERM (port multiplier, ticket #508)
    "",
    "-d sat"
  },
  { "USB: ; JMicron", // USB3->SATA
    "0x152d:0x3569",
    "", // 0x0203
    "",
    "-d sat"
  },
  { "USB: ; JMicron",
    "0x152d:0x(578e|a5(78|80)|b567)",
    "", // 0x578e(0x1402): Intenso Memory Center, 0xa578: Sabrent EC-DFLT,
    "", // 0xa580(0x003): CENMATE 2 Bay RAID Enclosure, 0xb567: Fantec AD-U3S
    "-d sat"
  },
  { "USB: ; JMicron JMS561", // USB3->2xSATA
    "0x152d:0x[8a]561",
    "", // 0x8561: 0x0107
    "",
    "-d sat"
  },
  { "USB: ; JMicron JMS581", // USB3.2->SATA+PCIe (NVMe)
    "0x152d:0xb581",
    "", // 0x4403: Unitek M.2 NVMe/SATA USB adapter
    "",
    "-d sntjmicron/sat"
  },
  // PNY
  { "USB: ; PNY",
    "0x154b:0x(5678|8001|f009)",
    "", // 0x5678: 0x5408
    "",
    "-d sat"
  },
  // Pinas
  { "USB: ; Pinas",
    "0x1741:0x1156", // Argon EON, device #2
    "", // 0x0100
    "",
    "-d sat"
  },
  // ASMedia
  { "USB: ; ASMedia ASM236x", // USB->PCIe (NVMe)
    "0x174c:0x236[24]",
    "",
    "",
    "-d sntasmedia"
  },
  { "USB: ; ASMedia ASM2464PD", // USB4->PCIe (NVMe) in USB3
    "0x174c:0x2463",
    "",
    "",
    "-d sntasmedia"
  },
  { "USB: ; ASMedia",
    "0x174c:0x....",
    "",
    "",
    "-d sat"
  },
  // ASMedia
  { "USB: ; ASMedia ASM1352-PM", // USB3->2xSATA
    "0x174d:0x1352",
    "", // 0x0100
    "",
    "-d sat"
  },
  // Pinas
  { "USB: ; Pinas",
    "0x174e:0x1155", // Argon EON, device #1
    "", // 0x0100
    "",
    "-d sat"
  },
  // LucidPort
  { "USB: ; LucidPORT USB300", // RaidSonic ICY BOX IB-110StU3-B, Sharkoon SATA QuickPort H3
    "0x1759:0x500[02]", // 0x5000: USB 2.0, 0x5002: USB 3.0
    "",
    "",
    "-d sat"
  },
  { "USB: ; LucidPort", // Fuj:tech SATA-USB3 dock
    "0x1759:0x5100",
    "", // 0x2580
    "",
    "-d sat"
  },
  // Verbatim
  { "USB: Verbatim Portable Hard Drive; Sunplus",
    "0x18a5:0x0214",
    "", // 0x0112
    "",
    "-d usbsunplus"
  },
  { "USB: Verbatim FW/USB160; Oxford OXUF934SSA-LQAG", // USB+IEEE1394->SATA
    "0x18a5:0x0215",
    "", // 0x0001
    "",
    "-d sat"
  },
  { "USB: Verbatim External Hard Drive 47519; Sunplus", // USB->SATA
    "0x18a5:0x0216",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: Verbatim Pocket Hard Drive; JMicron", // SAMSUNG HS25YJZ/3AU10-01
    "0x18a5:0x0227",
    "",
    "",
    "-d usbjmicron" // "-d usbjmicron,x" does not work
  },
  { "USB: Verbatim External Hard Drive; JMicron", // 2TB
    "0x18a5:0x022a",
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: Verbatim Store'n'Go; JMicron", // USB->SATA
    "0x18a5:0x022b",
    "", // 0x0100
    "",
    "-d usbjmicron"
  },
  { "USB: Verbatim Pocket Hard Drive; ", // 1TB USB 3.0
    "0x18a5:0x0237",
    "",
    "",
    "-d sat,12"
  },
  { "USB: Verbatim External Hard Drive; ", // USB 3.0
    "0x18a5:0x04(0[08]|46)", // 00=3TB, 08=1TB, 46=500MB Mobile
    "",
    "",
    "-d sat"
  },
  // Silicon Image
  { "USB: Vantec NST-400MX-SR; Silicon Image 5744",
    "0x1a4a:0x1670",
    "",
    "",
    "" // unsupported
  },
  // Corsair
  { "USB: Voyager GTX; ",
    "0x1b1c:0x1a0e",
    "",
    "",
    "-d sat"
  },
  // SunplusIT
  { "USB: ; SunplusIT",
    "0x1bcf:0x0c31",
    "",
    "",
    "-d usbsunplus"
  },
  // Actions Microelectronics
  { "USB: ; Actions AM8180", // rebranded Realtek RTL9210
    "0x1de1:0xe101",
    "", // 0x2001
    "",
    "-d sntrealtek"
  },
  // Kanguru Solutions
  { "USB: ; ", // ICY BOX IB-256WP
    "0x1e1d:0x20a0",
    "", // 0x3203
    "",
    "-d sat" // ATA output registers missing
  },
  // TrekStor
  { "USB: TrekStor DataStation; ", // DataStation maxi light (USB 3.0)
    "0x1e68:0x0050",
    "", // 0x0100
    "",
    "-d sat"
  },
  // Other World Computing
  { "USB: OWC Envoy Pro; ",
    "0x1e91:0xa2a5",
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: OWC Mercury Elite Pro Quad; ",
    "0x1e91:0xa4a7",
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: OWC Express 1M2; ASMedia ASM2464PD",
    "0x1e91:0xde79",
    "", // 0x0100
    "",
    "-d sntasmedia"
  },
  // Innostor
  { "USB: ; Innostor IS611", // USB3->SATA+PATA
    "0x1f75:0x0611", // SMART access via PATA does not work
    "",
    "",
    "-d sat"
  },
  { "USB: ; Innostor IS621", // USB3->SATA
    "0x1f75:0x0621", // Dynex 2.5" USB 3.0 Exclosure DX-HD302513
    "",
    "",
    "-d sat"
  },
  { "USB: ; Innostor IS888", // USB3->SATA
    "0x1f75:0x0888",
    "", // 0x0034, Sharkoon SATA QuickDeck Pro USB 3.0 (unsupported)
    "", // 0x0036, works with -d sat (ticket #827)
    "-d sat"
  },
  // VIA Labs
  { "USB: ; VIA VL700", // USB2/3->SATA
    "0x2109:0x0700", // Diginote 2.5" USB-3.0 HDD enclosure 80000894
    "", // 0x0005
    "",
    "-d sat,12" // ATA output registers missing
  },
  { "USB: ; VIA VL701", // USB2/3->SATA
    "0x2109:0x0701", // Intenso 2,5" 1TB USB3
    "", // 0x0107
    "",
    "-d sat" // ATA output registers missing
  },
  { "USB: ; VIA VL711", // USB2/3->SATA
    "0x2109:0x0711",
    "", // 0x0114, Mediasonic ProBox K32-SU3 (ticket #594)
    "", // 0x0507, Intenso 2,5" Memory Case 2TB USB3
    "-d sat"
  },
  { "USB: ; VIA VL715/6/7", // USB2/3->SATA, USB-C->SATA
    "0x2109:0x071[567]",
    "", // 0x0336/0x0000
    "",
    "-d sat"
  },
  // Transcend (?)
  { "USB: Transcend ESD310/400; ",
    "0x2174:0x2[01]00", // 0x2000: TS256GESD400K. 0x2100: TS512GESD310C
    "", // 0x1000, 0x0100
    "",
    "-d sat"
  },
  // 0x235c (?)
  { "USB: ; ",
    "0x235c:0xa006", // Terramaster D4-320 (see also 0x5432:0x235c)
    "", // 0x0100
    "",
    "-d sat"
  },
  // Norelsys
  { "USB: ; ", // USB 3.0
    "0x2537:0x106[68]", // 0x1066: Orico 2599US3, 0x1068: Fantec ER-35U3
    "", // 0x0100
    "",
    "-d sat"
  },
  // 0x2bdf (?)
  { "USB: ; ",
    "0x2bdf:0x0580", // HIKSEMI
    "", // 0x1601
    "",
    "-d sat"
  },
  // InX8 / AKiTiO
  { "USB: AkiTio NT2 U3.1C; ",
    "0x2ce5:0x0014",
    "", // 0x0100
    "",
    "-d sat"
  },
  // 0x2eb9 (?): See Realtek (0x0bda) above
  // KIOXIA (?)
  { "USB: ; ", // KIOXIA EXCERIA PLUS
    "0x30de:0x1000",
    "",
    "",
    "-d sntjmicron"
  },
  // 0x31db (?)
  { "USB: ; ",
    "0x31db:0x0716", // DockCase 10s PLP 2.5" Enclosure
    "", // 0x0148
    "",
    "-d sat"
  },
  // Power Quotient International
  { "USB: PQI bridge; ",
    "0x3538:0x0064",
    "",
    "",
    "-d usbsunplus"
  },
  { "USB: PQI H560; ",
    "0x3538:0x0902",
    "", // 0x0000
    "",
    "-d sat"
  },
  // Sharkoon
  { "USB: Sharkoon QuickPort XT USB 3.0; ",
    "0x357d:0x7788",
    "",
    "",
    "-d sat"
  },
  // Hitachi/SimpleTech
  { "USB: Hitachi Touro Desk; JMicron", // 3TB
    "0x4971:0x1011",
    "",
    "",
    "-d usbjmicron"
  },
  { "USB: Hitachi Touro; ",
    "0x4971:0x101[345]", // 14=1TB, 15=2TB, 13=Touro Desk Pro 3TB
    "", // 0x0000
    "",
    "-d sat" // ATA output registers missing
  },
  { "USB: Hitachi Touro Mobile; ", // 1TB
    "0x4971:0x102[034]",
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: SimpleTech;", // USB 3.0 HDD BOX Agestar,  Rock External HDD 3,5" UASP
    "0x4971:0x8017",
    "",
    "",
    "-d sat"
  },
  { "USB: Hitachi/SimpleTech; JMicron", // 1TB
    "0x4971:0xce17",
    "",
    "",
    "-d usbjmicron,x"
  },
  // 0x5432 (?)
  { "USB: ; ",
    "0x5432:0x235c", // TerraMaster D4-320 (see also 0x235c:0xa006)
    "", // 0x0100
    "",
    "-d sat"
  },
  { "USB: ; ",
    "0x5432:0x1352", // TerraMaster D8 Hybrid
    "", // 0x0100
    "",
    "-d sat"
  },
  // OnSpec
  { "USB: ; OnSpec", // USB->PATA
    "0x55aa:0x2b00",
    "", // 0x0100
    "",
    "" // unsupported
  },
  // 0x5910 (?)
  { "USB: ; ",
    "0x5910:0x13fd", // Sabrent EC-SSHD
    "", // 0x0153
    "",
    "-d sat"
  },
  // 0x6795 (?)
  { "USB: Sharkoon 2-Bay RAID Box; ", // USB 3.0
    "0x6795:0x2756",
    "", // 0x0100
    "",
    "-d sat"
  },
  // Transcend
  { "USB: ; ",
    "0x8564:0x7000",
    "", // 0x8000
    "",
    "-d sat"
  },
  // Other World Computing
  { "USB: USB3 to SATA; ",
    "0x7825:0xa2a4",
    "", // 0x4101
    "",
    "-d sat"
  },
  // JMicron II
  { "USB: ; JMicron JMS566",
    "0xa152:0xb566",
    "", // 0x0223
    "",
    "-d sat"
  },
  // 0xab12 (?)
  { "USB: ; JMicron JMS578",
    "0xab12:0x34cd",
    "", // 0x0405
    "",
    "-d sat"
  },
  // Logilink
  { "USB: ; ",
    "0xabcd:0x610[34]", // 0x6103: LogiLink AU0028A V1.0 USB 3.0 to IDE & SATA Adapter
      // 0x6104: LogiLink PCCloneEX Lite
    "",
    "",
    "-d sat"
  },
/*
}; // builtin_knowndrives[]
 */
